;------------------------------------------------------------------------
;
;   Copyright and Disclaimer:
;
;       ---------------------------------------------------------------
;       This software is provided "as is" without warranty of any kind,
;       either expressed or implied, including but not limited to the
;       implied warranties of merchantability and/or fitness for a
;       particular purpose.
;
;       Copyright (c) 2005 Conexant Systems, Inc.
;       All Rights Reserved.
;       ---------------------------------------------------------------
;
;   Abstract:
;
;       This is the 32-bit CX23880 IR driver inf file.
;
;------------------------------------------------------------------------

[Version]
signature="$CHICAGO$"

Class=HIDClass
ClassGuid={745a17a0-74d3-11d0-b6fe-00a0c90f57da}

Provider="Conexant"
DriverVer=03/16/2007,6.0.103.0
CatalogFile.ntx86=cx88ir.cat

[Manufacturer]
"Conexant"=Conexant

[SourceDisksNames]
1="Conexant Cx23880 Drivers",,,""

[SourceDisksFiles]
cx88ir.sys=1
;cpnotify.ax=1

[Conexant]

;---------------------------------------
; Goshawk - DVB-S using Conexant Rosie/Camaric QPSK tuner/demod combination with IR remote
;---------------------------------------
%CX23880.videoCnxtDVBS%=CX23880.CnxtDVBS,PCI\VEN_14F1&DEV_8804&SUBSYS_008414F1



[CX23880.CnxtDVBS]
Include=    ks.inf
Needs=      KS.Registration
AddReg=     CX880.AddReg,CnxtDVBS.AddReg
CopyFiles=  CX880.CopyDrivers


[DestinationDirs]
CX880.CopyDrivers=10,system32\drivers
CX880.CopyFilesDLL = 11

[CX880.CopyDrivers]
cx88ir.sys
HidClass.sys
HidParse.sys

[CX880.CopyFilesDLL]
Hid.dll

[CX880.AddReg]
HKR,,DevLoader,,*ntkern
HKR,,NTMPDriver,,cx88ir.sys


[CnxtDVBS.AddReg]
;NEC standard
HKR,"DriverData","IR_Standard",0x00010001, 0x01, 0x00, 0x00, 0x00
;command table 2: small gray remote
HKR,"DriverData","IR_Command_Table",0x00010001, 0x02, 0x00, 0x00, 0x00



;
; Services installation
;


[CX23880.CnxtDVBS.Services]
AddService = CX88VID,2,VID.ServiceInstall


[VID.ServiceInstall]
DisplayName   = %CX23880.DeviceDesc%
ServiceType   = 1
StartType     = 3
ErrorControl  = 1
ServiceBinary = %10%\system32\drivers\cx88ir.sys

;---------------------------------------------------------------
;                S t r i n g s
;---------------------------------------------------------------

[Strings]

CX23880.videoCnxtDVBS        = "Conexant 2388x IR Decoder (DVB-S)"
CX23880.DeviceDesc           = "Conexant 2388x IR "

