;------------------------------------------------------------------------
;
;   Copyright and Disclaimer:
;
;       ---------------------------------------------------------------
;       This software is provided "as is" without warranty of any kind,
;       either expressed or implied, including but not limited to the
;       implied warranties of merchantability and/or fitness for a
;       particular purpose.
;
;       Copyright (c) 1999-2000 Conexant Systems, Inc.
;       All Rights Reserved.
;       ---------------------------------------------------------------
;
;   File Revision Id:
;
;
;   Abstract:
;
;       This is the mpeg ts capture driver inf file.
;
;------------------------------------------------------------------------

[Version]
signature="$CHICAGO$"
Class=Media
ClassGUID={4d36e96c-e325-11ce-bfc1-08002be10318}
Provider="Conexant"
DriverVer=02/01/2005,4.0.108.2
CatalogFile.ntx86=cx88ts.cat

[Manufacturer]
"Conexant"=Conexant

[SourceDisksNames]
1="Conexant Cx23880 Drivers",,,""

[SourceDisksFiles]
cx88ts.sys=1

[Conexant]
%CX23880.null%=NullSection,  PCI\VEN_14F1&DEV_8802&SUBSYS_006614F1

%ThomsonDVBT.DeviceDesc%=CNXTDVBT,PCI\VEN_14F1&DEV_8802&SUBSYS_08A117DE
%SamsungDVBT.DeviceDesc%=CNXTDVBT,PCI\VEN_14F1&DEV_8802&SUBSYS_08A617DE
%SamsungDVBTFM.DeviceDesc%=CNXTDVBT,PCI\VEN_14F1&DEV_8802&SUBSYS_08A717DE
%SamsungDVBTFMMSI.DeviceDesc%=CNXTDVBT,PCI\VEN_14F1&DEV_8802&SUBSYS_86231462

%CONDVBS.DeviceDesc%=CnxtDVBS,PCI\VEN_14F1&DEV_8802&SUBSYS_08B117DE
%CON2DVBS.DeviceDesc%=CnxtDVBS,PCI\VEN_14F1&DEV_8802&SUBSYS_08B217DE
%CON2DVBSCI.DeviceDesc%=CnxtDVBS,PCI\VEN_14F1&DEV_8802&SUBSYS_08B317DE
%SamsungDVBS.DeviceDesc%=CnxtDVBS,PCI\VEN_14F1&DEV_8802&SUBSYS_08B617DE

%Kittyhawk2.DeviceDesc%=Kittyhawk2,PCI\VEN_14F1&DEV_8802&SUBSYS_08C117DE


[CNXTDVBT]
Include=    ks.inf
Needs=      KS.Registration
AddReg=     CX88TS.AddReg,CNXTDVBT.AddReg
CopyFiles=  CX88TS.CopyDrivers

[CnxtDVBS]
Include=    ks.inf
Needs=      KS.Registration
AddReg=     CX88TS.AddReg,CnxtDVBS.AddReg
CopyFiles=  CX88TS.CopyDrivers

[Kittyhawk2]
Include=    ks.inf
Needs=      KS.Registration
AddReg=     CX88TS.AddReg,Kittyhawk2.AddReg
CopyFiles=  CX88TS.CopyDrivers

[NullSection]

[NullSection.Services]
AddService = , 2  ; null service install

[DestinationDirs]
CX88TS.CopyDrivers=10,system32\drivers

[CX88TS.CopyDrivers]
cx88ts.sys

[CX88TS.AddReg]
HKR,,DevLoader,,*ntkern
HKR,,NTMPDriver,,cx88ts.sys
HKR,,OkToHibernate,3,01
HKR,,PageOutWhenUnopened,3,00
HKR,,DontSuspendIfStreamsAreRunning,3,01

HKLM,System\CurrentControlSet\Control\MediaCategories\%DiagPinID%,Display,1, 00,00,00,00
HKLM,System\CurrentControlSet\Control\MediaCategories\%DiagPinID%,Name,,%DiagPinName%

;
; Driver Configuration Registry Entries
;


[CNXTDVBT.AddReg]
HKR,"DriverData","dwTS_GEN_CNTRL",0x00010001,     0x04,0x00,0x00,0x00
HKR,"DriverData","dwIsTSStream",0x00010001,       0x00,0x00,0x00,0x00
HKR,"DriverData","dwTP_PACKET_SIZE",0x00010001,   0xBC,0x00,0x00,0x00

; DirectShow Filter output pin names
HKLM,System\CurrentControlSet\Control\MediaCategories\%PSPinID%,Display,1, 00,00,00,00
HKLM,System\CurrentControlSet\Control\MediaCategories\%PSPinID%,Name,,%PSpinName%

[CnxtDVBS.AddReg]
HKR,"DriverData","dwTS_GEN_CNTRL",0x00010001,     0x04,0x00,0x00,0x00
HKR,"DriverData","dwIsTSStream",0x00010001,       0x00,0x00,0x00,0x00
HKR,"DriverData","dwTP_PACKET_SIZE",0x00010001,   0xBC,0x00,0x00,0x00

; DirectShow Filter output pin names
HKLM,System\CurrentControlSet\Control\MediaCategories\%PSPinID%,Display,1, 00,00,00,00
HKLM,System\CurrentControlSet\Control\MediaCategories\%PSPinID%,Name,,%PSpinName%


[Kittyhawk2.AddReg]
HKR,"DriverData","dwTS_GEN_CNTRL",0x00010001,     0x00,0x00,0x00,0x00
HKR,"DriverData","dwIsTSStream",0x00010001,       0x00,0x00,0x00,0x00
HKR,"DriverData","dwTP_PACKET_SIZE",0x00010001,   0xBC,0x00,0x00,0x00

; DirectShow Filter output pin names
HKLM,System\CurrentControlSet\Control\MediaCategories\%PSPinID%,Display,1, 00,00,00,00
HKLM,System\CurrentControlSet\Control\MediaCategories\%PSPinID%,Name,,%PSpinName%


;
; Interfaces installation
;


;
; Thomson DVB-T, Stratford
;
[CNXTDVBT.Interfaces]
AddInterface={FD0A5AF4-B41D-11d2-9C95-00C04F7971E0},"GLOBAL",CNXTDVBT_Interface,

[CNXTDVBT_Interface]
AddReg=CNXTDVBT_Interface.AddReg

[CNXTDVBT_Interface.AddReg]
HKR,,CLSID,,{17CCA71B-ECD7-11D0-B908-00A0C9223196}
HKR,,FriendlyName,,%CNXTDVBTFriendlyName%

;
; Cnxts DVB-S, Goshawk
;
[CnxtDVBS.Interfaces]
AddInterface={FD0A5AF4-B41D-11d2-9C95-00C04F7971E0},"GLOBAL",CnxtDVBS_Interface,

[CnxtDVBS_Interface]
AddReg=CnxtDVBS_Interface.AddReg

[CnxtDVBS_Interface.AddReg]
HKR,,CLSID,,{17CCA71B-ECD7-11D0-B908-00A0C9223196}
HKR,,FriendlyName,,%CnxtDVBSFriendlyName%

;
; Thomson ATSC/NTSC/FM, Kittyhawk
;
[Kittyhawk2.Interfaces]
AddInterface={FD0A5AF4-B41D-11d2-9C95-00C04F7971E0},"GLOBAL",Kittyhawk2_Interface,

[Kittyhawk2_Interface]
AddReg=Kittyhawk2_Interface.AddReg

[Kittyhawk2_Interface.AddReg]
HKR,,CLSID,,{17CCA71B-ECD7-11D0-B908-00A0C9223196}
HKR,,FriendlyName,,%KittyhawkFriendlyName%


;
; Services installation
;


;
; Thomson DVB-T, Stratford
;
[CNXTDVBT.Services]
AddService = CX88TS,2,CNXTDVBT.ServiceInstall

[CNXTDVBT.ServiceInstall]
DisplayName   = %ThomsonDVBT.DeviceDesc%
ServiceType   = 1
StartType     = 2
ErrorControl  = 1
ServiceBinary = %10%\system32\drivers\cx88ts.sys

;
; Cnxts DVB-S, Goshawk
;
[CnxtDVBS.Services]
AddService = CX88TS,2,CnxtDVBS.ServiceInstall

[CnxtDVBS.ServiceInstall]
DisplayName   = %CnxtDVBS.DeviceDesc%
ServiceType   = 1
StartType     = 2
ErrorControl  = 1
ServiceBinary = %10%\system32\drivers\cx88ts.sys


;
; Thomson ATSC/NTSC/FM, Kittyhawk
;
[Kittyhawk2.Services]
AddService = CX88TS,2,Kittyhawk2.ServiceInstall

[Kittyhawk2.ServiceInstall]
DisplayName   = %Kittyhawk2.DeviceDesc%
ServiceType   = 1
StartType     = 2
ErrorControl  = 1
ServiceBinary = %10%\system32\drivers\cx88ts.sys


;---------------------------------------------------------------
;                S t r i n g s
;---------------------------------------------------------------

[Strings]
ThomsonDVBT.DeviceDesc= 	"KWorld DVBT 2388x Transport Stream Capture"
SamsungDVBT.DeviceDesc= 	"KWorld DVBT 2388x Transport Stream Capture"
SamsungDVBTFM.DeviceDesc= 	"KWorld DVBT-FM 2388x Transport Stream Capture"
SamsungDVBTFMMSI.DeviceDesc= 	"KWorld DVBT-FM 2388x Transport Stream Capture"

CONDVBS.DeviceDesc=     	"KWorld DVBS 2388x Transport Stream Capture"
CON2DVBS.DeviceDesc=    	"KWorld DVBS 2388x Transport Stream Capture"
CON2DVBSCI.DeviceDesc=  	"KWorld DVBS-CI 2388x Transport Stream Capture"
SamsungDVBS.DeviceDesc= 	"KWorld DVBS 2388x Transport Stream Capture"

Kittyhawk2.DeviceDesc=  	"KWorld ATSC 2388x Transport Stream Capture"

CNXTDVBTFriendlyName ="DigiGo DVBT 2388x Transport Stream Capture"
CnxtDVBSFriendlyName ="DigiGo DVBS 2388x Transport Stream Capture"
KittyhawkFriendlyName="DigiGo ATSC 2388x Transport Stream Capture"

TPPinName =           "MPEG-2 TS"
ESPinID =             "{1649D2C1-435E-11d3-A94B-00A0C9D8B34E}"
ESPinName =           "MPEG-2 Video ES"
PSPinID =             "{1649D2C1-435E-11d3-A94B-00A0C9D8B34E}"
PSPinName =           "MPEG-2 PS"
DiagPinID =           "{1649D2C4-435E-11d3-A94B-00A0C9D8B34E}"
DiagPinName =         "Diagnostics"

CX23880.null          = "KWorld (unused device function)"
