[Version]
LayoutFile=LAYOUT.INF, layout1.inf, layout2.inf
signature="$CHICAGO$"
Class=MEDIA
ClassGUID={4d36e96c-e325-11ce-bfc1-08002be10318}
Provider=%Compro%
CatalogFile=PhTvTune.cat
DriverVer=04/20/2005, 2.3.2.3

[ControlFlags]
;ExcludeFromSelect=*

[Manufacturer]
%Compro%=Compro

[DestinationDirs]
PhTVTune.CopyDrivers = 10,system32\drivers

[SourceDisksFiles]
PhTVTune.sys=1

[SourceDisksNames]
1=%DiskName%,,


[Compro]
%PhTVTune.DeviceDesc%=PhTVTune.Device,STREAM\PhTVTune

[PhTVTune.Device]
Include    = ks.inf, kscaptur.inf
Needs      = KS.Registration,KSCAPTUR.Registration
AddReg     = PhTVTune.AddReg
CopyFiles  = PhTVTune.CopyDrivers
KnownFiles = PhTVTune.KnownFiles

[PhTVTune.Device.NT]
Include    = ks.inf, kscaptur.inf
Needs      = KS.Registration,KSCAPTUR.Registration.NT
CopyFiles  = PhTVTune.CopyDrivers
AddReg     = PhTVTune.AddReg
KnownFiles = PhTVTune.KnownFiles

[PhTVTune.AddReg]
HKR,,DevLoader,,*ntkern
HKR,,NTMPDriver,,PhTVTune.sys
HKR,,PageOutWhenUnopened,3,0

HKR,,Address,,0xc0         ; I2C address
HKR,,EEPROMAddr,,0xa0     ; EEPRom address
HKR,,TunerType,,FI1236  ; "FI1216MK2": CCIR B/G system                  (Western Europe)
                           ; "FI1216MF" : CCIR B/G, L/L1 system            (W. Europe, SE Asia, OZ, NZ)
                           ; "FM1216MK2": CCIR B/G system + FM radio       (Western Europe)
                           ; "FI1236"   : RTMA M+N system                  (USA)
                           ; "FM1236"   : RTMA M+N system + FM radio       (USA)
                           ; "FI1246"   : CCIR I system                    (UK, Ireland, SA, H.K.)
                           ; "FM1246"   : CCIR I system + FM radio         (UK, Ireland, SA, H.K.)
                           ; "FI1256"   : OIRT system                      (China, Russia, E. Europe)
                           ; "FM1256"   : OIRT system + FM radio           (China, Russia, E. Europe)
                           ; "FI1286"   : M system                         (Japan)
                           ;
                           ; "FM1216ME" : CCIR B/G, L/L1, D/K, I system + FM radio (Europe, Asia)
                           ; "FQ1236MK3": RTMA M+N system                  (USA)
                           ; "FM1236MK3": RTMA M+N system + FM radio       (USA)
                           ;
                           ; "MT2032"   : PAL/SECAM microtuner + FM radio  (Western Europe)

HKR,,DefaultStandard,, 0x00000001  ; KS_AnalogVideo_NTSC_M

; =================== PhTVTune ==================================


[PhTVTune.CopyDrivers]
PhTVTune.sys 

[PhTVTune.KnownFiles]
PhTVTune.sys=safe

[PhTVTune.Device.Interfaces]
AddInterface={a799a800-a46d-11d0-a18c-00a02401dcd4},"GLOBAL",TvTuner,

[PhTVTune.Device.NT.Interfaces]
AddInterface={a799a800-a46d-11d0-a18c-00a02401dcd4},"GLOBAL",TvTuner,

[TvTuner]
AddReg=TvTuner.AddReg

[TvTuner.AddReg]
HKR,,CLSID,,{266EEE40-6C63-11cf-8A03-00AA006ECB65}
HKR,,FriendlyName,,%DeviceName%

[PhTVTune.Device.NT.Services]
AddService = PhTVTune,0x00000002,PhTVTune.ServiceInstall

[PhTVTune.ServiceInstall]
DisplayName   = %PhTVTune.DeviceDesc%
ServiceType   = %SERVICE_KERNEL_DRIVER%
StartType     = %SERVICE_DEMAND_START%
ErrorControl  = %SERVICE_ERROR_NORMAL%
ServiceBinary = %12%\PhTVTune.sys

;---------------------------------------------------------------
;                S t r i n g s
;---------------------------------------------------------------

[Strings]

;----------------
; Non-Localizable
;----------------

SERVICE_KERNEL_DRIVER=1
SERVICE_ERROR_NORMAL=1
SERVICE_AUTO_START=2
SERVICE_DEMAND_START=3



Compro               = "Compro Technology Inc."
DiskName              = "Compro VideoMate TV Tuner Install disk"
PhTVTune.DeviceDesc = "VideoMate TV Tuner"
DeviceName            = "VideoMate TV Tuner"
