;****************************************************************************************
;
; rt2500usb.inf
;
;   This installation script supports Windows 98,Me,2000 & XP for the
;   Ralink RT2500 series USB Wireless LAN Card.
;
;   Copyright (c)2002-2009, Ralink Technology Corp., All Rights Reserved
;   Developed by RaLink Technology, Corp. -- http://www.ralinktech.com
;
;****************************************************************************************

[Version]
DriverVer=02/12/2009, 2.01.01.0015
Signature="$Chicago$"
Compatible=1
Class=Net
ClassGUID={4d36e972-e325-11ce-bfc1-08002be10318}
Provider=%Provider%
CatalogFile=rt2500usb.CAT            ;for WHQL certified


[ControlFlags]
;***********Ralink 802.11g board  ***********
;ExcludeFromSelect = USB\VID_148F&PID_2570

[Manufacturer]
%Ralink%        = Ralink
%Amigo%         = Amigo
%MSI%           = MSI
%SMC%           = SMC
%ASUS%          = ASUS
%ZINWELL%       = ZINWELL
%VTech%         = VTech
%SURECOM%       = SURECOM
%Gigabyte%      = Gigabyte
%Siemens%       = Siemens
%BUFFALO%       = BUFFALO
%Sagem%         = Sagem
%Conceptronic%  = Conceptronic
%CNet%          = CNet

[Ralink]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%Ralink.DeviceDesc%         = RALINK.ndi,           USB\VID_148F&PID_2570

[Amigo]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%Amigo_1.DeviceDesc%        = AMIGO_1.ndi,          USB\VID_148F&PID_9020
%Amigo_2.DeviceDesc%        = AMIGO_2.ndi,          USB\VID_0EB0&PID_9020

[MSI]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%m2500usb_6861.DeviceDesc%  = m2500usb_6861.ndi,    USB\VID_0DB0&PID_6861
%m2500usb_6865.DeviceDesc%  = m2500usb_6865.ndi,    USB\VID_0DB0&PID_6865
%m2500usb_6869.DeviceDesc%  = m2500usb_6869.ndi,    USB\VID_0DB0&PID_6869

[SMC]
; DisplayName               Section               DeviceID
; -----------               -------               --------
%SMC.DeviceDesc%            = SMC.ndi,              USB\VID_0707&PID_EE13

[ASUS]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%ASUS.DeviceDesc%           = ASUS.ndi,             USB\VID_0B05&PID_1706
%ASUSGEN.DeviceDesc%        = ASUSGEN.ndi,          USB\VID_0B05&PID_1707

[ZINWELL]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%ZINWELLUSB.DeviceDesc%     = ZINWELLUSB.ndi,       USB\VID_5A57&PID_0260

[VTech]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%VTechUSB.DeviceDesc%       = VTech.ndi,            USB\VID_0F88&PID_3012

[SURECOM]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%SURECOM.DeviceDesc%        = SURECOM.ndi,          USB\VID_0769&PID_11F3

[Gigabyte]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%Gigabyte.DeviceDesc%       = Gigabyte.ndi,         USB\VID_1044&PID_8007

[Siemens]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%Siemens.DeviceDesc%       = SIEMENS.ndi,           USB\VID_0681&PID_3C06

[BUFFALO]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%BUFFALO_5E.DeviceDesc%     = BUFFALO_5E.ndi,       USB\VID_0411&PID_005E
%BUFFALO_66.DeviceDesc%     = BUFFALO_66.ndi,       USB\VID_0411&PID_0066
%BUFFALO_67.DeviceDesc%     = BUFFALO_67.ndi,       USB\VID_0411&PID_0067
%BUFFALO_97.DeviceDesc%     = BUFFALO_97.ndi,       USB\VID_0411&PID_0097

[Sagem]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%Sagem.DeviceDesc%          = Sagem.ndi,            USB\VID_079B&PID_004B

[Conceptronic]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%Conceptronic.DeviceDesc%   = Conceptronic.ndi,     USB\VID_14B2&PID_3C02

[CNet]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%CNet.DeviceDesc%           = CNet.ndi,             USB\VID_1371&PID_9022

;*******************************************************************************************
; Windows 9X specific entries
;*******************************************************************************************

[RALINK.ndi]
AddReg                  = USB_184F_2570.ndi.reg, Common.reg, USB9X.ndi.reg
CopyFiles=win9x.CopyFiles

[AMIGO_1.ndi]
AddReg                  = USB_148F_9020.ndi.reg, Common.reg, USB9X.ndi.reg
CopyFiles               = win9x.CopyFiles

[AMIGO_2.ndi]
AddReg                  = USB_0EB0_9020.ndi.reg, Common.reg, USB9X.ndi.reg
CopyFiles               = win9x.CopyFiles

[m2500usb_6861.ndi]
AddReg                  = USB_0DB0_6861.ndi.reg, Common.reg, USB9X.ndi.reg
CopyFiles               = win9x.CopyFiles

[m2500usb_6865.ndi]
AddReg                  = USB_0DB0_6865.ndi.reg, Common.reg, USB9X.ndi.reg
CopyFiles               = win9x.CopyFiles

[m2500usb_6869.ndi]
AddReg                  = USB_0DB0_6869.ndi.reg, Common.reg, USB9X.ndi.reg
CopyFiles               = win9x.CopyFiles

[SMC.ndi]
AddReg                  = USB_0707_EE13.ndi.reg, Common.reg, USB9X.ndi.reg
CopyFiles               = win9x.CopyFiles

[ASUS.ndi]
AddReg                  = USB_0B05_1706.ndi.reg, Common.reg, USB9X.ndi.reg
CopyFiles=win9x.CopyFiles

[ASUSGEN.ndi]
AddReg                  = USB_0B05_1707.ndi.reg, Common.reg, USB9X.ndi.reg
CopyFiles               = win9x.CopyFiles

[ZINWELLUSB.ndi]
AddReg                  = USB_5A57_0260.ndi.reg, Common.reg, USB9X.ndi.reg
CopyFiles               = win9x.CopyFiles

[VTech.ndi]
AddReg                  = USB_0F88_3012.ndi.reg, Common.reg, USB9X.ndi.reg
CopyFiles               = win9x.CopyFiles

[SURECOM.ndi]
AddReg                  = USB_0769_11F3.ndi.reg, Common.reg, USB9X.ndi.reg
CopyFiles               = win9x.CopyFiles

[Gigabyte.ndi]
AddReg                  = USB_1044_8007.ndi.reg, Common.reg, USB9X.ndi.reg
CopyFiles               = win9x.CopyFiles

[SIEMENS.ndi]
AddReg                  = USB_0681_3C06.ndi.reg, Common.reg, USB9X.ndi.reg
CopyFiles               = win9x.CopyFiles

[BUFFALO_5E.ndi]
AddReg                  = USB_0411_005E.ndi.reg, Common.reg, USB9X.ndi.reg
CopyFiles               = win9x.CopyFiles

[BUFFALO_66.ndi]
AddReg                  = USB_0411_0066.ndi.reg, Common.reg, USB9X.ndi.reg
CopyFiles               = win9x.CopyFiles

[BUFFALO_67.ndi]
AddReg                  = USB_0411_0067.ndi.reg, Common.reg, USB9X.ndi.reg
CopyFiles               = win9x.CopyFiles

[BUFFALO_97.ndi]
AddReg                  = USB_0411_0097.ndi.reg, Common.reg, USB9X.ndi.reg
CopyFiles               = win9x.CopyFiles

[Sagem.ndi]
AddReg                  = USB_079B_004B.ndi.reg, Common.reg, USB9X.ndi.reg
CopyFiles               = win9x.CopyFiles

[Conceptronic.ndi]
AddReg                  = USB_14B2_3C02.ndi.reg, Common.reg, USB9X.ndi.reg
CopyFiles               = win9x.CopyFiles

[CNet.ndi]
AddReg                  = USB_1371_9022.ndi.reg, Common.reg, USB9X.ndi.reg
CopyFiles               = win9x.CopyFiles

;*******************************************************************************************
; NT specific entries
;*******************************************************************************************

[RALINK.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles

[AMIGO_1.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles

[AMIGO_2.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles

[m2500usb_6861.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles

[m2500usb_6865.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles

[m2500usb_6869.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles

[SMC.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles

[ASUS.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles

[ASUSGEN.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles

[ZINWELLUSB.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles

[VTech.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles

[SURECOM.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles

[Gigabyte.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles

[SIEMENS.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles

[BUFFALO_5E.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles

[BUFFALO_66.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles

[BUFFALO_67.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles

[BUFFALO_97.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles

[Sagem.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles

[Conceptronic.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles

[CNet.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles

; NT services sections
[RALINK.ndi.NT.Services]
AddService              = RT2500USB, 2, RALINK.Service, common.EventLog

[AMIGO_1.ndi.NT.Services]
AddService              = RT2500USB, 2, AMIGO.Service, common.EventLog

[AMIGO_2.ndi.NT.Services]
AddService              = RT2500USB, 2, AMIGO.Service, common.EventLog

[m2500usb_6861.ndi.NT.Services]
AddService              = RT2500USB, 2, m2500usb.Service, common.EventLog

[m2500usb_6865.ndi.NT.Services]
AddService              = RT2500USB, 2, m2500usb.Service, common.EventLog

[m2500usb_6869.ndi.NT.Services]
AddService              = RT2500USB, 2, m2500usb.Service, common.EventLog

[SMC.ndi.NT.Services]
AddService              = RT2500USB, 2, SMC.Service, common.EventLog

[ASUS.ndi.NT.Services]
AddService              = RT2500USB, 2, ASUS.Service, common.EventLog

[ASUSGEN.ndi.NT.Services]
AddService              = RT2500USB, 2, ASUS.Service, common.EventLog

[ZINWELLUSB.ndi.NT.Services]
AddService              = RT2500USB, 2, ZINWELLUSB.Service, common.EventLog

[VTech.ndi.NT.Services]
AddService              = RT2500USB, 2, VTech.Service, common.EventLog

[SURECOM.ndi.NT.Services]
AddService              = RT2500USB, 2, SURECOM.Service, common.EventLog

[Gigabyte.ndi.NT.Services]
AddService              = RT2500USB, 2, Gigabyte.Service, common.EventLog

[SIEMENS.ndi.NT.Services]
AddService              = RT2500USB, 2, SIEMENS.Service, common.EventLog

[BUFFALO_5E.ndi.NT.Services]
AddService              = RT2500USB, 2, BUFFALO.Service, common.EventLog

[BUFFALO_66.ndi.NT.Services]
AddService              = RT2500USB, 2, BUFFALO.Service, common.EventLog

[BUFFALO_67.ndi.NT.Services]
AddService              = RT2500USB, 2, BUFFALO.Service, common.EventLog

[BUFFALO_97.ndi.NT.Services]
AddService              = RT2500USB, 2, BUFFALO.Service, common.EventLog

[Sagem.ndi.NT.Services]
AddService              = RT2500USB, 2, Sagem.Service, common.EventLog

[Conceptronic.ndi.NT.Services]
AddService              = RT2500USB, 2, Conceptronic.Service, common.EventLog

[CNet.ndi.NT.Services]
AddService              = RT2500USB, 2, CNet.Service, common.EventLog

;*******************************************************************************************
; common regs for NT and W9x
;*******************************************************************************************


[Common.reg]
;*******************************************************************************************
; System Level Property

;
; Current Profile
;
HKR, ,                  CurProfile,      0,""
HKR, Default,           CurProfile,      0,""

;
; Radio On/Off
;
HKR, ,                            Radio,           0, "0"
HKR, NDI\params\Radio,            ParamDesc,       0, "Radio On/Off"
HKR, NDI\params\Radio,            type,            0, "enum"
HKR, NDI\params\Radio,            default,         0, "0"
HKR, NDI\params\Radio\enum,       1,               0, "Disable"
HKR, NDI\params\Radio\enum,       0,               0, "Enable"

;
; Auto Reconnect Mode
;
HKR, ,                                  AutoReconnect,   0, "1"
HKR, NDI\params\AutoReconnect,          ParamDesc,       0, "Auto Reconnect Mode"
HKR, NDI\params\AutoReconnect,          type,            0, "enum"
HKR, NDI\params\AutoReconnect,          default,         0, "1"
HKR, NDI\params\AutoReconnect\enum,     0,               0, "Disable"
HKR, NDI\params\AutoReconnect\enum,     1,               0, "Enable"

;
; Show Hidden SSID in Site Survey Page
;
HKR, ,                                  ShowHiddenSSID,  0, "0" ; 0=disable(default), 1=enable

;
; Select Config Utility
;
HKR, ,                                  ConfigSelect,    0, "0"  ; 0=RaConfig, 1=ZeroConfig

;
; Country Region 
;
HKR, ,                                  CountryRegion,      0, "0"
;HKR, NDI\params\CountryRegion,         ParamDesc,          0, "Country Region"
;HKR, NDI\params\CountryRegion,         type,               0, "enum"
;HKR, NDI\params\CountryRegion,         default,            0, "0"
;HKR, NDI\params\CountryRegion\enum,    0,                  0, "FCC (Channel 1 - 11)"
;HKR, NDI\params\CountryRegion\enum,    1,                  0, "IC (Channel 1 - 11)"
;HKR, NDI\params\CountryRegion\enum,    2,                  0, "ETSI (Channel 1 - 13)"
;HKR, NDI\params\CountryRegion\enum,    3,                  0, "Spain (Channel 10 - 11)"
;HKR, NDI\params\CountryRegion\enum,    4,                  0, "France (Channel 10 - 13)"
;HKR, NDI\params\CountryRegion\enum,    5,                  0, "MKK (Channel 14)"
;HKR, NDI\params\CountryRegion\enum,    6,                  0, "MKK1 (Channel 1 - 14)"
;HKR, NDI\params\CountryRegion\enum,    7,                  0, "Israel (Channel 3 - 9)"

;*******************************************************************************************
; Advance Page

;
; WirelessMode
;
HKR, ,                            WirelessMode,    0, "0"

;
; Enable TX Burst
;
HKR, ,                            TXBurst,         0, "0"

;
; Use Short Slot Time
;
HKR, ,                            ShortSlot,       0, "0"

;
; Use Turbo rate
;
HKR, ,                            TurboRate,       0, "0"

;
; Use Ofdm rate in adhoc mode
;
HKR, ,                            AdhocOfdm,       0, "0"

;
; Use BG Protection
;
HKR, ,                            BGProtection,    0, "0"
 
;
; Vendor Description
;
HKR, ,                            VendorDesc,      0, %VENDOR_DESC_DEF_STR%
HKR, Default,                     VendorDesc,      0, %VENDOR_DESC_DEF_STR%

;
; PSP XLink mode
;
HKR, ,                            PSPXlink,        0, "0"
HKR, NDI\params\PSPXlink,         ParamDesc,       0, "PSP Xlink Mode"
HKR, NDI\params\PSPXlink,         type,            0, "enum"
HKR, NDI\params\PSPXlink,         default,         0, "0"
HKR, NDI\params\PSPXlink\enum,    0,               0, "Disable"
HKR, NDI\params\PSPXlink\enum,    1,               0, "Enable"

;*******************************************************************************************
; Profile

;
; SSID
;
;HKR, ,                            SSID,            0, %SSID_DEF_STR%
;HKR, Default,                     SSID,            0, %SSID_DEF_STR%
;HKR, NDI\params\SSID,             ParamDesc,       0, "SSID"
;HKR, NDI\params\SSID,             type,            0, "edit"
;HKR, NDI\params\SSID,             limitText,       0, "32"
;HKR, NDI\params\SSID,             default,         0, %SSID_DEF_STR%

;
; Network Type
;
HKR, ,                            NetworkType,     0, %NETWORK_TYPE_DEF_STR%
HKR, Default,                     NetworkType,     0, %NETWORK_TYPE_DEF_STR%
HKR, NDI\params\NetworkType,      ParamDesc,       0, "Network Type"
HKR, NDI\params\NetworkType,      type,            0, "enum"
HKR, NDI\params\NetworkType,      default,         0, %NETWORK_TYPE_DEF_STR%
HKR, NDI\params\NetworkType\enum, 0,               0, "802.11 Ad Hoc"
HKR, NDI\params\NetworkType\enum, 1,               0, "Infrastructure"

;
; Channel
;
HKR, ,                            Channel,         0, %CHANNEL%
HKR, Default,                     Channel,         0, %CHANNEL%


;*******************************************************************************************
; System Configuration Page

;
; Local Administration MAC Network Address
;
HKR, ,                            NetworkAddress,  0, ""
HKR, Default,                     NetworkAddress,  0, ""
HKR, NDI\params\NetworkAddress,   ParamDesc,       0, "Local Administration MAC Network Address"
HKR, NDI\params\NetworkAddress,   type,            0, "edit"
HKR, NDI\params\NetworkAddress,   limitText,       0, "12"
HKR, NDI\params\NetworkAddress,   default,         0, ""
HKR, NDI\params\NetworkAddress,   optional,        0,  "1"

;
; Power Saving Mode
;
HKR, ,                            PSMode,          0, "0"
HKR, Default,                     PSMode,          0, "0"
HKR, NDI\params\PSMode,           ParamDesc,       0, "Power Saving Mode"
HKR, NDI\params\PSMode,           type,            0, "enum"
HKR, NDI\params\PSMode,           default,         0, "0"
HKR, NDI\params\PSMode\enum,      0,               0, "CAM (Constantly Awake Mode)"
HKR, NDI\params\PSMode\enum,      1,               0, "Max_PSP (Max Power Savings)"
HKR, NDI\params\PSMode\enum,      2,               0, "Fast_PSP (Power Save Mode)"

;
; CAM when AC Power
;
HKR, ,                            ACPowerCam,      0, "0"
HKR, Default,                     ACPowerCam,      0, "0"
HKR, NDI\params\ACPowerCam,       ParamDesc,       0, "CAM when AC Power"
HKR, NDI\params\ACPowerCam,       type,            0, "enum"
HKR, NDI\params\ACPowerCam,       default,         0, "0"
HKR, NDI\params\ACPowerCam\enum,  0,               0, "Disable"
HKR, NDI\params\ACPowerCam\enum,  1,               0, "Enable"

;
; Preamble Type
;
HKR, ,                            PreambleType,    0, "0"
HKR, Default,                     PreambleType,    0, "0"

;
; TX Power
;
HKR, ,                            TXPower,         0, "0"
HKR, Default,                     TXPower,         0, "0"

;
; RTS Threshold
;
HKR, ,                            RTSThresh,       0, "2347"
HKR, Default,                     RTSThresh,       0, "2347"
HKR, NDI\params\RTSThresh,        ParamDesc,       0, "RTS Threshold"
HKR, NDI\params\RTSThresh,        type,            0, "int"
HKR, Ndi\params\RTSThresh,        default,         0, "2347"
HKR, NDI\params\RTSThresh,        min,             0, "0"
HKR, NDI\params\RTSThresh,        max,             0, "2347"
HKR, NDI\params\RTSThresh,        step,            0, "1"
HKR, NDI\params\RTSThresh,        optional,        0, "0"

;
; Fragment Threshold
;
HKR, ,                            FragThresh,      0, "2346"
HKR, Default,                     FragThresh,      0, "2346"
HKR, NDI\params\FragThresh,       ParamDesc,       0, "Fragment Threshold"
HKR, NDI\params\FragThresh,       type,            0, "int"
HKR, Ndi\params\FragThresh,       default,         0, "2346"
HKR, NDI\params\FragThresh,       min,             0, "256"
HKR, NDI\params\FragThresh,       max,             0, "2346"
HKR, NDI\params\FragThresh,       step,            0, "1"
HKR, NDI\params\FragThresh,       optional,        0, "0"

;*******************************************************************************************
; Authentication & Security Page

;
; Authentication Type
;
HKR, ,                            AuthenType,      0, "0" ; Open System
HKR, Default,                     AuthenType,      0, "0"

;
; Encryption
;
HKR, ,                            Encryption,      0, "1" ; Disable
HKR, Default,                     Encryption,      0, "1"

;
; WEP Keys Length
;
HKR, ,                            WEPKeyLen,       0, "0"
HKR, Default,                     WEPKeyLen,       0, "0"

;
; WEP Key to use
;
HKR, ,                            WEPKeyUse,       0,"1"
HKR, Default,                     WEPKeyUse,       0,"1"

;
; WEP Key1
;
HKR, ,                  WEPKey1,         0,""
HKR, Default,           WEPKey1,         0,""

;
; WEP Key2
;
HKR, ,                  WEPKey2,         0,""
HKR, Default,           WEPKey2,         0,""

;
; WEP Key3
;
HKR, ,                  WEPKey3,         0,""
HKR, Default,           WEPKey3,         0,""

;
; WEP Key4
;
HKR, ,                  WEPKey4,         0,""
HKR, Default,           WEPKey4,         0,""

;
; WPA PSK
;
HKR, ,                WPAPSK,          0, ""
HKR, Default,         WPAPSK,          0, ""

;*******************************************************************************************
; 802.1x & LEAP

;
; Use 8021X
;
HKR, ,                Use8021X,        0, "0"
HKR, Default,         Use8021X,        0, "0"
 
;
; Authen Protocol
;
HKR, ,                AuthenProtocol,  0, "0"
HKR, Default,         AuthenProtocol,  0, "0"

;
; Tunnel Protocol
;
HKR, ,                TunnelProtocol,  0, "3"
HKR, Default,         TunnelProtocol,  0, "3"

;
; ID
;
HKR, ,                ID,              0, ""
HKR, Default,         ID,              0, ""

;
; Password
;
HKR, ,                Password,        0, ""
HKR, Default,         Password,        0, ""

;
; Tunnel ID
;
HKR, ,                TunnelID,        0, ""
HKR, Default,         TunnelID,        0, ""

;
; Tunnel Password
;
HKR, ,                TunnelPassword,  0, ""
HKR, Default,         TunnelPassword,  0, ""

;
; Session Resumption
;
HKR, ,                SessionResumption, 0, "0"
HKR, Default,         SessionResumption, 0, "0"

;
; Password Mode
;
HKR, ,                PasswordMode,    0, "1"
HKR, Default,         PasswordMode,    0, "1"

;
; Use Client Cert
;
HKR, ,                UseClientCert,   0, "0"
HKR, Default,         UseClientCert,   0, "0"

;
; Use Server Cert
;
HKR, ,                UseServerCert,   0, "0"
HKR, Default,         UseServerCert,   0, "0"

;
; Client Cert Len
;
HKR, ,                ClientCertLen,   0, "0"
HKR, Default,         ClientCertLen,   0, "0"

;
; Client Cert Data
;
HKR, ,                ClientCertData,  0, ""
HKR, Default,         ClientCertData,  0, ""

;
; Server Cert Len
;
HKR, ,                ServerCertLen,   0, "0"
HKR, Default,         ServerCertLen,   0, "0"

;
; Server Cert Data
;
HKR, ,                ServerCertData,  0, ""
HKR, Default,         ServerCertData,  0, ""

;
; Server Name
;
HKR, ,                ServerName,      0, ""
HKR, Default,         ServerName,      0, ""

;
; Name Rule
;
HKR, ,                NameRule,        0, "0"
HKR, Default,         NameRule,        0, "0"

;
; Intermediate Cert
;
HKR, ,                IntermediateCert, 0, "0"
HKR, Default,         IntermediateCert, 0, "0"

;
; Leap Enabled
;
HKR, ,                LeapEnabled,     0, "0"
HKR, Default,         LeapEnabled,     0, "0"

;
; Leap User Name
;
HKR, ,                LeapUserName,    0, ""
HKR, Default,         LeapUserName,    0, ""

;
; Leap Password
;
HKR, ,                LeapPassword,    0, ""
HKR, Default,         LeapPassword,    0, ""

;*******************************************************************************************
; APConfig use
;

;
; WPA Group-Key ReKey Interval
;
HKR, ,                  RekeyInterval,   0, "60"

;
; WPA Group-Key ReKey Method
;
HKR, ,                  RekeyMethod,     0, "0"

;*******************************************************************************************
; DeviceID for Win9X 
;*******************************************************************************************
[USB_184F_2570.ndi.reg]
HKR, Ndi,                         DeviceID,        0, "USB\VID_148F&PID_2570"

[USB_148F_9020.ndi.reg]
HKR, Ndi,                         DeviceID,         0, "USB\VID_148F&PID_9020"

[USB_0EB0_9020.ndi.reg]
HKR, Ndi,                         DeviceID,         0, "USB\VID_0EB0&PID_9020"

[USB_0DB0_6861.ndi.reg]
HKR, Ndi,                         DeviceID,         0, "USB\VID_0DB0&PID_6861"

[USB_0DB0_6865.ndi.reg]
HKR, Ndi,                         DeviceID,         0, "USB\VID_0DB0&PID_6865"

[USB_0DB0_6869.ndi.reg]
HKR, Ndi,                         DeviceID,         0, "USB\VID_0DB0&PID_6869"

[USB_0707_EE13.ndi.reg]
HKR, Ndi,                         DeviceID,         0, "USB\VID_0707&PID_EE13"

[USB_0B05_1706.ndi.reg]
HKR, Ndi,                         DeviceID,         0, "USB\VID_0B05&PID_1706"

[USB_0B05_1707.ndi.reg]
HKR, Ndi,                         DeviceID,         0, "USB\VID_0B05&PID_1707"

[USB_5A57_0260.ndi.reg]
HKR, Ndi,                         DeviceID,         0, "USB\VID_5A57&PID_0260"

[USB_0F88_3012.ndi.reg]
HKR, Ndi,                         DeviceID,         0, "USB\VID_0F88&PID_3012"

[USB_0769_11F3.ndi.reg]
HKR, Ndi,                         DeviceID,         0, "USB\VID_0769&PID_11F3"

[USB_1044_8007.ndi.reg]
HKR, Ndi,                         DeviceID,         0, "USB\VID_1044&PID_8007"

[USB_0681_3C06.ndi.reg]
HKR, Ndi,                         DeviceID,        0, "USB\VID_0681&PID_3C06"

[USB_0411_005E.ndi.reg]
HKR, Ndi,                         DeviceID,        0, "USB\VID_0411&PID_005E"

[USB_0411_0066.ndi.reg]
HKR, Ndi,                         DeviceID,        0, "USB\VID_0411&PID_0066"

[USB_0411_0067.ndi.reg]
HKR, Ndi,                         DeviceID,        0, "USB\VID_0411&PID_0067"

[USB_0411_0097.ndi.reg]
HKR, Ndi,                         DeviceID,        0, "USB\VID_0411&PID_0097"

[USB_079B_004B.ndi.reg]
HKR, Ndi,                         DeviceID,        0, "USB\VID_079B&PID_004B"

[USB_14B2_3C02.ndi.reg]
HKR, Ndi,                         DeviceID,        0, "USB\VID_14B2&PID_3C02"

[USB_1371_9022.ndi.reg]
HKR, Ndi,                         DeviceID,        0, "USB\VID_1371&PID_9022"

[USB9X.ndi.reg]
HKR, ,                            NTMPDriver,      0, rt25u98.sys

HKR, ,                            BusType,          0, 15
HKR, NDI,                         CardType,         0, "PNP"

HKR, ,                            RunningWin9X,     0, "1"
HKR, ,                            DevLoader,        0, "*ndis"
HKR, ,                            DeviceVxDs,       0, "rt25u98.sys"
HKR, ,                            EnumPropPages,    0, "netdi.dll,EnumPropPages"

HKR, Ndi\Interfaces,              DefUpper,         0, "ndis3"
HKR, Ndi\Interfaces,              DefLower,         0, "ethernet"
HKR, Ndi\Interfaces,              UpperRange,       0, "ndis3"
HKR, Ndi\Interfaces,              LowerRange,       0, "ethernet"

HKR, NDIS,                        LogDriverName,    0, "rt25u98"
HKR, NDIS,                        MajorNdisVersion, 1, 03
HKR, NDIS,                        MinorNdisVersion, 1, 0A

;
; Interfaces
;
;
; Install sections
;HKR,Ndi\Install,ndis3,,"rt25u98.install"

;*******************************************************************************************
; DestinationDirs
;*******************************************************************************************

[DestinationDirs]
NT.CopyFiles=12    ; system32\drivers subdirectory on NT
win9x.CopyFiles=11    ; system32 subdirectory on win9x

[NT.CopyFiles]
rt2500usb.sys ; NT Installation

[win9x.CopyFiles]
rt25u98.sys                    ; Win9x Installation

[SourceDisksNames]
1=%INSTALL_DISK_STR%,,,

[SourceDisksFiles] 
rt2500usb.sys=1
rt25u98.sys=1


;*******************************************************************************************
; NT specific
;*******************************************************************************************
[RTUSB.ndi.NT.reg]
HKR, Ndi,                   Service,            0, "rt2500usb"
HKR, Ndi\Interfaces,        UpperRange,         0, "ndis5"
HKR, Ndi\Interfaces,        LowerRange,         0, "ethernet"

[Ralink.Service]
DisplayName                 = %Ralink.Service.DispName%
ServiceType                 = 1                             ;%SERVICE_KERNEL_DRIVER%
StartType                   = 3                             ;%SERVICE_AUTO_START%
ErrorControl                = 1                             ;%SERVICE_ERROR_NORMAL%
ServiceBinary               = %12%\rt2500usb.sys
LoadOrderGroup              = NDIS

[AMIGO.Service]
DisplayName                 = %AMIGO.Service.DispName%
ServiceType                 = 1                             ;%SERVICE_KERNEL_DRIVER%
StartType                   = 3                             ;%SERVICE_AUTO_START%
ErrorControl                = 1                             ;%SERVICE_ERROR_NORMAL%
ServiceBinary               = %12%\rt2500usb.sys
LoadOrderGroup              = NDIS

[m2500usb.Service]
DisplayName                 = %m2500usb.Service.DispName%
ServiceType                 = 1                             ;%SERVICE_KERNEL_DRIVER%
StartType                   = 3                             ;%SERVICE_AUTO_START%
ErrorControl                = 1                             ;%SERVICE_ERROR_NORMAL%
ServiceBinary               = %12%\rt2500usb.sys
LoadOrderGroup              = NDIS

[SMC.Service]
DisplayName                = %SMC.Service.DispName%
ServiceType                 = 1                             ;%SERVICE_KERNEL_DRIVER%
StartType                   = 3                             ;%SERVICE_AUTO_START%
ErrorControl                = 1                             ;%SERVICE_ERROR_NORMAL%
ServiceBinary               = %12%\rt2500usb.sys
LoadOrderGroup              = NDIS

[ASUS.Service]
DisplayName                 = %ASUS.Service.DispName%
ServiceType                 = 1                             ;%SERVICE_KERNEL_DRIVER%
StartType                   = 3                             ;%SERVICE_AUTO_START%
ErrorControl                = 1                             ;%SERVICE_ERROR_NORMAL%
ServiceBinary               = %12%\rt2500usb.sys
LoadOrderGroup              = NDIS

[ZINWELLUSB.Service]
DisplayName                 = %ZINWELL.Service.DispName%
ServiceType                 = 1                             ;%SERVICE_KERNEL_DRIVER%
StartType                   = 3                             ;%SERVICE_AUTO_START%
ErrorControl                = 1                             ;%SERVICE_ERROR_NORMAL%
ServiceBinary               = %12%\rt2500usb.sys
LoadOrderGroup              = NDIS

[VTech.Service]
DisplayName                 = %VTech.Service.DispName%
ServiceType                 = 1                             ;%SERVICE_KERNEL_DRIVER%
StartType                   = 3                             ;%SERVICE_AUTO_START%
ErrorControl                = 1                             ;%SERVICE_ERROR_NORMAL%
ServiceBinary               = %12%\rt2500usb.sys
LoadOrderGroup              = NDIS

[SURECOM.Service]
DisplayName                 = %SURECOM.Service.DispName%
ServiceType                 = 1                             ;%SERVICE_KERNEL_DRIVER%
StartType                   = 3                             ;%SERVICE_AUTO_START%
ErrorControl                = 1                             ;%SERVICE_ERROR_NORMAL%
ServiceBinary               = %12%\rt2500usb.sys
LoadOrderGroup              = NDIS

[Gigabyte.Service]
DisplayName                 = %Gigabyte.Service.DispName%
ServiceType                 = 1                             ;%SERVICE_KERNEL_DRIVER%
StartType                   = 3                             ;%SERVICE_AUTO_START%
ErrorControl                = 1                             ;%SERVICE_ERROR_NORMAL%
ServiceBinary               = %12%\rt2500usb.sys
LoadOrderGroup              = NDIS

[SIEMENS.Service]
DisplayName                 = %SIEMENS.Service.DispName%
ServiceType                 = 1                             ;%SERVICE_KERNEL_DRIVER%
StartType                   = 3                             ;%SERVICE_AUTO_START%
ErrorControl                = 1                             ;%SERVICE_ERROR_NORMAL%
ServiceBinary               = %12%\rt2500usb.sys
LoadOrderGroup              = NDIS

[BUFFALO.Service]
DisplayName                 = %BUFFALO.Service.DispName%
ServiceType                 = 1                             ;%SERVICE_KERNEL_DRIVER%
StartType                   = 3                             ;%SERVICE_AUTO_START%
ErrorControl                = 1                             ;%SERVICE_ERROR_NORMAL%
ServiceBinary               = %12%\rt2500usb.sys
LoadOrderGroup              = NDIS

[Sagem.Service]
DisplayName                 = %Sagem.Service.DispName%
ServiceType                 = 1                             ;%SERVICE_KERNEL_DRIVER%
StartType                   = 3                             ;%SERVICE_AUTO_START%
ErrorControl                = 1                             ;%SERVICE_ERROR_NORMAL%
ServiceBinary               = %12%\rt2500usb.sys
LoadOrderGroup              = NDIS

[Conceptronic.Service]
DisplayName                 = %Conceptronic.Service.DispName%
ServiceType                 = 1                             ;%SERVICE_KERNEL_DRIVER%
StartType                   = 3                             ;%SERVICE_AUTO_START%
ErrorControl                = 1                             ;%SERVICE_ERROR_NORMAL%
ServiceBinary               = %12%\rt2500usb.sys
LoadOrderGroup              = NDIS

[CNet.Service]
DisplayName                 = %CNet.Service.DispName%
ServiceType                 = 1                             ;%SERVICE_KERNEL_DRIVER%
StartType                   = 3                             ;%SERVICE_AUTO_START%
ErrorControl                = 1                             ;%SERVICE_ERROR_NORMAL%
ServiceBinary               = %12%\rt2500usb.sys
LoadOrderGroup              = NDIS

[common.EventLog]
AddReg=common.AddEventLog.reg

[common.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000,"%%SystemRoot%%\System32\netevent.dll,%%SystemRoot%%\System32\drivers\rt2500usb.sys"
HKR, , TypesSupported,   0x00010001, 7


;*******************************************************************************************
; Strings
;*******************************************************************************************
[strings]
Provider                    = "Ralink"
Ralink                      = "Ralink Technology Corp."
Amigo                       = "Amigo Technology Inc."
MSI                         = "802.11 Wireless"
SMC                         = "SMC Networks, Inc"
ASUS                        = "ASUSTeK Computer Inc."
ZINWELL                     = "ZINWELL"
VTech                       = "VTech Telecommunications Ltd"
SURECOM                     = "SURECOM Technology Corp"
Gigabyte                    = "Gigabyte Technology Corp."
Siemens                     = "Siemens"
BUFFALO                     = "BUFFALO INC."
Sagem                       = "Sagem, SA"
Conceptronic                = "2L (Conceptronic)"
CNet                        = "CNet Technology Inc."

RALINK.DeviceDesc           = "RT2500 USB Wireless LAN Card"
Amigo_1.DeviceDesc          = "Wireless USB Card"
Amigo_2.DeviceDesc          = "IEEE 802.11g Wireless Pocket USB"
m2500usb_6861.DeviceDesc    = "Wireless 11g USB 2.0 Stick"
m2500usb_6865.DeviceDesc    = "Wireless 11g MiniUSB 2.0 Adapter"
m2500usb_6869.DeviceDesc    = "Wireless 11g MiniUSB 2.0 Bluetooth Combo"
SMC.DeviceDesc              = "EZ Connect g 2.4GHz 802.11g Wireless USB Adapter"
ASUS.DeviceDesc             = "ASUS USB Wireless Network Adapter"
ASUSGEN.DeviceDesc          = "802.11b/g USB Wireless Network Adapter"
ZINWELLUSB.DeviceDesc       = "802.11g USB Adapter"
VTechUSB.DeviceDesc         = "VTech Wireless 802.11g USB 2.0 Adapter"
SURECOM.DeviceDesc          = "SURECOM 802.11g WLAN USB Adapter"
Gigabyte.DeviceDesc         = "Gigabyte WBKG USB WLAN Card"
Siemens.DeviceDesc          = "Siemens 802.11g USB Wireless Network Adapter"
BUFFALO_5E.DeviceDesc       = "BUFFALO WLI-U2-KG54-YB Wireless LAN Adapter"
BUFFALO_66.DeviceDesc       = "BUFFALO WLI-U2-KG54 Wireless LAN Adapter"
BUFFALO_67.DeviceDesc       = "BUFFALO WLI-U2-KG54-AI Wireless LAN Adapter"
BUFFALO_97.DeviceDesc       = "BUFFALO WLI-U2-KG54-BB Wireless LAN Adapter"
Sagem.DeviceDesc            = "SAGEM Wi-Fi 11g USB adapter"
Conceptronic.DeviceDesc     = "Conceptronic 54Mbps USB adapter"
CNet.DeviceDesc             = "CNet Wireless-G USB dongle"

INSTALL_DISK_STR            = "Wireless 11g USB Installation Disk"

RALINK.Service.DispName     = "RT2500 USB Wireless LAN Driver"
AMIGO.Service.DispName      = "AMIGO RT2500 USB Wieless Driver"
m2500usb.Service.DispName   = "Wireless 11g RT2500 USB 2.0 Network Driver"
SMC.Service.DispName        = "SMC RT2500 USB Wireless LAN Driver"
ASUS.Service.DispName       = "ASUS RT2500 USB Wireless LAN Driver"
ZINWELL.Service.DispName    = "ZINWELL RT2500 USB 802.11g Wireless Driver"
VTech.Service.DispName      = "VTech RT2500 USB 802.11g Wireless Driver"
SURECOM.Service.DispName    = "SURECOM RT2500 USB 802.11g WLAN Driver"
Gigabyte.Service.DispName   = "Gigabyte RT2500 USB WLAN Driver"
SIEMENS.Service.DispName    = "Siemens 802.11g RT2500 USB Wireless Driver"
BUFFALO.Service.DispName    = "BUFFALO RT2500 USB Wireless Driver"
Sagem.Service.DispName      = "SAGEM Wi-Fi 11g RT2500 USB adapter Driver"
Conceptronic.Service.DispName = "Conceptronic 54Mbps RT2500 USB adapter Driver"
CNet.Service.DispName       = "CNet RT2500 USB Wireless Driver"

;
; Don't put spaces around=sign otherwise installer will not be able to
; find these lines.
;SSID_DEF_STR            = ""
VENDOR_DESC_DEF_STR     = ""
NETWORK_TYPE_DEF_STR    = "1"
CHANNEL                 = "1"
