;-------------------------------------------------------
; File: lvPEPIs.inf
; Logitech Video2 Camera Installation file
; Copyright (c) 1996-2005 Logitech Inc.
;-------------------------------------------------------

[Version]
Signature="$CHICAGO$"
Class=MEDIA
ClassGUID={4d36e96c-e325-11ce-bfc1-08002be10318}
provider=%PVD%
CatalogFile=lvPEPIs.cat
LayoutFile=layout.inf, layout1.inf, layout2.inf
DriverVer=05/27/2005, 8.4.7.1032

[SourceDisksNames]
1=%DISK_NAME%,LogiVideo,,

[SourceDisksFiles]
lvcoinst.dll=1
lvcoinst.ini=1
LVUSBSta.sys=1
lv302af.sys=1

[Manufacturer]
%MfgName%=Logitech

[Logitech]
%USB\VID_046D&PID_08A1.DeviceDesc%=EXPRESSPLUS,USB\Vid_046d&Pid_08A1&MI_01               ; 08A1 - QuickCam IM w/ Audio
%USB\VID_046D&PID_08A6.DeviceDesc%=QC.PEPIN2,USB\Vid_046d&Pid_08A6&MI_01                 ; 08A6 - QuickCam IM w/ Audio (Pepin2)
%USB\VID_046D&PID_08A7.DeviceDesc%=QC.LUGU,USB\Vid_046d&Pid_08A7&MI_01                   ; 08A7 - Logitech QuickCam Image
%USB\VID_046D&PID_08A9.DeviceDesc%=QC.HARRISON,USB\Vid_046d&Pid_08A9&MI_01               ; 08A9 - Logitech QuickCam for Notebooks Deluxe
%USB\VID_046D&PID_08AD.DeviceDesc%=QC.COMMUN,USB\Vid_046d&Pid_08AD&MI_01                 ; 08AD - Logitech QuickCam Communicate STX
%USB\VID_046D&PID_08AE.DeviceDesc%=QC.LINCOLN,USB\Vid_046d&Pid_08AE&MI_01                ; 08AE - Logitech QuickCam for Notebooks
%USB\VID_046D&PID_08A3.DeviceDesc%=CHAT,USB\Vid_046d&Pid_08A3&MI_01                      ; 08A3 - QuickCam Chat

[DestinationDirs]
DefaultDestDir = 10,system32\drivers
CopyCoInstaller=11
USBMonitor.CopyFiles=10,system32\drivers
LvPepFilter.CopySys=10,system32\drivers

[ControlFlags]
ExcludeFromSelect=*

[EXPRESSPLUS]
Include=ks.inf, wdmaudio.inf, wdma_usb.inf
Needs=KS.Registration, WDMAUDIO.Registration, USBAudio
AddReg=PCM2USB.AddReg, RecordDevice.AddReg.ALL, RecordDevice.AddReg
CopyFiles=LvPepFilter.CopySys

[EXPRESSPLUS.Interfaces]
AddInterface=%KSCATEGORY_AUDIO%,"GLOBAL",EXPRESSPLUS.Interface,
AddInterface=%KSCATEGORY_RENDER%,"GLOBAL",EXPRESSPLUS.Interface,
AddInterface=%KSCATEGORY_CAPTURE%,"GLOBAL",EXPRESSPLUS.Interface,

[EXPRESSPLUS.NT]
Include=ks.inf, wdmaudio.inf, wdma_usb.inf
Needs=KS.Registration, WDMAUDIO.Registration.NT, USBAudio.NT
AddReg=PCM2USB.AddReg, RecordDevice.AddReg.EXPRESSPLUS, RecordDevice.AddReg.NT
CopyFiles=USBMonitor.CopyFiles,LvPepFilter.CopySys

[EXPRESSPLUS.HW]
AddReg=AddLowerFilter

[EXPRESSPLUS.NT.HW]
AddReg=AddLowerFilter.NT

[AddLowerFilter]
HKR,,LowerFilters,0x10000,"lv302af.sys"

[AddLowerFilter.NT]
HKR,,LowerFilters,0x10008,pepifilter

[RecordDevice.AddReg.EXPRESSPLUS]
HKCU,%MediaPrefered%,"Record",,%USB\VID_046D&PID_08A1.DeviceDesc%
HKCU,%MediaPrefered%,"UserRecord",,%USB\VID_046D&PID_08A1.DeviceDesc%

[EXPRESSPLUS.NT.Interfaces]
AddInterface=%KSCATEGORY_AUDIO%,"GLOBAL",EXPRESSPLUS.Interface,
AddInterface=%KSCATEGORY_RENDER%,"GLOBAL",EXPRESSPLUS.Interface,
AddInterface=%KSCATEGORY_CAPTURE%,"GLOBAL",EXPRESSPLUS.Interface,

[EXPRESSPLUS.Interface]
AddReg=EXPRESSPLUS.Int.Addreg

[EXPRESSPLUS.Int.AddReg]
HKR,,CurveType,1,01,00,00,00
HKR,,FriendlyName,,%USB\VID_046D&PID_08A1.DeviceDesc%
HKR,,CLSID,,%Proxy.CLSID%
HKR,,LVFunctions,0x10001,0x03
HKR,,LVFeatures,0x10001,0x00
HKR,,LVCategories,0x10001,0x1141
HKR,,LVDistribution,0x10001,0x1
HKR,Mixer\0\Controls\1,Channel0,0x10001,51914

[EXPRESSPLUS.NT.Services]
Include=wdma_usb.inf
Needs=USBAudio.NT.Services
AddService = pepifilter,0x00000000,pepifilter_Service

[EXPRESSPLUS.NT.CoInstallers]
CopyFiles=CopyCoInstaller
AddReg=CoInstaller.AddReg

[LvPepFilter.CopySys]
lv302af.sys

[pepifilter_Service]
DisplayName    = %pepifilter.SrvDesc%
ServiceType    = 1                   ; = SERVICE_KERNEL_DRIVER
StartType      = 3                   ; = SERVICE_DEMAND_START
ErrorControl   = 1                   ; = SERVICE_ERROR_NORMAL
ServiceBinary  = %12%\lv302af.sys

[QC.PEPIN2]
Include=ks.inf, wdmaudio.inf, wdma_usb.inf
Needs=KS.Registration, WDMAUDIO.Registration, USBAudio
AddReg=PCM2USB.AddReg, RecordDevice.AddReg.ALL, RecordDevice.AddReg
CopyFiles=LvPepFilter.CopySys

[QC.PEPIN2.Interfaces]
AddInterface=%KSCATEGORY_AUDIO%,"GLOBAL",QC.PEPIN2.Interface,
AddInterface=%KSCATEGORY_RENDER%,"GLOBAL",QC.PEPIN2.Interface,
AddInterface=%KSCATEGORY_CAPTURE%,"GLOBAL",QC.PEPIN2.Interface,

[QC.PEPIN2.NT]
Include=ks.inf, wdmaudio.inf, wdma_usb.inf
Needs=KS.Registration, WDMAUDIO.Registration.NT, USBAudio.NT
AddReg=PCM2USB.AddReg, RecordDevice.AddReg.QC.PEPIN2, RecordDevice.AddReg.NT
CopyFiles=USBMonitor.CopyFiles,LvPepFilter.CopySys

[QC.PEPIN2.HW]
AddReg=AddLowerFilter

[QC.PEPIN2.NT.HW]
AddReg=AddLowerFilter.NT

[RecordDevice.AddReg.QC.PEPIN2]
HKCU,%MediaPrefered%,"Record",,%USB\VID_046D&Pid_08A6.DeviceDesc%
HKCU,%MediaPrefered%,"UserRecord",,%USB\VID_046D&Pid_08A6.DeviceDesc%

[QC.PEPIN2.NT.Interfaces]
AddInterface=%KSCATEGORY_AUDIO%,"GLOBAL",QC.PEPIN2.Interface,
AddInterface=%KSCATEGORY_RENDER%,"GLOBAL",QC.PEPIN2.Interface,
AddInterface=%KSCATEGORY_CAPTURE%,"GLOBAL",QC.PEPIN2.Interface,

[QC.PEPIN2.Interface]
AddReg=QC.PEPIN2.Int.Addreg

[QC.PEPIN2.Int.AddReg]
HKR,,CurveType,1,01,00,00,00
HKR,,FriendlyName,,%USB\VID_046D&Pid_08A6.DeviceDesc%
HKR,,CLSID,,%Proxy.CLSID%
HKR,,LVFunctions,0x10001,0x03
HKR,,LVFeatures,0x10001,0x00
HKR,,LVCategories,0x10001,0x1141
HKR,,LVDistribution,0x10001,0x1
HKR,Mixer\0\Controls\1,Channel0,0x10001,51914

[QC.PEPIN2.NT.Services]
Include=wdma_usb.inf
Needs=USBAudio.NT.Services
AddService = pepifilter,0x00000000,pepifilter_Service

[QC.PEPIN2.NT.CoInstallers]
CopyFiles=CopyCoInstaller
AddReg=CoInstaller.AddReg

[QC.LUGU]
Include=ks.inf, wdmaudio.inf, wdma_usb.inf
Needs=KS.Registration, WDMAUDIO.Registration, USBAudio
AddReg=PCM2USB.AddReg, RecordDevice.AddReg.ALL, RecordDevice.AddReg
CopyFiles=LvPepFilter.CopySys

[QC.LUGU.Interfaces]
AddInterface=%KSCATEGORY_AUDIO%,"GLOBAL",QC.LUGU.Interface,
AddInterface=%KSCATEGORY_RENDER%,"GLOBAL",QC.LUGU.Interface,
AddInterface=%KSCATEGORY_CAPTURE%,"GLOBAL",QC.LUGU.Interface,

[QC.LUGU.NT]
Include=ks.inf, wdmaudio.inf, wdma_usb.inf
Needs=KS.Registration, WDMAUDIO.Registration.NT, USBAudio.NT
AddReg=PCM2USB.AddReg, RecordDevice.AddReg.QC.LUGU, RecordDevice.AddReg.NT
CopyFiles=USBMonitor.CopyFiles,LvPepFilter.CopySys

[QC.LUGU.HW]
AddReg=AddLowerFilter

[QC.LUGU.NT.HW]
AddReg=AddLowerFilter.NT

[RecordDevice.AddReg.QC.LUGU]
HKCU,%MediaPrefered%,"Record",,%USB\VID_046D&PID_08A7.DeviceDesc%
HKCU,%MediaPrefered%,"UserRecord",,%USB\VID_046D&PID_08A7.DeviceDesc%

[QC.LUGU.NT.Interfaces]
AddInterface=%KSCATEGORY_AUDIO%,"GLOBAL",QC.LUGU.Interface,
AddInterface=%KSCATEGORY_RENDER%,"GLOBAL",QC.LUGU.Interface,
AddInterface=%KSCATEGORY_CAPTURE%,"GLOBAL",QC.LUGU.Interface,

[QC.LUGU.Interface]
AddReg=QC.LUGU.Int.Addreg

[QC.LUGU.Int.AddReg]
HKR,,CurveType,1,01,00,00,00
HKR,,FriendlyName,,%USB\VID_046D&PID_08A7.DeviceDesc%
HKR,,CLSID,,%Proxy.CLSID%
HKR,,LVFunctions,0x10001,0x03
HKR,,LVFeatures,0x10001,0x00
HKR,,LVCategories,0x10001,0x1141
HKR,,LVDistribution,0x10001,0x1
HKR,Mixer\0\Controls\1,Channel0,0x10001,51914

[QC.LUGU.NT.Services]
Include=wdma_usb.inf
Needs=USBAudio.NT.Services
AddService = pepifilter,0x00000000,pepifilter_Service

[QC.LUGU.NT.CoInstallers]
CopyFiles=CopyCoInstaller
AddReg=CoInstaller.AddReg

[QC.COMMUN]
Include=ks.inf, wdmaudio.inf, wdma_usb.inf
Needs=KS.Registration, WDMAUDIO.Registration, USBAudio
AddReg=PCM2USB.AddReg, RecordDevice.AddReg.ALL, RecordDevice.AddReg
CopyFiles=LvPepFilter.CopySys

[QC.COMMUN.Interfaces]
AddInterface=%KSCATEGORY_AUDIO%,"GLOBAL",QC.COMMUN.Interface,
AddInterface=%KSCATEGORY_RENDER%,"GLOBAL",QC.COMMUN.Interface,
AddInterface=%KSCATEGORY_CAPTURE%,"GLOBAL",QC.COMMUN.Interface,

[QC.COMMUN.NT]
Include=ks.inf, wdmaudio.inf, wdma_usb.inf
Needs=KS.Registration, WDMAUDIO.Registration.NT, USBAudio.NT
AddReg=PCM2USB.AddReg, RecordDevice.AddReg.QC.COMMUN, RecordDevice.AddReg.NT
CopyFiles=USBMonitor.CopyFiles,LvPepFilter.CopySys

[QC.COMMUN.HW]
AddReg=AddLowerFilter

[QC.COMMUN.NT.HW]
AddReg=AddLowerFilter.NT

[RecordDevice.AddReg.QC.COMMUN]
HKCU,%MediaPrefered%,"Record",,%USB\VID_046D&PID_08AD.DeviceDesc%
HKCU,%MediaPrefered%,"UserRecord",,%USB\VID_046D&PID_08AD.DeviceDesc%

[QC.COMMUN.NT.Interfaces]
AddInterface=%KSCATEGORY_AUDIO%,"GLOBAL",QC.COMMUN.Interface,
AddInterface=%KSCATEGORY_RENDER%,"GLOBAL",QC.COMMUN.Interface,
AddInterface=%KSCATEGORY_CAPTURE%,"GLOBAL",QC.COMMUN.Interface,

[QC.COMMUN.Interface]
AddReg=QC.COMMUN.Int.Addreg

[QC.COMMUN.Int.AddReg]
HKR,,CurveType,1,01,00,00,00
HKR,,FriendlyName,,%USB\VID_046D&PID_08AD.DeviceDesc%
HKR,,CLSID,,%Proxy.CLSID%
HKR,,LVFunctions,0x10001,0x03
HKR,,LVFeatures,0x10001,0x00
HKR,,LVCategories,0x10001,0x1141
HKR,,LVDistribution,0x10001,0x1
HKR,Mixer\0\Controls\1,Channel0,0x10001,51914

[QC.COMMUN.NT.Services]
Include=wdma_usb.inf
Needs=USBAudio.NT.Services
AddService = pepifilter,0x00000000,pepifilter_Service

[QC.COMMUN.NT.CoInstallers]
CopyFiles=CopyCoInstaller
AddReg=CoInstaller.AddReg

[QC.LINCOLN]
Include=ks.inf, wdmaudio.inf, wdma_usb.inf
Needs=KS.Registration, WDMAUDIO.Registration, USBAudio
AddReg=PCM2USB.AddReg, RecordDevice.AddReg.ALL, RecordDevice.AddReg
CopyFiles=LvPepFilter.CopySys

[QC.LINCOLN.Interfaces]
AddInterface=%KSCATEGORY_AUDIO%,"GLOBAL",QC.LINCOLN.Interface,
AddInterface=%KSCATEGORY_RENDER%,"GLOBAL",QC.LINCOLN.Interface,
AddInterface=%KSCATEGORY_CAPTURE%,"GLOBAL",QC.LINCOLN.Interface,

[QC.LINCOLN.NT]
Include=ks.inf, wdmaudio.inf, wdma_usb.inf
Needs=KS.Registration, WDMAUDIO.Registration.NT, USBAudio.NT
AddReg=PCM2USB.AddReg, RecordDevice.AddReg.QC.LINCOLN, RecordDevice.AddReg.NT
CopyFiles=USBMonitor.CopyFiles,LvPepFilter.CopySys

[QC.LINCOLN.HW]
AddReg=AddLowerFilter

[QC.LINCOLN.NT.HW]
AddReg=AddLowerFilter.NT

[RecordDevice.AddReg.QC.LINCOLN]
HKCU,%MediaPrefered%,"Record",,%USB\VID_046D&PID_08AE.DeviceDesc%
HKCU,%MediaPrefered%,"UserRecord",,%USB\VID_046D&PID_08AE.DeviceDesc%

[QC.LINCOLN.NT.Interfaces]
AddInterface=%KSCATEGORY_AUDIO%,"GLOBAL",QC.LINCOLN.Interface,
AddInterface=%KSCATEGORY_RENDER%,"GLOBAL",QC.LINCOLN.Interface,
AddInterface=%KSCATEGORY_CAPTURE%,"GLOBAL",QC.LINCOLN.Interface,

[QC.LINCOLN.Interface]
AddReg=QC.LINCOLN.Int.Addreg

[QC.LINCOLN.Int.AddReg]
HKR,,CurveType,1,01,00,00,00
HKR,,FriendlyName,,%USB\VID_046D&PID_08AE.DeviceDesc%
HKR,,CLSID,,%Proxy.CLSID%
HKR,,LVFunctions,0x10001,0x03
HKR,,LVFeatures,0x10001,0x00
HKR,,LVCategories,0x10001,0x1141
HKR,,LVDistribution,0x10001,0x1
HKR,Mixer\0\Controls\1,Channel0,0x10001,51914

[QC.LINCOLN.NT.Services]
Include=wdma_usb.inf
Needs=USBAudio.NT.Services
AddService = pepifilter,0x00000000,pepifilter_Service

[QC.LINCOLN.NT.CoInstallers]
CopyFiles=CopyCoInstaller
AddReg=CoInstaller.AddReg

[QC.HARRISON]
Include=ks.inf, wdmaudio.inf, wdma_usb.inf
Needs=KS.Registration, WDMAUDIO.Registration, USBAudio
AddReg=PCM2USB.AddReg, RecordDevice.AddReg.ALL, RecordDevice.AddReg
CopyFiles=LvPepFilter.CopySys

[QC.HARRISON.Interfaces]
AddInterface=%KSCATEGORY_AUDIO%,"GLOBAL",QC.HARRISON.Interface,
AddInterface=%KSCATEGORY_RENDER%,"GLOBAL",QC.HARRISON.Interface,
AddInterface=%KSCATEGORY_CAPTURE%,"GLOBAL",QC.HARRISON.Interface,

[QC.HARRISON.NT]
Include=ks.inf, wdmaudio.inf, wdma_usb.inf
Needs=KS.Registration, WDMAUDIO.Registration.NT, USBAudio.NT
AddReg=PCM2USB.AddReg, RecordDevice.AddReg.QC.HARRISON, RecordDevice.AddReg.NT
CopyFiles=USBMonitor.CopyFiles,LvPepFilter.CopySys

[QC.HARRISON.HW]
AddReg=AddLowerFilter

[QC.HARRISON.NT.HW]
AddReg=AddLowerFilter.NT

[RecordDevice.AddReg.QC.HARRISON]
HKCU,%MediaPrefered%,"Record",,%USB\VID_046D&PID_08A9.DeviceDesc%
HKCU,%MediaPrefered%,"UserRecord",,%USB\VID_046D&PID_08A9.DeviceDesc%

[QC.HARRISON.NT.Interfaces]
AddInterface=%KSCATEGORY_AUDIO%,"GLOBAL",QC.HARRISON.Interface,
AddInterface=%KSCATEGORY_RENDER%,"GLOBAL",QC.HARRISON.Interface,
AddInterface=%KSCATEGORY_CAPTURE%,"GLOBAL",QC.HARRISON.Interface,

[QC.HARRISON.Interface]
AddReg=QC.HARRISON.Int.Addreg

[QC.HARRISON.Int.AddReg]
HKR,,CurveType,1,01,00,00,00
HKR,,FriendlyName,,%USB\VID_046D&PID_08A9.DeviceDesc%
HKR,,CLSID,,%Proxy.CLSID%
HKR,,LVFunctions,0x10001,0x03
HKR,,LVFeatures,0x10001,0x00
HKR,,LVCategories,0x10001,0x1141
HKR,,LVDistribution,0x10001,0x1
HKR,Mixer\0\Controls\1,Channel0,0x10001,51914

[QC.HARRISON.NT.Services]
Include=wdma_usb.inf
Needs=USBAudio.NT.Services
AddService = pepifilter,0x00000000,pepifilter_Service

[QC.HARRISON.NT.CoInstallers]
CopyFiles=CopyCoInstaller
AddReg=CoInstaller.AddReg

[CHAT]
Include=ks.inf, wdmaudio.inf, wdma_usb.inf
Needs=KS.Registration, WDMAUDIO.Registration, USBAudio
AddReg=PCM2USB.AddReg, RecordDevice.AddReg.ALL, RecordDevice.AddReg
CopyFiles=LvPepFilter.CopySys

[CHAT.Interfaces]
AddInterface=%KSCATEGORY_AUDIO%,"GLOBAL",CHAT.Interface,
AddInterface=%KSCATEGORY_RENDER%,"GLOBAL",CHAT.Interface,
AddInterface=%KSCATEGORY_CAPTURE%,"GLOBAL",CHAT.Interface,

[CHAT.NT]
Include=ks.inf, wdmaudio.inf, wdma_usb.inf
Needs=KS.Registration, WDMAUDIO.Registration.NT, USBAudio.NT
AddReg=PCM2USB.AddReg, RecordDevice.AddReg.CHAT, RecordDevice.AddReg.NT
CopyFiles=USBMonitor.CopyFiles,LvPepFilter.CopySys

[CHAT.HW]
AddReg=AddLowerFilter

[CHAT.NT.HW]
AddReg=AddLowerFilter.NT

[RecordDevice.AddReg.CHAT]
HKCU,%MediaPrefered%,"Record",,%USB\VID_046D&PID_08A2.DeviceDesc%
HKCU,%MediaPrefered%,"UserRecord",,%USB\VID_046D&PID_08A2.DeviceDesc%

[CHAT.NT.Interfaces]
AddInterface=%KSCATEGORY_AUDIO%,"GLOBAL",CHAT.Interface,
AddInterface=%KSCATEGORY_RENDER%,"GLOBAL",CHAT.Interface,
AddInterface=%KSCATEGORY_CAPTURE%,"GLOBAL",CHAT.Interface,

[CHAT.Interface]
AddReg=CHAT.Int.Addreg

[CHAT.Int.AddReg]
HKR,,CurveType,1,01,00,00,00
HKR,,FriendlyName,,%USB\VID_046D&PID_08A3.DeviceDesc%
HKR,,CLSID,,%Proxy.CLSID%
HKR,,LVFunctions,0x10001,0x03
HKR,,LVFeatures,0x10001,0x00
HKR,,LVCategories,0x10001,0x1141
HKR,,LVDistribution,0x10001,0x0
HKR,Mixer\0\Controls\1,Channel0,0x10001,51914

[CHAT.NT.Services]
Include=wdma_usb.inf
Needs=USBAudio.NT.Services
AddService = pepifilter,0x00000000,pepifilter_Service

[CHAT.NT.CoInstallers]
CopyFiles=CopyCoInstaller
AddReg=CoInstaller.AddReg

[PCM2USB.AddReg]
HKR,,OkToHibernate,3,01
HKR,,SetupPreferredAudioDevices,3,00
HKR,,IgnoreHWString,0x10001,0x01

[RecordDevice.AddReg]
HKLM,"Software\Logitech\QuickCam\Drivers","Audio",,%USBGenericDesc%
HKCU,%MediaPrefered%,"PreferredOnly",1,01,00,00,00

[RecordDevice.AddReg.NT]
HKLM,"Software\Logitech\QuickCam\Drivers","Audio",,%USBGenericDesc%
HKCU,%MediaPrefered%,"PreferredOnly",1,01,00,00,00
HKCU,%MediaPrefered%,"SetupPreferredAudioDevicesCount",1,00,00,00,00

[RecordDevice.AddReg.ALL]
HKCU,%MediaPrefered%,"Record",,%USBGenericDesc%
HKCU,%MediaPrefered%,"UserRecord",,%USBGenericDesc%

[USBMonitor.CopyFiles]
LVUSBSta.sys,,,64

[CopyCoInstaller]
lvcoinst.dll,,,64
lvcoinst.ini,,,64

[CoInstaller.AddReg]
HKR,,CoInstallers32,0x00010000,"lvcoinst.dll,LvCoInstaller"

[Uninstall]
DelFiles = LvPepFilter.CopySys,USBMonitor.CopyFiles,CopyCoInstaller
DelReg   = recorddevice.addreg.all,recorddevice.addreg,recorddevice.addreg.expressplus,recorddevice.addreg.nt,recorddevice.addreg.chat,recorddevice.addreg.qc.harrison,recorddevice.addreg.qc.commun,recorddevice.addreg.qc.lincoln,recorddevice.addreg.qc.pepin2,recorddevice.addreg.qc.lugu

[Strings]
PVD="Logitech"
MfgName="Logitech"
DISK_NAME="Logitech USB Video Camera Disk"
USBGenericDesc="Logitech Microphone"
USB\VID_046D&PID_08A1.DeviceDesc="QuickCam Mic (IM)"
USB\VID_046D&PID_08A2.DeviceDesc="Labtec Mic (WebCam Pro)"
USB\VID_046D&PID_08A3.DeviceDesc="QuickCam Chat"
USB\VID_046D&PID_08A6.DeviceDesc="Logitech Mic (IM)"
USB\VID_046D&PID_08A7.DeviceDesc="Logitech Mic (Image)"
USB\VID_046D&PID_08A9.DeviceDesc="Logitech Mic (Notebooks Deluxe)"
USB\VID_046D&PID_08AD.DeviceDesc="Logitech Mic (Communicate STX)"
USB\VID_046D&PID_08AE.DeviceDesc="Logitech Mic (Notebooks)"
MediaPrefered="Software\Microsoft\Multimedia\Sound Mapper"
Proxy.CLSID     = "{17CCA71B-ECD7-11D0-B908-00A0C9223196}"
KSCATEGORY_AUDIO="{6994ad04-93ef-11d0-a3cc-00a0c9223196}"
KSCATEGORY_RENDER="{65E8773E-8F56-11D0-A3B9-00A0C9223196}"
KSCATEGORY_CAPTURE="{65E8773D-8F56-11D0-A3B9-00A0C9223196}"
pepifilter.SrvDesc="Volume Adapter"



