;------------------------------------------------------------------
;------------------------------------------------------------------
;
;   BN2-350.INF  -- This file contains installation information
;   For windows NT
;   Copyright (c) 2004
;   DSP : ALI-5603C
;   Sensor:   VGA OVT-7640/7648/7649,MT9V011(MI360),HV7131R
;            1.3M OVT-9620/9630/9640,MT9001C12ST,HV7151SP
;
;------------------------------------------------------------------
;------------------------------------------------------------------

[Version]
Signature="$CHICAGO$"
Class=Image
ClassGUID={6bdd1fc6-810f-11d0-bec7-08002be2092f}
Provider=%VENDOR%
CatalogFile=M5603Cvd.cat
DriverVer=02/25/2004,1.1.1.0
 
; All PnP devices should be excluded from manual AddDevice Applet list
[ControlFlags]
ExcludeFromSelect=*

[Manufacturer]
%Mfg%=CamM5603C.Section

[DestinationDirs]
DefaultDestDir                 = 10
CamM5603C.Sensor               = 10,system
CamM5603C.DLCode               = 10,system32\drivers
CamM5603C.CopyDriversNT        = 10,system32\drivers
CamM5603C.System.CopyList      = 10,system
CamM5603C.TwainIni.CopyList    = 10
CamM5603C.TwainDriver.CopyList = 10,TWAIN_32\Bs350u2
CamM5603C.Prop.CopyFilesNT     = 10,system32
CamM5603C.AP.CopyFiles         = 10,VdCap03C
CamM5603C.Uninstall.CopyList   = 10
;---------------------------------------------------------------
;           USB2.0 Web Camera
;---------------------------------------------------------------

[CamM5603C.Section]
%CamM5603C.DeviceDesc%=CamM5603C.Device,USB\VID_0402&PID_5603

[CamM5603C.Device.NT]
Include=ks.inf, kscaptur.inf, ksfilter.inf
Needs=KS.Registration,KSCAPTUR.Registration.NT
SubClass=StillImage
;DeviceType= 0 default, 1 scanner, 2 camera, 3 streaming vedio
DeviceType=3
DeviceSubType=0
Capabilities=0x31
Events=LiveCam.Events
DeviceData=LiveCam.DeviceData
ICMProfiles="sRGB Color Space Profile.icm" 
AddReg=VfWWDM.AddREg.NT, CamM5603C.AddReg, CamM5603C.Prop.AddReg,CameraEnvSetting,SensorRegSetting,Uninstall.AddReg,AddReg.Runonce
CopyFiles=CamM5603C.Sensor,CamM5603C.DLCode,CamM5603C.CopyDriversNT,CamM5603C.System.CopyList,CamM5603C.TwainIni.CopyList,\
CamM5603C.TwainDriver.CopyList,CamM5603C.Prop.CopyFilesNT,CamM5603C.AP.CopyFiles,CamM5603C.Uninstall.CopyList

[LiveCam.Events]
; These are events that the device issues to trigger application
; launching.

[LiveCam.DeviceData]
; Ancillary data to be associated with this device.  TwainDS is the
; name of the data source that a TWAIN-compliant app will be open
; in response to an event.
TwainDS="BisonCam, USB2.0"

Server=local
UI DLL=sti.dll
UI Class ID={4DB1AD10-3391-11D2-9A33-00C04FA36145}

[VfWWDM.AddREg.NT]
HKLM,%MediaResourcesMSVideo%\MSVideo.E_CAMVFW,"Description",,%E_CamVfWWDMDriverDesc%
HKLM,%MediaResourcesMSVideo%\MSVideo.E_CAMVFW,"FriendlyName",,%E_CamVfWWDMDriverDesc%
HKLM,%MediaResourcesMSVideo%\MSVideo.E_CAMVFW,"Driver",,"VfwECamC.dll"

HKLM,%MMDriverDesc%,VfwECamC.dll,,%E_CamVfWWDMDriverDesc%
HKLM,%MMDrivers%,MSVideo,,VfwECamC.dll

[Uninstall.AddReg]
HKLM,SoftWare\Microsoft\Windows\CurrentVersion\Uninstall\%InstallShiled.GUID%,,0x00000002,
HKLM,SOFTWARE\Microsoft\Windows\CurrentVersion\Uninstall\%InstallShiled.GUID%,"DisplayName",0x00000002,"%CamM5603C.DeviceDesc%"
HKLM,SOFTWARE\Microsoft\Windows\CurrentVersion\Uninstall\%InstallShiled.GUID%,"UninstallString",0x00000002,"%10%\Bs350u2r.exe"
HKLM,SOFTWARE\Microsoft\Windows\CurrentVersion\Uninstall\%InstallShiled.GUID%,"DisplayIcon",0x00000002,"%10%\vdcap03c\Livecam.exe"

[CamM5603C.AddReg]
HKR,,HardwareConfig,1,1
HKR,,DevLoader,,*ntkern
HKR,,NTMPDriver,,Bs350u2.sys
;HKR,,DontSuspendIfStreamsAreRunning,3,01
HKR,,CreateFileName,,"USBWebCamera"
HKR,,USDClass,,"{0527d1d0-88c2-11d2-82c7-00c04f8ec183}"
HKR,,DevStatus,,"Inactive"

[AddReg.Runonce]
;HKLM,"Software\Microsoft\Windows\CurrentVersion\Run","StillMnt",0x00000000,"Bs350u2r.exe /StartStillMnt"
;HKLM,"Software\Microsoft\Windows\CurrentVersion\RunOnce","StillMnt",0x00000000,"Bs350u2r.exe /StartStillMnt"

[CamM5603C.Prop.AddReg]
;IPCamCtrl
HKCR,CLSID\{EB9639A2-9773-4AF4-AF2B-3032DC22283B},,,M5603CPropCtrl Class
HKCR,CLSID\{EB9639A2-9773-4AF4-AF2B-3032DC22283B}\InprocServer32,,,FiltProp.dll
HKCR,CLSID\{EB9639A2-9773-4AF4-AF2B-3032DC22283B}\InprocServer32,ThreadingModel,,Both
HKLM,System\CurrentControlSet\Control\MediaInterfaces\{EB9639A2-9773-4AF4-AF2B-3032DC22283B},,,M5603C Control Interface
HKLM,System\CurrentControlSet\Control\MediaInterfaces\{EB9639A2-9773-4AF4-AF2B-3032DC22283B},IID,1, A2, 39, 96, EB, 73, 97, F4, 4A, AF, 2B, 30, 32, DC, 22, 28, 3B
;; CustomCamera Property Page
HKCR,CLSID\{0707404D-A067-4FA0-A993-29F715D79F9B},,,M5603CPropCtrl Class
HKCR,CLSID\{0707404D-A067-4FA0-A993-29F715D79F9B}\InprocServer32,,,FiltProp.dll
HKCR,CLSID\{0707404D-A067-4FA0-A993-29F715D79F9B}\InprocServer32,ThreadingModel,,Both
;; CustomCamera Property Page
HKCR,CLSID\{1378E693-F7FC-4DF9-B663-8380F98BE808},,,M5603CPropCtrl Class
HKCR,CLSID\{1378E693-F7FC-4DF9-B663-8380F98BE808}\InprocServer32,,,FiltProp.dll
HKCR,CLSID\{1378E693-F7FC-4DF9-B663-8380F98BE808}\InprocServer32,ThreadingModel,,Both
;Property Page M5603Ctrl
HKLM,SYSTEM\CurrentControlSet\Control\MediaSets\{EB9639A2-9773-4AF4-AF2B-3032DC22283B}
HKLM,SYSTEM\CurrentControlSet\Control\MediaSets\{EB9639A2-9773-4AF4-AF2B-3032DC22283B}\PropertyPages
HKLM,SYSTEM\CurrentControlSet\Control\MediaSets\{EB9639A2-9773-4AF4-AF2B-3032DC22283B}\PropertyPages\{0707404D-A067-4FA0-A993-29F715D79F9B}
HKLM,SYSTEM\CurrentControlSet\Control\MediaSets\{EB9639A2-9773-4AF4-AF2B-3032DC22283B}\PropertyPages\{1378E693-F7FC-4DF9-B663-8380F98BE808}

[CamM5603C.Sensor]
SenH0110.csr
SenF0110.csr

[CamM5603C.DLCode]
CamH0110.bin
CamF0110.bin

[CamM5603C.CopyDriversNT]
Bs350u2.sys

[CamM5603C.System.CopyList]
FiltProp.dll

[CamM5603C.TwainIni.CopyList]
VdTwn03C.ini
VdTwn03C.src

[CamM5603C.TwainDriver.CopyList]
TwainUI.dll
Bs350u2.ds

[CamM5603C.Prop.CopyFilesNT]
VfwECamC.dll
vfwExtC.dll

[CamM5603C.AP.CopyFiles]
LiveCam.exe
StillMnt.exe

[CamM5603C.Uninstall.CopyList]
Bs350u2r.exe

[SourceDisksNames]
1=%DISK_NAME%,,,

[SourceDisksFiles]
Bs350u2r.exe=1
Bs350u2.ds=1
TwainUI.dll=1
FiltProp.dll=1
VdTwn03C.ini=1
VdTwn03C.src=1
VfwECamC.dll=1
vfwExtC.dll=1
SenH0110.csr=1
SenF0110.csr=1
Bs350u2.sys=1
CamH0110.bin=1
CamF0110.bin=1
LiveCam.exe=1
StillMnt.exe=1

[CamM5603C.Device.NT.Services]
AddService=Cam5603C,0x00000002,CamM5603C.ServiceInstall

[CamM5603C.ServiceInstall]
DisplayName   = %CamM5603C.DeviceDesc%
ServiceType   = %SERVICE_KERNEL_DRIVER%
StartType     = %SERVICE_DEMAND_START%
ErrorControl  = %SERVICE_ERROR_NORMAL%
ServiceBinary = %10%\System32\Drivers\Bs350u2.sys

[CamM5603C.Device.NT.Interfaces]
AddInterface=%KSCATEGORY_CAPTURE%,GLOBAL,CamM5603C.VideoCapture

[CamM5603C.VideoCapture]
AddReg=CamM5603C.VideoCapture.AddReg

[CamM5603C.VideoCapture.AddReg]
HKR,,CLSID,,%ProxyVCap.CLSID%
HKR,,FriendlyName,,%CamM5603C.DeviceDesc%
HKR,,ExtensionDLL,,%CamM5603C.ExtensionDLL%

[CameraEnvSetting]
;*********************************************
; Camera global environment setting
;*********************************************
HKR,,  CamSensorVendor, 0x00010001,  00000000
HKR,,  CamMajorType,    0x00010001,  00000001
HKR,,  CamSubType,      0x00010001,  00000001
HKR,,  CamAudioSupport, 0x00010001,  00000000
HKR,,  SnapshotPos,     0x00010001,  00000000

HKLM,%CAMERA_ENV_REGISTRY%,  UsbVersion,   0x00010001,  00000000
HKLM,%CAMERA_ENV_REGISTRY%,  Alg,          0x00010001,  00000000
HKLM,%CAMERA_ENV_REGISTRY%,  Environment,  0x00010001,  00000000
HKLM,%CAMERA_ENV_REGISTRY%,  DefaultFlip,  0x00010001,  00000000
HKLM,%CAMERA_ENV_REGISTRY%,  DebugMode,    0x00010001,  00000000
HKLM,%CAMERA_ENV_REGISTRY%,  StillImage,   0x00010001,  00000010
HKLM,%CAMERA_ENV_REGISTRY%,  TwainImage,   0x00010001,  00000050
HKLM,%CAMERA_ENV_REGISTRY%,  CurWinSize,   0x00010001,  0x0000ff
HKLM,%CAMERA_ENV_REGISTRY%,  ExtWinSize,   0x00010001,  0x0000ff
HKLM,%CAMERA_ENV_REGISTRY%,  DeviceId,     0x00000000,  %CamM5603C.DeviceId%
HKLM,%CAMERA_ENV_REGISTRY%,  FriendlyName, 0x00000000,  %CamM5603C.DeviceDesc%
HKLM,%CAMERA_ENV_REGISTRY%,  Mfg,          0x00000000,  %Mfg%


;*********************************************
; Default environment setting
;*********************************************
;*********************************************
; Default setting 0
;*********************************************
;;;;; Default setting (Envir 0) ;;;;;
;GammaSRC : 1---CRT, 
HKLM,"%CAMERA_DEFAULT_SETTING%\ALG0\Envir0",  FlipVerHor,  0x00010001,  00000000
HKLM,"%CAMERA_DEFAULT_SETTING%\ALG0\Envir0",  FlickerVal,  0x00010001,  00000002
HKLM,"%CAMERA_DEFAULT_SETTING%\ALG0\Envir0",  Brightness,  0x00010001,  00000050
HKLM,"%CAMERA_DEFAULT_SETTING%\ALG0\Envir0",  Saturation,  0x00010001,  00000040
HKLM,"%CAMERA_DEFAULT_SETTING%\ALG0\Envir0",  Sharpness,   0x00010001,  00000050
HKLM,"%CAMERA_DEFAULT_SETTING%\ALG0\Envir0",  Gamma,       0x00010001,  00000000 
HKLM,"%CAMERA_DEFAULT_SETTING%\ALG0\Envir0",  GammaSRC,    0x00010001,  00000002
HKLM,"%CAMERA_DEFAULT_SETTING%\ALG0\Envir0",  GammaCRT,    0x00010001,  00000001 
HKLM,"%CAMERA_DEFAULT_SETTING%\ALG0\Envir0",  GammaLCD,    0x00010001,  00000000 
HKLM,"%CAMERA_DEFAULT_SETTING%\ALG0\Envir0",  GammaMIN,    0x00010001,  00000000
HKLM,"%CAMERA_DEFAULT_SETTING%\ALG0\Envir0",  GammaMAX,    0x00010001,  00000020

;;;;; Default setting (Envir 1) ;;;;;
HKLM,"%CAMERA_DEFAULT_SETTING%\ALG0\Envir1",  FlipVerHor,  0x00010001,  00000000
HKLM,"%CAMERA_DEFAULT_SETTING%\ALG0\Envir1",  FlickerVal,  0x00010001,  00000002
HKLM,"%CAMERA_DEFAULT_SETTING%\ALG0\Envir1",  Brightness,  0x00010001,  00000050
HKLM,"%CAMERA_DEFAULT_SETTING%\ALG0\Envir1",  Saturation,  0x00010001,  00000040
HKLM,"%CAMERA_DEFAULT_SETTING%\ALG0\Envir1",  Sharpness,   0x00010001,  00000050
HKLM,"%CAMERA_DEFAULT_SETTING%\ALG0\Envir1",  Gamma,       0x00010001,  00000000 
HKLM,"%CAMERA_DEFAULT_SETTING%\ALG0\Envir1",  GammaSRC,    0x00010001,  00000002
HKLM,"%CAMERA_DEFAULT_SETTING%\ALG0\Envir1",  GammaCRT,    0x00010001,  00000001 
HKLM,"%CAMERA_DEFAULT_SETTING%\ALG0\Envir1",  GammaLCD,    0x00010001,  00000000 
HKLM,"%CAMERA_DEFAULT_SETTING%\ALG0\Envir1",  GammaMIN,    0x00010001,  00000000
HKLM,"%CAMERA_DEFAULT_SETTING%\ALG0\Envir1",  GammaMAX,    0x00010001,  00000020

;;;;; Default setting (Envir 2) ;;;;;
HKLM,"%CAMERA_DEFAULT_SETTING%\ALG0\Envir2",  FlipVerHor,  0x00010001,  00000000
HKLM,"%CAMERA_DEFAULT_SETTING%\ALG0\Envir2",  FlickerVal,  0x00010001,  00000002
HKLM,"%CAMERA_DEFAULT_SETTING%\ALG0\Envir2",  Brightness,  0x00010001,  00000050
HKLM,"%CAMERA_DEFAULT_SETTING%\ALG0\Envir2",  Saturation,  0x00010001,  00000040
HKLM,"%CAMERA_DEFAULT_SETTING%\ALG0\Envir2",  Sharpness,   0x00010001,  00000050
HKLM,"%CAMERA_DEFAULT_SETTING%\ALG0\Envir2",  Gamma,       0x00010001,  00000000 
HKLM,"%CAMERA_DEFAULT_SETTING%\ALG0\Envir2",  GammaSRC,    0x00010001,  00000002
HKLM,"%CAMERA_DEFAULT_SETTING%\ALG0\Envir2",  GammaCRT,    0x00010001,  00000001 
HKLM,"%CAMERA_DEFAULT_SETTING%\ALG0\Envir2",  GammaLCD,    0x00010001,  00000000 
HKLM,"%CAMERA_DEFAULT_SETTING%\ALG0\Envir2",  GammaMIN,    0x00010001,  00000000
HKLM,"%CAMERA_DEFAULT_SETTING%\ALG0\Envir2",  GammaMAX,    0x00010001,  00000020

;;;;; Default setting (Envir 3) ;;;;;
HKLM,"%CAMERA_DEFAULT_SETTING%\ALG0\Envir3",  FlipVerHor,  0x00010001,  00000000
HKLM,"%CAMERA_DEFAULT_SETTING%\ALG0\Envir3",  FlickerVal,  0x00010001,  00000002
HKLM,"%CAMERA_DEFAULT_SETTING%\ALG0\Envir3",  Brightness,  0x00010001,  00000050
HKLM,"%CAMERA_DEFAULT_SETTING%\ALG0\Envir3",  Saturation,  0x00010001,  00000040
HKLM,"%CAMERA_DEFAULT_SETTING%\ALG0\Envir3",  Sharpness,   0x00010001,  00000050
HKLM,"%CAMERA_DEFAULT_SETTING%\ALG0\Envir3",  Gamma,       0x00010001,  00000000 
HKLM,"%CAMERA_DEFAULT_SETTING%\ALG0\Envir3",  GammaSRC,    0x00010001,  00000002
HKLM,"%CAMERA_DEFAULT_SETTING%\ALG0\Envir3",  GammaCRT,    0x00010001,  00000001 
HKLM,"%CAMERA_DEFAULT_SETTING%\ALG0\Envir3",  GammaLCD,    0x00010001,  00000000 
HKLM,"%CAMERA_DEFAULT_SETTING%\ALG0\Envir3",  GammaMIN,    0x00010001,  00000000
HKLM,"%CAMERA_DEFAULT_SETTING%\ALG0\Envir3",  GammaMAX,    0x00010001,  00000020

;*********************************************
; User environment setting
;*********************************************

;;;;; User setting (Envir 0) ;;;;;
HKLM,"%CAMERA_USER_SETTING%\Envir0",  FlipVerHor,  0x00010001,  00000000
HKLM,"%CAMERA_USER_SETTING%\Envir0",  FlickerVal,  0x00010001,  00000002
HKLM,"%CAMERA_USER_SETTING%\Envir0",  Brightness,  0x00010001,  00000050
HKLM,"%CAMERA_USER_SETTING%\Envir0",  Saturation,  0x00010001,  00000040
HKLM,"%CAMERA_USER_SETTING%\Envir0",  Sharpness,   0x00010001,  00000050
HKLM,"%CAMERA_USER_SETTING%\Envir0",  Gamma,       0x00010001,  00000000
HKLM,"%CAMERA_USER_SETTING%\Envir0",  GammaSRC,    0x00010001,  00000002
HKLM,"%CAMERA_USER_SETTING%\Envir0",  GammaCRT,    0x00010001,  00000001 
HKLM,"%CAMERA_USER_SETTING%\Envir0",  GammaLCD,    0x00010001,  00000000 
HKLM,"%CAMERA_USER_SETTING%\Envir0",  GammaMIN,    0x00010001,  00000000
HKLM,"%CAMERA_USER_SETTING%\Envir0",  GammaMAX,    0x00010001,  00000020

;;;;; User setting (Envir 1) ;;;;;
HKLM,"%CAMERA_USER_SETTING%\Envir1",  FlipVerHor,  0x00010001,  00000000
HKLM,"%CAMERA_USER_SETTING%\Envir1",  FlickerVal,  0x00010001,  00000002
HKLM,"%CAMERA_USER_SETTING%\Envir1",  Brightness,  0x00010001,  00000050
HKLM,"%CAMERA_USER_SETTING%\Envir1",  Saturation,  0x00010001,  00000040
HKLM,"%CAMERA_USER_SETTING%\Envir1",  Sharpness,   0x00010001,  00000050
HKLM,"%CAMERA_USER_SETTING%\Envir1",  Gamma,       0x00010001,  00000000
HKLM,"%CAMERA_USER_SETTING%\Envir1",  GammaSRC,    0x00010001,  00000002
HKLM,"%CAMERA_USER_SETTING%\Envir1",  GammaCRT,    0x00010001,  00000001 
HKLM,"%CAMERA_USER_SETTING%\Envir1",  GammaLCD,    0x00010001,  00000000 
HKLM,"%CAMERA_USER_SETTING%\Envir1",  GammaMIN,    0x00010001,  00000000
HKLM,"%CAMERA_USER_SETTING%\Envir1",  GammaMAX,    0x00010001,  00000020

;;;;; User setting (Envir 2) ;;;;;
HKLM,"%CAMERA_USER_SETTING%\Envir2",  FlipVerHor,  0x00010001,  00000000
HKLM,"%CAMERA_USER_SETTING%\Envir2",  FlickerVal,  0x00010001,  00000002
HKLM,"%CAMERA_USER_SETTING%\Envir2",  Brightness,  0x00010001,  00000050
HKLM,"%CAMERA_USER_SETTING%\Envir2",  Saturation,  0x00010001,  00000040
HKLM,"%CAMERA_USER_SETTING%\Envir2",  Sharpness,   0x00010001,  00000050
HKLM,"%CAMERA_USER_SETTING%\Envir2",  Gamma,       0x00010001,  00000000
HKLM,"%CAMERA_USER_SETTING%\Envir2",  GammaSRC,    0x00010001,  00000002
HKLM,"%CAMERA_USER_SETTING%\Envir2",  GammaCRT,    0x00010001,  00000001 
HKLM,"%CAMERA_USER_SETTING%\Envir2",  GammaLCD,    0x00010001,  00000000 
HKLM,"%CAMERA_USER_SETTING%\Envir2",  GammaMIN,    0x00010001,  00000000
HKLM,"%CAMERA_USER_SETTING%\Envir2",  GammaMAX,    0x00010001,  00000020

;;;;; User setting (Envir 3) ;;;;;
HKLM,"%CAMERA_USER_SETTING%\Envir3",  FlipVerHor,  0x00010001,  00000000
HKLM,"%CAMERA_USER_SETTING%\Envir3",  FlickerVal,  0x00010001,  00000002
HKLM,"%CAMERA_USER_SETTING%\Envir3",  Brightness,  0x00010001,  00000050
HKLM,"%CAMERA_USER_SETTING%\Envir3",  Saturation,  0x00010001,  00000040
HKLM,"%CAMERA_USER_SETTING%\Envir3",  Sharpness,   0x00010001,  00000050
HKLM,"%CAMERA_USER_SETTING%\Envir3",  Gamma,       0x00010001,  00000000
HKLM,"%CAMERA_USER_SETTING%\Envir3",  GammaSRC,    0x00010001,  00000002
HKLM,"%CAMERA_USER_SETTING%\Envir3",  GammaCRT,    0x00010001,  00000001 
HKLM,"%CAMERA_USER_SETTING%\Envir3",  GammaLCD,    0x00010001,  00000000 
HKLM,"%CAMERA_USER_SETTING%\Envir3",  GammaMIN,    0x00010001,  00000000
HKLM,"%CAMERA_USER_SETTING%\Envir3",  GammaMAX,    0x00010001,  00000020

;*********************************************
; Debug environment setting
;*********************************************

HKLM,"%CAMERA_DEBUG_REGREPORT%"

HKLM,"%CAMERA_REGISTER_ADDR%"   , GetSingleRegister, 0x00010001, 00000000
HKLM,"%CAMERA_REGISTER_ADDR%"   , SetSingleRegister, 0x00010001, 00000000
HKLM,"%CAMERA_EEPROM_SETTING%"  , Result           , 0x00010001, 00000000

[SensorRegSetting]
HKR,%SENSOR_REG_INDEX%,xbDSPCTRL,		0x00010001,		0x8000
HKR,%SENSOR_REG_INDEX%,xbLineStart0,		0x00010001,		0x8001
HKR,%SENSOR_REG_INDEX%,xbLineEnd0,		0x00010001,		0x8002
HKR,%SENSOR_REG_INDEX%,xbPixStart0,		0x00010001,		0x8003
HKR,%SENSOR_REG_INDEX%,xbPixEnd0,		0x00010001,		0x8004
HKR,%SENSOR_REG_INDEX%,xbImgWinMSBL,		0x00010001,		0x8005
HKR,%SENSOR_REG_INDEX%,xbImgWinMSBP,		0x00010001,		0x8006
HKR,%SENSOR_REG_INDEX%,xbLineLength,		0x00010001,		0x8007
HKR,%SENSOR_REG_INDEX%,xbBKNUMH0,		0x00010001,		0x8008
HKR,%SENSOR_REG_INDEX%,xbBKNUMV0,		0x00010001,		0x8009
HKR,%SENSOR_REG_INDEX%,xbBKNUMMSB,		0x00010001,		32778	;0x800A
                      
HKR,%SENSOR_REG_INDEX%,xbBLACKCTL,		0x00010001,		32779	;0x800B
HKR,%SENSOR_REG_INDEX%,xbOBSTART_MSB,		0x00010001,		32780	;0x800C
HKR,%SENSOR_REG_INDEX%,xbBlackLineStart,	0x00010001,		32781	;0x800D
HKR,%SENSOR_REG_INDEX%,xbBlackStart,		0x00010001,		32782	;0x800E
HKR,%SENSOR_REG_INDEX%,xbBlackClampLSB,		0x00010001,		0x8010
HKR,%SENSOR_REG_INDEX%,xbBlackClampMSB,		0x00010001,		32783	;0x800F

HKR,%SENSOR_REG_INDEX%,xbRGAMA,			0x00010001,		0x8011
HKR,%SENSOR_REG_INDEX%,xbGGAMA,			0x00010001,		0x8012
HKR,%SENSOR_REG_INDEX%,xbBGAMA,			0x00010001,		0x8013

HKR,%SENSOR_REG_INDEX%,xbSIF_RGain,		0x00010001,		0x8014
HKR,%SENSOR_REG_INDEX%,xbSIF_GGain,		0x00010001,		0x8015
HKR,%SENSOR_REG_INDEX%,xbSIF_BGain,		0x00010001,		0x8016

HKR,%SENSOR_REG_INDEX%,xbDMCTRL,		0x00010001,		0x8017
HKR,%SENSOR_REG_INDEX%,xbDMLOW,			0x00010001,		0x8018
HKR,%SENSOR_REG_INDEX%,xbDMHIGH,		0x00010001,		0x8019
HKR,%SENSOR_REG_INDEX%,xbDMHVDF,		0x00010001,		32794	;0x801A
                     
HKR,%SENSOR_REG_INDEX%,xbDMNCTL,		0x00010001,		32795	;0x801B
HKR,%SENSOR_REG_INDEX%,xbDWNVECV,		0x00010001,		32796	;0x801C
HKR,%SENSOR_REG_INDEX%,xbDWNVECH,		0x00010001,		32797	;0x801D

HKR,%SENSOR_REG_INDEX%,xbRDARK,			0x00010001,		32798	;0x801E
HKR,%SENSOR_REG_INDEX%,xbRLIGHT,		0x00010001,		32799	;0x801F
HKR,%SENSOR_REG_INDEX%,xbREDDTH,		0x00010001,		0x8020
HKR,%SENSOR_REG_INDEX%,xbREDLTH,		0x00010001,		0x8021
HKR,%SENSOR_REG_INDEX%,xbGDARK,			0x00010001,		0x8022
HKR,%SENSOR_REG_INDEX%,xbGLIGHT,		0x00010001,		0x8023
HKR,%SENSOR_REG_INDEX%,xbGREENDTH,		0x00010001,		0x8024
HKR,%SENSOR_REG_INDEX%,xbGREENLTH,		0x00010001,		0x8025
HKR,%SENSOR_REG_INDEX%,xbBDARK,			0x00010001,		0x8026
HKR,%SENSOR_REG_INDEX%,xbBLIGHT,		0x00010001,		0x8027
HKR,%SENSOR_REG_INDEX%,xbBLUEDTH,		0x00010001,		0x8028
HKR,%SENSOR_REG_INDEX%,xbBLUELTH,		0x00010001,		0x8029
                     
HKR,%SENSOR_REG_INDEX%,xbSMETCTRL,		0x00010001,		32810	;0x802A
                     
HKR,%SENSOR_REG_INDEX%,xbSMETWIN_MSBL,		0x00010001,		32811	;0x802B
HKR,%SENSOR_REG_INDEX%,xbSMETWIN_MSBP,		0x00010001,		32812	;0x802C
HKR,%SENSOR_REG_INDEX%,xbSMET_SLINE,		0x00010001,		32813	;0x802D
HKR,%SENSOR_REG_INDEX%,xbSMET_ELINE,		0x00010001,		32814	;0x802E
HKR,%SENSOR_REG_INDEX%,xbSMET_SPIX,		0x00010001,		32815	;0x802F
HKR,%SENSOR_REG_INDEX%,xbSMET_EPIX,		0x00010001,		0x8030
HKR,%SENSOR_REG_INDEX%,xbSMET_BINHTH,		0x00010001,		0x8031
HKR,%SENSOR_REG_INDEX%,xbSMET_BINLTH,		0x00010001,		0x8032
HKR,%SENSOR_REG_INDEX%,xbMETCTRL,		0x00010001,		0x8033

HKR,%SENSOR_REG_INDEX%,xbMETWIN_MSB,		0x00010001,		0x8034
HKR,%SENSOR_REG_INDEX%,xbAEWIN_X1,		0x00010001,		0x8035
HKR,%SENSOR_REG_INDEX%,xbAEWIN_Y1,		0x00010001,		0x8036
HKR,%SENSOR_REG_INDEX%,xbAEWIN_X2,		0x00010001,		0x8037
HKR,%SENSOR_REG_INDEX%,xbAEWIN_Y2,		0x00010001,		0x8038
HKR,%SENSOR_REG_INDEX%,xbAWBWIN_X1,		0x00010001,		0x8039
HKR,%SENSOR_REG_INDEX%,xbAWBWIN_Y1,		0x00010001,		32826	;0x803A
HKR,%SENSOR_REG_INDEX%,xbAWBWIN_X2,		0x00010001,		32827	;0x803B
HKR,%SENSOR_REG_INDEX%,xbAWBWIN_Y2,		0x00010001,		32828	;0x803C
HKR,%SENSOR_REG_INDEX%,xbYTH_H,			0x00010001,		32829	;0x803D
HKR,%SENSOR_REG_INDEX%,xbYTH_L,			0x00010001,		32830	;0x803E
HKR,%SENSOR_REG_INDEX%,xbUTH_H,			0x00010001,		32831	;0x803F
HKR,%SENSOR_REG_INDEX%,xbUTH_L,			0x00010001,		0x8040
HKR,%SENSOR_REG_INDEX%,xbVTH_H,			0x00010001,		0x8041
HKR,%SENSOR_REG_INDEX%,xbVTH_L,			0x00010001,		0x8042
HKR,%SENSOR_REG_INDEX%,xbRGBTHR_H,		0x00010001,		0x8043
                     
HKR,%SENSOR_REG_INDEX%,xbCOF_RR,		0x00010001,		0x8044
HKR,%SENSOR_REG_INDEX%,xbCOF_GR,		0x00010001,		0x8045
HKR,%SENSOR_REG_INDEX%,xbCOF_BR,		0x00010001,		0x8046
HKR,%SENSOR_REG_INDEX%,xbCOF_RG,		0x00010001,		0x8047
HKR,%SENSOR_REG_INDEX%,xbCOF_GG,		0x00010001,		0x8048
HKR,%SENSOR_REG_INDEX%,xbCOF_BG,		0x00010001,		0x8049
HKR,%SENSOR_REG_INDEX%,xbCOF_RB,		0x00010001,		32842	;0x804A
HKR,%SENSOR_REG_INDEX%,xbCOF_GB,		0x00010001,		32843	;0x804B
HKR,%SENSOR_REG_INDEX%,xbCOF_BB,		0x00010001,		32844	;0x804C
HKR,%SENSOR_REG_INDEX%,xbCOF_RY,		0x00010001,		32845	;0x804D
HKR,%SENSOR_REG_INDEX%,xbCOF_GY,		0x00010001,		32846	;0x804E
HKR,%SENSOR_REG_INDEX%,xbCOF_BY,		0x00010001,		32847	;0x804F
HKR,%SENSOR_REG_INDEX%,xbCOF_ROFFSET,		0x00010001,		0x8050
HKR,%SENSOR_REG_INDEX%,xbCOF_GOFFSET,		0x00010001,		0x8051
HKR,%SENSOR_REG_INDEX%,xbCOF_BOFFSET,		0x00010001,		0x8052
HKR,%SENSOR_REG_INDEX%,xbCOF_YOFFSET,		0x00010001,		0x8053
HKR,%SENSOR_REG_INDEX%,xbCOF_AWB_RGAIN,		0x00010001,		0x8054
HKR,%SENSOR_REG_INDEX%,xbCOF_AWB_GGAIN,		0x00010001,		0x8055
HKR,%SENSOR_REG_INDEX%,xbCOF_AWB_BGAIN,		0x00010001,		0x8056
              		       
HKR,%SENSOR_REG_INDEX%,xbCOF_EDGE_HTH,		0x00010001,		0x8057
HKR,%SENSOR_REG_INDEX%,xbCOF_EDGE_LTH,		0x00010001,		0x8058
HKR,%SENSOR_REG_INDEX%,xbCOF_EDGE_GAIN,		0x00010001,		0x8059
HKR,%SENSOR_REG_INDEX%,xbCOF_HF_GAIN,		0x00010001,		32858	;0x805A
                     
HKR,%SENSOR_REG_INDEX%,xbCOF_YTURNPT,		0x00010001,		32859	;0x805B
HKR,%SENSOR_REG_INDEX%,xbCOF_RU,		0x00010001,		32860	;0x805C
HKR,%SENSOR_REG_INDEX%,xbCOF_GU,		0x00010001,		32861	;0x805D
HKR,%SENSOR_REG_INDEX%,xbCOF_BU,		0x00010001,		32862	;0x805E
HKR,%SENSOR_REG_INDEX%,xbCOF_RV,		0x00010001,		32863	;0x805F
HKR,%SENSOR_REG_INDEX%,xbCOF_GV,		0x00010001,		0x8060
HKR,%SENSOR_REG_INDEX%,xbCOF_BV,		0x00010001,		0x8061

HKR,%SENSOR_REG_INDEX%,xbCOF_TD_YOFFSET,	0x00010001,		0x8062
HKR,%SENSOR_REG_INDEX%,xbCOF_TD_UOFFSET,	0x00010001,		0x8063
HKR,%SENSOR_REG_INDEX%,xbCOF_TD_VOFFSET,	0x00010001,		0x8064
HKR,%SENSOR_REG_INDEX%,xbCOF_AE_YGAIN,		0x00010001,		0x8065
HKR,%SENSOR_REG_INDEX%,xbCOF_AE_UGAIN,		0x00010001,		0x8066
HKR,%SENSOR_REG_INDEX%,xbCOF_AE_VGAIN,		0x00010001,		0x8067
HKR,%SENSOR_REG_INDEX%,xbBADPIX,		0x00010001,		0x8068
HKR,%SENSOR_REG_INDEX%,xbPRC_SHT,		0x00010001,		0x8069
HKR,%SENSOR_REG_INDEX%,xbBBUF_EN,		0x00010001,		32874	;0x806A
         		                                                       
HKR,%SENSOR_REG_INDEX%,xbOBREAD1,		0x00010001,		32906	;0x808A
HKR,%SENSOR_REG_INDEX%,xbOBREAD0,		0x00010001,		32907	;0x808B
HKR,%SENSOR_REG_INDEX%,xbSMET_RED3,		0x00010001,		32908	;0x808C
HKR,%SENSOR_REG_INDEX%,xbSMET_RED2,		0x00010001,		32909	;0x808D
HKR,%SENSOR_REG_INDEX%,xbSMET_RED1,		0x00010001,		32910	;0x808E
HKR,%SENSOR_REG_INDEX%,xbSMET_RED0,		0x00010001,		32911	;0x808F

HKR,%SENSOR_REG_INDEX%,xbSMET_GREEN3,		0x00010001,		0x8090
HKR,%SENSOR_REG_INDEX%,xbSMET_GREEN2,		0x00010001,		0x8091
HKR,%SENSOR_REG_INDEX%,xbSMET_GREEN1,		0x00010001,		0x8092
HKR,%SENSOR_REG_INDEX%,xbSMET_GREEN0,		0x00010001,		0x8093
                     
HKR,%SENSOR_REG_INDEX%,xbSMET_BLUE3,		0x00010001,		0x8094
HKR,%SENSOR_REG_INDEX%,xbSMET_BLUE2,		0x00010001,		0x8095
HKR,%SENSOR_REG_INDEX%,xbSMET_BLUE1,		0x00010001,		0x8096
HKR,%SENSOR_REG_INDEX%,xbSMET_BLUE0,		0x00010001,		0x8097
HKR,%SENSOR_REG_INDEX%,xbSMET_MAX,		0x00010001,		0x8098
HKR,%SENSOR_REG_INDEX%,xbSMET_BINCNT2,		0x00010001,		0x8099
HKR,%SENSOR_REG_INDEX%,xbSMET_BINCNT1,		0x00010001,		32922	;0x809A
HKR,%SENSOR_REG_INDEX%,xbSMET_BINCNT0,		0x00010001,		32923	;0x809B
                     
HKR,%SENSOR_REG_INDEX%,xbMET_Y13,		0x00010001,		32924	;0x809C
HKR,%SENSOR_REG_INDEX%,xbMET_Y12,		0x00010001,		32925	;0x809D
HKR,%SENSOR_REG_INDEX%,xbMET_Y11,		0x00010001,		32926	;0x809E
HKR,%SENSOR_REG_INDEX%,xbMET_Y10,		0x00010001,		32927	;0x809F
HKR,%SENSOR_REG_INDEX%,xbMET_Y23,		0x00010001,		32928	;0x80A0
HKR,%SENSOR_REG_INDEX%,xbMET_Y22,		0x00010001,		32929	;0x80A1
HKR,%SENSOR_REG_INDEX%,xbMET_Y21,		0x00010001,		32930	;0x80A2
HKR,%SENSOR_REG_INDEX%,xbMET_Y20,		0x00010001,		32931	;0x80A3
HKR,%SENSOR_REG_INDEX%,xbMET_Y33,		0x00010001,		32932	;0x80A4
HKR,%SENSOR_REG_INDEX%,xbMET_Y32,		0x00010001,		32933	;0x80A5
HKR,%SENSOR_REG_INDEX%,xbMET_Y31,		0x00010001,		32934	;0x80A6
HKR,%SENSOR_REG_INDEX%,xbMET_Y30,		0x00010001,		32935	;0x80A7
HKR,%SENSOR_REG_INDEX%,xbMET_Y43,		0x00010001,		32936	;0x80A8
HKR,%SENSOR_REG_INDEX%,xbMET_Y42,		0x00010001,		32937	;0x80A9
HKR,%SENSOR_REG_INDEX%,xbMET_Y41,		0x00010001,		32938	;0x80AA
HKR,%SENSOR_REG_INDEX%,xbMET_Y40,		0x00010001,		32939	;0x80AB
HKR,%SENSOR_REG_INDEX%,xbMET_Y53,		0x00010001,		32940	;0x80AC
HKR,%SENSOR_REG_INDEX%,xbMET_Y52,		0x00010001,		32941	;0x80AD
HKR,%SENSOR_REG_INDEX%,xbMET_Y51,		0x00010001,		32942	;0x80AE
HKR,%SENSOR_REG_INDEX%,xbMET_Y50,		0x00010001,		32943	;0x80AF
HKR,%SENSOR_REG_INDEX%,xbMET_RED3,		0x00010001,		32944	;0x80B0
HKR,%SENSOR_REG_INDEX%,xbMET_RED2,		0x00010001,		32945	;0x80B1
HKR,%SENSOR_REG_INDEX%,xbMET_RED1,		0x00010001,		32946	;0x80B2
HKR,%SENSOR_REG_INDEX%,bMET_RED0,		0x00010001,		32947	;0x80B3
HKR,%SENSOR_REG_INDEX%,xbMET_GREEN3,		0x00010001,		32948	;0x80B4
HKR,%SENSOR_REG_INDEX%,xbMET_GREEN2,		0x00010001,		32949	;0x80B5
HKR,%SENSOR_REG_INDEX%,xbMET_GREEN1,		0x00010001,		32950	;0x80B6
HKR,%SENSOR_REG_INDEX%,xbMET_GREEN0,		0x00010001,		32951	;0x80B7
HKR,%SENSOR_REG_INDEX%,xbMET_BLUE3,		0x00010001,		32952	;0x80B8
HKR,%SENSOR_REG_INDEX%,xbMET_BLUE2,		0x00010001,		32953	;0x80B9
HKR,%SENSOR_REG_INDEX%,xbMET_BLUE1,		0x00010001,		32954	;0x80BA
HKR,%SENSOR_REG_INDEX%,xbMET_BLUE0,		0x00010001,		32955	;0x80BB
HKR,%SENSOR_REG_INDEX%,xbMET_RGBCNT3,		0x00010001,		32956	;0x80BC
HKR,%SENSOR_REG_INDEX%,xbMET_RGBCNT2,		0x00010001,		32957	;0x80BD
HKR,%SENSOR_REG_INDEX%,xbMET_RGBCNT1,		0x00010001,		32958	;0x80BE
HKR,%SENSOR_REG_INDEX%,xbMET_RGBCNT0,		0x00010001,		32959	;0x80BF
                     
HKR,%SENSOR_REG_INDEX%,xbMET_H03,		0x00010001,		32960	;0x80C0
HKR,%SENSOR_REG_INDEX%,xbMET_H02,		0x00010001,		32961	;0x80C1
HKR,%SENSOR_REG_INDEX%,xbMET_H01,		0x00010001,		32962	;0x80C2
HKR,%SENSOR_REG_INDEX%,xbMET_H00,		0x00010001,		32963	;0x80C3
HKR,%SENSOR_REG_INDEX%,xbMET_H13,		0x00010001,		32964	;0x80C4
HKR,%SENSOR_REG_INDEX%,xbMET_H12,		0x00010001,		32965	;0x80C5
HKR,%SENSOR_REG_INDEX%,xbMET_H11,		0x00010001,		32966	;0x80C6
HKR,%SENSOR_REG_INDEX%,xbMET_H10,		0x00010001,		32967	;0x80C7
HKR,%SENSOR_REG_INDEX%,xbMET_H23,		0x00010001,		32968	;0x80C8
HKR,%SENSOR_REG_INDEX%,xbMET_H22,		0x00010001,		32969	;0x80C9
HKR,%SENSOR_REG_INDEX%,xbMET_H21,		0x00010001,		32970	;0x80CA
HKR,%SENSOR_REG_INDEX%,xbMET_H20,		0x00010001,		32971	;0x80CB
HKR,%SENSOR_REG_INDEX%,xbMET_H33,		0x00010001,		32972	;0x80CC
HKR,%SENSOR_REG_INDEX%,xbMET_H32,		0x00010001,		32973	;0x80CD
HKR,%SENSOR_REG_INDEX%,xbMET_H31,		0x00010001,		32974	;0x80CE
HKR,%SENSOR_REG_INDEX%,xbMET_H30,		0x00010001,		32975	;0x80CF
HKR,%SENSOR_REG_INDEX%,xbMET_H43,		0x00010001,		32976	;0x80D0
HKR,%SENSOR_REG_INDEX%,xbMET_H42,		0x00010001,		32977	;0x80D1
HKR,%SENSOR_REG_INDEX%,xbMET_H41,		0x00010001,		32978	;0x80D2
HKR,%SENSOR_REG_INDEX%,xbMET_H40,		0x00010001,		32979	;0x80D3
HKR,%SENSOR_REG_INDEX%,xbMET_H53,		0x00010001,		32980	;0x80D4
HKR,%SENSOR_REG_INDEX%,xbMET_H52,		0x00010001,		32981	;0x80D5
HKR,%SENSOR_REG_INDEX%,xbMET_H51,		0x00010001,		32982	;0x80D6
HKR,%SENSOR_REG_INDEX%,xbMET_H50,		0x00010001,		32983	;0x80D7
HKR,%SENSOR_REG_INDEX%,xbMET_H63,		0x00010001,		32984	;0x80D8
HKR,%SENSOR_REG_INDEX%,xbMET_H62,		0x00010001,		32985	;0x80D9
HKR,%SENSOR_REG_INDEX%,xbMET_H61,		0x00010001,		32986	;0x80DA
HKR,%SENSOR_REG_INDEX%,xbMET_H60,		0x00010001,		32987	;0x80DB
HKR,%SENSOR_REG_INDEX%,xbMET_H73,		0x00010001,		32988	;0x80DC
HKR,%SENSOR_REG_INDEX%,xbMET_H72,		0x00010001,		32989	;0x80DD
HKR,%SENSOR_REG_INDEX%,xbMET_H71,		0x00010001,		32990	;0x80DE
HKR,%SENSOR_REG_INDEX%,xbMET_H70,		0x00010001,		32991	;0x80DF
HKR,%SENSOR_REG_INDEX%,xbMET_H83,		0x00010001,		32992	;0x80E0
HKR,%SENSOR_REG_INDEX%,xbMET_H82,		0x00010001,		32993	;0x80E1
HKR,%SENSOR_REG_INDEX%,xbMET_H81,		0x00010001,		32994	;0x80E2
HKR,%SENSOR_REG_INDEX%,xbMET_H80,		0x00010001,		32995	;0x80E3
HKR,%SENSOR_REG_INDEX%,xbMET_H93,		0x00010001,		32996	;0x80E4
HKR,%SENSOR_REG_INDEX%,xbMET_H92,		0x00010001,		32997	;0x80E5
HKR,%SENSOR_REG_INDEX%,xbMET_H91,		0x00010001,		32998	;0x80E6
HKR,%SENSOR_REG_INDEX%,xbMET_H90,		0x00010001,		32999	;0x80E7
HKR,%SENSOR_REG_INDEX%,xbMET_HA3,		0x00010001,		33000	;0x80E8
HKR,%SENSOR_REG_INDEX%,xbMET_HA2,		0x00010001,		33001	;0x80E9
HKR,%SENSOR_REG_INDEX%,xbMET_HA1,		0x00010001,		33002	;0x80EA
HKR,%SENSOR_REG_INDEX%,xbMET_HA0,		0x00010001,		33003	;0x80EB
HKR,%SENSOR_REG_INDEX%,xbMET_HB3,		0x00010001,		33004	;0x80EC
HKR,%SENSOR_REG_INDEX%,xbMET_HB2,		0x00010001,		33005	;0x80ED
HKR,%SENSOR_REG_INDEX%,xbMET_HB1,		0x00010001,		33006	;0x80EE
HKR,%SENSOR_REG_INDEX%,xbMET_HB0,		0x00010001,		33007	;0x80EF
HKR,%SENSOR_REG_INDEX%,xbMET_HC3,		0x00010001,		33008	;0x80F0
HKR,%SENSOR_REG_INDEX%,xbMET_HC2,		0x00010001,		33009	;0x80F1
HKR,%SENSOR_REG_INDEX%,xbMET_HC1,		0x00010001,		33010	;0x80F2
HKR,%SENSOR_REG_INDEX%,xbMET_HC0,		0x00010001,		33011	;0x80F3
HKR,%SENSOR_REG_INDEX%,xbMET_HD3,		0x00010001,		33012	;0x80F4
HKR,%SENSOR_REG_INDEX%,xbMET_HD2,		0x00010001,		33013	;0x80F5
HKR,%SENSOR_REG_INDEX%,xbMET_HD1,		0x00010001,		33014	;0x80F6
HKR,%SENSOR_REG_INDEX%,xbMET_HD0,		0x00010001,		33015	;0x80F7
HKR,%SENSOR_REG_INDEX%,xbMET_HE3,		0x00010001,		33016	;0x80F8
HKR,%SENSOR_REG_INDEX%,xbMET_HE2,		0x00010001,		33017	;0x80F9
HKR,%SENSOR_REG_INDEX%,xbMET_HE1,		0x00010001,		33018	;0x80FA
HKR,%SENSOR_REG_INDEX%,xbMET_HE0,		0x00010001,		33019	;0x80FB
HKR,%SENSOR_REG_INDEX%,xbMET_HF3,		0x00010001,		33020	;0x80FC
HKR,%SENSOR_REG_INDEX%,xbMET_HF2,		0x00010001,		33021	;0x80FD
HKR,%SENSOR_REG_INDEX%,xbMET_HF1,		0x00010001,		33022	;0x80FE
HKR,%SENSOR_REG_INDEX%,xbMET_HF0,		0x00010001,		33023	;0x80FF
                     
HKR,%SENSOR_REG_INDEX%,xbSensorType,	0x00010001,		0x8100
HKR,%SENSOR_REG_INDEX%,xbLineOfFrameH,	0x00010001,		0x8102
HKR,%SENSOR_REG_INDEX%,xbLineOfFrameL,	0x00010001,		0x8103
HKR,%SENSOR_REG_INDEX%,xbPixOfLineH,	0x00010001,		0x8104
HKR,%SENSOR_REG_INDEX%,xbPixOfLineL,	0x00010001,		0x8105
HKR,%SENSOR_REG_INDEX%,xbVSyncPort,		0x00010001,		0x8106
HKR,%SENSOR_REG_INDEX%,xbHSyncPort,		0x00010001,		0x8107
                     
HKR,%SENSOR_REG_INDEX%,xbHBlockNoJp,	0x00010001,		0x8160
HKR,%SENSOR_REG_INDEX%,xbVBlockNoJp,	0x00010001,		0x8161
HKR,%SENSOR_REG_INDEX%,xbJpegControl,	0x00010001,		0x8162
HKR,%SENSOR_REG_INDEX%,xbQTableIndex,	0x00010001,		0x8163
                     
HKR,%SENSOR_REG_INDEX%,xbSenClkControl,	0x00010001,		0x8180
HKR,%SENSOR_REG_INDEX%,xbSenClkDivision,0x00010001,		0x8181
HKR,%SENSOR_REG_INDEX%,xbCprClkControl,	0x00010001,		0x8182
HKR,%SENSOR_REG_INDEX%,xbCprClkDivision,0x00010001,		0x8183
HKR,%SENSOR_REG_INDEX%,xbMcuClkControl,	0x00010001,		0x8184
HKR,%SENSOR_REG_INDEX%,xbMcuClkDivision,0x00010001,		0x8185
HKR,%SENSOR_REG_INDEX%,xbDctClkControl,	0x00010001,		0x8186
HKR,%SENSOR_REG_INDEX%,xbDctClkDivision,0x00010001,		0x8187
HKR,%SENSOR_REG_INDEX%,xbEcClkControl,	0x00010001,		0x8188
HKR,%SENSOR_REG_INDEX%,xbEcClkDivision,	0x00010001,		0x8189
HKR,%SENSOR_REG_INDEX%,xbLbufClkControl,0x00010001,		33162	;0x818A
HKR,%SENSOR_REG_INDEX%,xbLbufClkDivision,0x00010001,		33163	;0x818B

HKR,%SENSOR_REG_INDEX%,xbInterFlag,		0x00010001,		0x8171
HKR,%SENSOR_REG_INDEX%,xbGPIODIRH,		0x00010001,		0x8172
HKR,%SENSOR_REG_INDEX%,xbGPIODATAH,		0x00010001,		0x8174
HKR,%SENSOR_REG_INDEX%,xbMISC_IO_DIR,	0x00010001,		0x8176
HKR,%SENSOR_REG_INDEX%,xbMISC_IO_DAT,	0x00010001,		0x8177
HKR,%SENSOR_REG_INDEX%,xbGpioDir,	    0x00010001,    	0x8173
HKR,%SENSOR_REG_INDEX%,xbGpioDat,		0x00010001,    	0x8175

HKR,%SENSOR_REG_INDEX%,obAC_Link_Control1,	    0x00010001,		0x8120
HKR,%SENSOR_REG_INDEX%,obAC_Link_Control2,	    0x00010001,		0x8121
HKR,%SENSOR_REG_INDEX%,obAC_Link_State,		    0x00010001,		0x8122
HKR,%SENSOR_REG_INDEX%,obPCM_SLOT_INDEX,	    0x00010001,		0x8124
HKR,%SENSOR_REG_INDEX%,obGPIO_SLOT_INDDEX,	    0x00010001,		0x8125
HKR,%SENSOR_REG_INDEX%,obAcRx_Status_AddressH,	0x00010001,		0x8128
HKR,%SENSOR_REG_INDEX%,obAcRx_Status_DataL,	    0x00010001,		0x8129
HKR,%SENSOR_REG_INDEX%,obAcRx_Status_DataH,	    0x00010001,		33066	;0x812A
HKR,%SENSOR_REG_INDEX%,obACTx_Command_Address,	0x00010001,		0x8131
HKR,%SENSOR_REG_INDEX%,obACTx_Command_DataL,	0x00010001,		0x8132
HKR,%SENSOR_REG_INDEX%,obACTx_Command_DataH,	0x00010001,		0x8133

HKR,%SENSOR_REG_INDEX%,xbEPEFCTR,		0x00010001,		33103	;0x814F
HKR,%SENSOR_REG_INDEX%,xbTestReg,		0x00010001,		0x8153
HKR,%SENSOR_REG_INDEX%,xbOBSFRAME,		0x00010001,		0x8156
HKR,%SENSOR_REG_INDEX%,xbMiscCtl,		0x00010001,		0x8170
HKR,%SENSOR_REG_INDEX%,xbEPAFCTR,		0x00010001,		0x8147
HKR,%SENSOR_REG_INDEX%,xbEPBFCTR,		0x00010001,		0x8149
HKR,%SENSOR_REG_INDEX%,xbSIF_Reset,		0x00010001,		0x8101
HKR,%SENSOR_REG_INDEX%,xbPwrCtl,		0x00010001,		0x8159
HKR,%SENSOR_REG_INDEX%,xbEPSETR0,		0x00010001,		0x8142
HKR,%SENSOR_REG_INDEX%,xbALT2SIZE,		0x00010001,		0x8154
HKR,%SENSOR_REG_INDEX%,xbALT3SIZE,		0x00010001,		0x8155
HKR,%SENSOR_REG_INDEX%,xbDEVCTR1,		0x00010001,		0x8141
HKR,%SENSOR_REG_INDEX%,xbFwVersionLSB,	0x00010001,		4095	;0x0FFF
HKR,%SENSOR_REG_INDEX%,xbFwVersionMSB,	0x00010001,		4094	;0x0FFE
HKR,%SENSOR_REG_INDEX%,xbFwMode0,		0x00010001,		4093	;0x0FFD
HKR,%SENSOR_REG_INDEX%,xbSnapShot,		0x00010001,		4092	;0x0FFC
HKR,%SENSOR_REG_INDEX%,xbFwMode1,		0x00010001,		4091	;0x0FFB
HKR,%SENSOR_REG_INDEX%,xbAeUpdateRate,	0x00010001,		4090	;0x0FFA
HKR,%SENSOR_REG_INDEX%,xbAwbMinB,		0x00010001,		4089	;0x0FF9
HKR,%SENSOR_REG_INDEX%,xbAwbMinG,		0x00010001,		4088	;0x0FF8
HKR,%SENSOR_REG_INDEX%,xbAwbMinR,		0x00010001,		4087	;0x0FF7
HKR,%SENSOR_REG_INDEX%,xbAwbMaxB,		0x00010001,		4086	;0x0FF6
HKR,%SENSOR_REG_INDEX%,xbAwbMaxG,		0x00010001,		4085	;0x0FF5
HKR,%SENSOR_REG_INDEX%,xbAwbMaxR,		0x00010001,		4084	;0x0FF4	
HKR,%SENSOR_REG_INDEX%,xbAeTargetLSB,	0x00010001,		4083	;0x0FF3
HKR,%SENSOR_REG_INDEX%,xbAeTargetMSB,	0x00010001,		4082	;0x0FF2
HKR,%SENSOR_REG_INDEX%,xbExposureIndex,	0x00010001,		4081	;0x0FF1
HKR,%SENSOR_REG_INDEX%,xbAeTabNum,		0x00010001,		4080	;0x0FF0
HKR,%SENSOR_REG_INDEX%,xbAeTabPosLSB,	0x00010001,		4079	;0x0FEF	
HKR,%SENSOR_REG_INDEX%,xbAeTabPosMSB,	0x00010001,		4078	;0x0FEE
HKR,%SENSOR_REG_INDEX%,xbExposureLSB,	0x00010001,		4075	;0x0FEB
HKR,%SENSOR_REG_INDEX%,xbExposureMSB,	0x00010001,		4074	;0x0FEA
HKR,%SENSOR_REG_INDEX%,xbI2CDevAddr,	0x00010001,		4073	;0x0FE9
HKR,%SENSOR_REG_INDEX%,xbI2CRegAddr,	0x00010001,		4072	;0x0FE8
HKR,%SENSOR_REG_INDEX%,xbLastAeInc,		0x00010001,		4071	;0x0FE7
HKR,%SENSOR_REG_INDEX%,xbLastAeDec,		0x00010001,		4070	;0x0FE6
HKR,%SENSOR_REG_INDEX%,xbAgcGain,		0x00010001,		4069	;0x0FE5
HKR,%SENSOR_REG_INDEX%,xbDebug,			0x00010001,		4068	;0x0FE4
HKR,%SENSOR_REG_INDEX%,xbFlickerTabBegin,	0x00010001,		4067	;0x0FE3
HKR,%SENSOR_REG_INDEX%,xbImageSize,		0x00010001,		4066	;0x0FE2
HKR,%SENSOR_REG_INDEX%,xbAgcmax,		0x00010001,		4065	;0x0FE1
HKR,%SENSOR_REG_INDEX%,xbAgcMin,		0x00010001,		4064	;0x0FE0
HKR,%SENSOR_REG_INDEX%,xbAeInc,			0x00010001,		4063	;0x0FDF
HKR,%SENSOR_REG_INDEX%,xbAeDec,			0x00010001,		4062	;0x0FDE

                                                                  
HKR,%SENSOR_REG_INDEX%,xb0F80,			0x00010001,		3968	;0x0F80
HKR,%SENSOR_REG_INDEX%,xb0F81,			0x00010001,		3969	;0x0F81
HKR,%SENSOR_REG_INDEX%,xb0F82,			0x00010001,		3970	;0x0F82
HKR,%SENSOR_REG_INDEX%,xb0F83,			0x00010001,		3971	;0x0F83
HKR,%SENSOR_REG_INDEX%,xb0F84,			0x00010001,		3972	;0x0F84
HKR,%SENSOR_REG_INDEX%,xb0F85,			0x00010001,		3973	;0x0F85
HKR,%SENSOR_REG_INDEX%,xb0F86,			0x00010001,		3974	;0x0F86
HKR,%SENSOR_REG_INDEX%,xb0F87,			0x00010001,		3975	;0x0F87
HKR,%SENSOR_REG_INDEX%,xb0F88,			0x00010001,		3976	;0x0F88
HKR,%SENSOR_REG_INDEX%,xb0F89,			0x00010001,		3977	;0x0F89
HKR,%SENSOR_REG_INDEX%,xb0F8A,			0x00010001,		3978	;0x0F8A
HKR,%SENSOR_REG_INDEX%,xb0F8B,			0x00010001,		3979	;0x0F8B
HKR,%SENSOR_REG_INDEX%,xb0F8C,			0x00010001,		3980	;0x0F8C
HKR,%SENSOR_REG_INDEX%,xb0F8D,			0x00010001,		3981	;0x0F8D
HKR,%SENSOR_REG_INDEX%,xb0F8E,			0x00010001,		3982	;0x0F8E
HKR,%SENSOR_REG_INDEX%,xb0F8F,			0x00010001,		3983	;0x0F8F
HKR,%SENSOR_REG_INDEX%,xb0F90,			0x00010001,		3984	;0x0F90
HKR,%SENSOR_REG_INDEX%,xb0F91,			0x00010001,		3985	;0x0F91
HKR,%SENSOR_REG_INDEX%,xb0F92,			0x00010001,		3986	;0x0F92
HKR,%SENSOR_REG_INDEX%,xb0F93,			0x00010001,		3987	;0x0F93
HKR,%SENSOR_REG_INDEX%,xb0F94,			0x00010001,		3988	;0x0F94
HKR,%SENSOR_REG_INDEX%,xb0F95,			0x00010001,		3989	;0x0F95
HKR,%SENSOR_REG_INDEX%,xb0F96,			0x00010001,		3990	;0x0F96
HKR,%SENSOR_REG_INDEX%,xb0F97,			0x00010001,		3991	;0x0F97
HKR,%SENSOR_REG_INDEX%,xb0F98,			0x00010001,		3992	;0x0F98
HKR,%SENSOR_REG_INDEX%,xb0F99,			0x00010001,		3993	;0x0F99
HKR,%SENSOR_REG_INDEX%,xb0F9A,			0x00010001,		3994	;0x0F9A
HKR,%SENSOR_REG_INDEX%,xb0F9B,			0x00010001,		3995	;0x0F9B
HKR,%SENSOR_REG_INDEX%,xb0F9C,			0x00010001,		3996	;0x0F9C
HKR,%SENSOR_REG_INDEX%,xb0F9D,			0x00010001,		3997	;0x0F9D
HKR,%SENSOR_REG_INDEX%,xb0F9E,			0x00010001,		3998	;0x0F9E
HKR,%SENSOR_REG_INDEX%,xb0F9F,			0x00010001,		3999	;0x0F9F
HKR,%SENSOR_REG_INDEX%,xb0FA0,			0x00010001,		4000	;0x0FA0
HKR,%SENSOR_REG_INDEX%,xb0FA1,			0x00010001,		4001	;0x0FA1
HKR,%SENSOR_REG_INDEX%,xb0FA2,			0x00010001,		4002	;0x0FA2
HKR,%SENSOR_REG_INDEX%,xb0FA3,			0x00010001,		4003	;0x0FA3
HKR,%SENSOR_REG_INDEX%,xb0FA4,			0x00010001,		4004	;0x0FA4
HKR,%SENSOR_REG_INDEX%,xb0FA5,			0x00010001,		4005	;0x0FA5
HKR,%SENSOR_REG_INDEX%,xb0FA6,			0x00010001,		4006	;0x0FA6
HKR,%SENSOR_REG_INDEX%,xb0FA7,			0x00010001,		4007	;0x0FA7
HKR,%SENSOR_REG_INDEX%,xb0FA8,			0x00010001,		4008	;0x0FA8
HKR,%SENSOR_REG_INDEX%,xb0FA9,			0x00010001,		4009	;0x0FA9
HKR,%SENSOR_REG_INDEX%,xb0FAA,			0x00010001,		4010	;0x0FAA
HKR,%SENSOR_REG_INDEX%,xb0FAB,			0x00010001,		4011	;0x0FAB
HKR,%SENSOR_REG_INDEX%,xb0FAC,			0x00010001,		4012	;0x0FAC
HKR,%SENSOR_REG_INDEX%,xb0FAD,			0x00010001,		4013	;0x0FAD
HKR,%SENSOR_REG_INDEX%,xb0FAE,			0x00010001,		4014	;0x0FAE
HKR,%SENSOR_REG_INDEX%,xb0FAF,			0x00010001,		4015	;0x0FAF
HKR,%SENSOR_REG_INDEX%,xb0FB0,			0x00010001,		4016	;0x0FB0
HKR,%SENSOR_REG_INDEX%,xb0FB1,			0x00010001,		4017	;0x0FB1
HKR,%SENSOR_REG_INDEX%,xb0FB2,			0x00010001,		4018	;0x0FB2
HKR,%SENSOR_REG_INDEX%,xb0FB3,			0x00010001,		4019	;0x0FB3
HKR,%SENSOR_REG_INDEX%,xb0FB4,			0x00010001,		4020	;0x0FB4
HKR,%SENSOR_REG_INDEX%,xb0FB5,			0x00010001,		4021	;0x0FB5
HKR,%SENSOR_REG_INDEX%,xb0FB6,			0x00010001,		4022	;0x0FB6
HKR,%SENSOR_REG_INDEX%,xb0FB7,			0x00010001,		4023	;0x0FB7
HKR,%SENSOR_REG_INDEX%,xb0FB8,			0x00010001,		4024	;0x0FB8
HKR,%SENSOR_REG_INDEX%,xb0FB9,			0x00010001,		4025	;0x0FB9
HKR,%SENSOR_REG_INDEX%,xb0FBA,			0x00010001,		4026	;0x0FBA
HKR,%SENSOR_REG_INDEX%,xb0FBB,			0x00010001,		4027	;0x0FBB
HKR,%SENSOR_REG_INDEX%,xb0FBC,			0x00010001,		4028	;0x0FBC
HKR,%SENSOR_REG_INDEX%,xb0FBD,			0x00010001,		4029	;0x0FBD
HKR,%SENSOR_REG_INDEX%,xb0FBE,			0x00010001,		4030	;0x0FBE
HKR,%SENSOR_REG_INDEX%,xb0FBF,			0x00010001,		4031	;0x0FBF
HKR,%SENSOR_REG_INDEX%,xb0FC0,			0x00010001,		4032	;0x0FC0
HKR,%SENSOR_REG_INDEX%,xb0FC1,			0x00010001,		4033	;0x0FC1
HKR,%SENSOR_REG_INDEX%,xb0FC2,			0x00010001,		4034	;0x0FC2
HKR,%SENSOR_REG_INDEX%,xb0FC3,			0x00010001,		4035	;0x0FC3
HKR,%SENSOR_REG_INDEX%,xb0FC4,			0x00010001,		4036	;0x0FC4
HKR,%SENSOR_REG_INDEX%,xb0FC5,			0x00010001,		4037	;0x0FC5
HKR,%SENSOR_REG_INDEX%,xb0FC6,			0x00010001,		4038	;0x0FC6
HKR,%SENSOR_REG_INDEX%,xb0FC7,			0x00010001,		4039	;0x0FC7
HKR,%SENSOR_REG_INDEX%,xb0FC8,			0x00010001,		4040	;0x0FC8
HKR,%SENSOR_REG_INDEX%,xb0FC9,			0x00010001,		4041	;0x0FC9
HKR,%SENSOR_REG_INDEX%,xb0FCA,			0x00010001,		4042	;0x0FCA
HKR,%SENSOR_REG_INDEX%,xb0FCB,			0x00010001,		4043	;0x0FCB
HKR,%SENSOR_REG_INDEX%,xb0FCC,			0x00010001,		4044	;0x0FCC
HKR,%SENSOR_REG_INDEX%,xb0FCD,			0x00010001,		4045	;0x0FCD
HKR,%SENSOR_REG_INDEX%,xb0FCE,			0x00010001,		4046	;0x0FCE
HKR,%SENSOR_REG_INDEX%,xb0FCF,			0x00010001,		4047	;0x0FCF
HKR,%SENSOR_REG_INDEX%,xb0FD0,			0x00010001,		4048	;0x0FD0
HKR,%SENSOR_REG_INDEX%,xb0FD1,			0x00010001,		4049	;0x0FD1
HKR,%SENSOR_REG_INDEX%,xb0FD2,			0x00010001,		4050	;0x0FD2
HKR,%SENSOR_REG_INDEX%,xb0FD3,			0x00010001,		4051	;0x0FD3
HKR,%SENSOR_REG_INDEX%,xb0FD4,			0x00010001,		4052	;0x0FD4
HKR,%SENSOR_REG_INDEX%,xb0FD5,			0x00010001,		4053	;0x0FD5
HKR,%SENSOR_REG_INDEX%,xb0FD6,			0x00010001,		4054	;0x0FD6
HKR,%SENSOR_REG_INDEX%,xb0FD7,			0x00010001,		4055	;0x0FD7
HKR,%SENSOR_REG_INDEX%,xb0FD8,			0x00010001,		4056	;0x0FD8
HKR,%SENSOR_REG_INDEX%,xb0FD9,			0x00010001,		4057	;0x0FD9
HKR,%SENSOR_REG_INDEX%,xb0FDA,			0x00010001,		4058	;0x0FDA
HKR,%SENSOR_REG_INDEX%,xb0FDB,			0x00010001,		4059	;0x0FDB
HKR,%SENSOR_REG_INDEX%,xb0FDC,			0x00010001,		4060	;0x0FDC
HKR,%SENSOR_REG_INDEX%,xb0FDD,			0x00010001,		4061	;0x0FDD
HKR,%SENSOR_REG_INDEX%,xb0FDE,			0x00010001,		4062	;0x0FDE
HKR,%SENSOR_REG_INDEX%,xb0FDF,			0x00010001,		4063	;0x0FDF
HKR,%SENSOR_REG_INDEX%,xb0FE0,			0x00010001,		4064	;0x0FE0
HKR,%SENSOR_REG_INDEX%,xb0FE1,			0x00010001,		4065	;0x0FE1
HKR,%SENSOR_REG_INDEX%,xb0FE2,			0x00010001,		4066	;0x0FE2
HKR,%SENSOR_REG_INDEX%,xb0FE3,			0x00010001,		4067	;0x0FE3
HKR,%SENSOR_REG_INDEX%,xbPreAmpR,		0x00010001,		4073	;0x0FE9
HKR,%SENSOR_REG_INDEX%,xbPreAmpB,		0x00010001,		4072	;0x0FE8
HKR,%SENSOR_REG_INDEX%,xbBrightness,	0x00010001,		4090	;0x0FFA

[Strings]
;----------------
; Non-Localizable
;----------------
ProxyVCap.CLSID = "{17CCA71B-ECD7-11D0-B908-00A0C9223196}"
KSCATEGORY_CAPTURE = "{65E8773D-8F56-11D0-A3B9-00A0C9223196}"
; note: only register value is case sensitive, key is not.
SERVICE_KERNEL_DRIVER=1
; PnP should use demand start
SERVICE_DEMAND_START=3
SERVICE_ERROR_NORMAL=1
;----------------
; Localizable
;----------------
DISK_NAME              = "BisonCam, Disk"
VENDOR                 = "WebCam"
Mfg    	               = "WebCam"
CamM5603C.DeviceId     = "VID_0402&PID_5603"
CamM5603C.DeviceDesc   = "BisonCam, USB2.0"
E_CamVfWWDMDriverDesc  = "BisonCam, USB2.0 Vfw"
CamM5603C.ExtensionDLL = "vfwExtC.dll"
MediaResourcesMSVideo  = "SYSTEM\CurrentControlSet\Control\MediaResources\msvideo"
MMDriverDesc           = "Software\Microsoft\Windows NT\CurrentVersion\drivers.desc"
MMDrivers              = "Software\Microsoft\Windows NT\CurrentVersion\Drivers32"
CAMERA_ENV_REGISTRY    = "Software\WebCam\M5603C"
CAMERA_USER_SETTING    = "Software\WebCam\M5603C\User"
CAMERA_DEFAULT_SETTING = "Software\WebCam\M5603C\Default"
CAMERA_DEBUG_SETTING   = "Software\WebCam\Debug"
CAMERA_DEBUG_REGREPORT = "Software\WebCam\Debug\RegReport"
CAMERA_REGISTER_ADDR   = "Software\WebCam\Debug\RegisterAddr"
CAMERA_EEPROM_SETTING  = "Software\WebCam\Debug\EEPROM"
SENSOR_REG_INDEX       = "SensorSetting"
InstallShiled.GUID     = "{C9E3ACAB-1A3B-4B67-A653-916F250ABAD4}"
