;****************************************************************************************
;
; RT2500.inf
;
;   This installation script supports Windows 98,Me,2000 & XP for the
;   Ralink RT2500 series Wireless LAN Card.
;
;   Copyright (c)2002-2004, Ralink Technology Corp., All Rights Reserved
;   All Rights Reserved.
;   Developed by RaLink Technology, Corp. -- http://www.ralinktech.com
;
;****************************************************************************************

[Version]
Signature       = "$Chicago$"
Class           = Net
ClassGUID       = {4d36e972-e325-11ce-bfc1-08002be10318}
Provider        = %Ralink%
Compatible      = 1
DriverVer       = 06/01/2006, 3.02.00.0000
CatalogFile     = RT2500.CAT

[ControlFlags]
;ExcludeFromSelect = PCI\VEN_1814&DEV_0201

[Manufacturer]
%Ralink%        = Ralink
%Asus%          = ASUS
%Delta%         = Delta
%ZINWELL%       = ZINWELL
%AMIT%          = AMIT
%CASTLENET%     = CASTLENET
%ACCTON%        = ACCTON
%Edimax%        = Edimax
%Hawking%       = Hawking
%Surecom%       = Surecom
%Gigabyte%      = Gigabyte
%Billionton%    = Billionton
%VTech%         = VTech
%Sitecom%       = Sitecom
%Siemens%       = Siemens
%Conceptronic%  = Conceptronic
%CNet%          = CNet

[Ralink]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%Ralink.DeviceDesc%         = RALINK.ndi,           PCI\VEN_1814&DEV_0201&SUBSYS_25601814
;
; QCOM They did not wamt to use their own manufacture name
;
%QCOM_PCMCIA.DeviceDesc%    = RALINK.ndi,           PCI\VEN_1814&DEV_0201&SUBSYS_615118E8
%QCOM_PCI.DeviceDesc%       = RALINK.ndi,           PCI\VEN_1814&DEV_0201&SUBSYS_614618E8
;
; MSI White box, they did not intend to use their company name
;
%M2500_6833.DeviceDesc%     = RALINK.ndi,           PCI\VEN_1814&DEV_0201&SUBSYS_68331462
%M2500_6834.DeviceDesc%     = RALINK.ndi,           PCI\VEN_1814&DEV_0201&SUBSYS_68341462
%M2500_6835.DeviceDesc%     = RALINK.ndi,           PCI\VEN_1814&DEV_0201&SUBSYS_68351462
;
; Winstron, they did not intend to use their company name
;
%WLANm.DeviceDesc%          = RALINK.ndi,           PCI\VEN_1814&DEV_0201&SUBSYS_12A0185F
%WLANc.DeviceDesc%          = RALINK.ndi,           PCI\VEN_1814&DEV_0201&SUBSYS_22A0185F
;
; Amigo, they did not intend to use their company name
;
%AMIGO.DeviceDesc1%         = RALINK.ndi,           PCI\VEN_1814&DEV_0201&SUBSYS_914016EF&REV_01
%AMIGO.DeviceDesc2%         = RALINK.ndi,           PCI\VEN_1814&DEV_0201&SUBSYS_922016EF&REV_01
%AMIGO.DeviceDesc3%         = RALINK.ndi,           PCI\VEN_1814&DEV_0201&SUBSYS_923016EF&REV_01
;
; CNet
;
%CNetCardbus.DeviceDesc%    = RALINK.ndi,           PCI\VEN_1814&DEV_0201&SUBSYS_001E1371
%CNetPCI.DeviceDesc%        = RALINK.ndi,           PCI\VEN_1814&DEV_0201&SUBSYS_00201371
%CNetMPCI.DeviceDesc%       = RALINK.ndi,           PCI\VEN_1814&DEV_0201&SUBSYS_001F1371

[ASUS]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%ASUS.DeviceDesc%           = ASUS.ndi,             PCI\VEN_1814&DEV_0201&SUBSYS_107F1043
%ASUS.DeviceDesc%           = ASUS.ndi,             PCI\VEN_1814&DEV_0201&SUBSYS_127F1043
%ASUS.DeviceDesc%           = ASUS.ndi,             PCI\VEN_1814&DEV_0201&SUBSYS_130F1043
%ASUS.DeviceDesc%           = ASUS.ndi,             PCI\VEN_1814&DEV_0201&SUBSYS_137F1043
%ASUSGEN.DeviceDesc%        = ASUS.ndi,             PCI\VEN_1814&DEV_0201&SUBSYS_137E1043

[Delta]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%DELTA.DeviceDesc%          = DELTA.NDI,            PCI\VEN_1814&DEV_0201&SUBSYS_70104033 

[ZINWELL]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%ZINWELLPCI.DeviceDesc%     = ZINWELL.ndi,          PCI\VEN_1814&DEV_0201&SUBSYS_03615A57
%ZINWELLMPCI.DeviceDesc%    = ZINWELL.ndi,          PCI\VEN_1814&DEV_0201&SUBSYS_03605A57
%ZINWELLCARD.DeviceDesc%    = ZINWELL.ndi,          PCI\VEN_1814&DEV_0201&SUBSYS_01605A57
%ZINWELLOEM1.DeviceDesc%    = ZINWELL.ndi,          PCI\VEN_1814&DEV_0201&SUBSYS_300918A3
%ZINWELLOEM2.DeviceDesc%    = ZINWELL.ndi,          PCI\VEN_1814&DEV_0201&SUBSYS_301018A3

[AMIT]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%AMIT.DeviceDesc%           = AMIT.ndi,             PCI\VEN_1814&DEV_0201&SUBSYS_531018EB
%AMITMINI.DeviceDesc%       = AMIT.ndi,             PCI\VEN_1814&DEV_0201&SUBSYS_531118EB
%AMITPCI.DeviceDesc%        = AMIT.ndi,             PCI\VEN_1814&DEV_0201&SUBSYS_531218EB

[CASTLENET]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%CASTLENET.DeviceDesc%      = CASTLENET.ndi,        PCI\VEN_1814&DEV_0201&SUBSYS_12801688

[ACCTON]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%WN4306A.DeviceDesc%        = WN4306A.ndi,          PCI\VEN_1814&DEV_0201&SUBSYS_43061113

[Edimax]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%Edimax7108.DeviceDesc%     = EDIMAX.ndi,           PCI\VEN_1814&DEV_0201&SUBSYS_71081432
%Edimax7128.DeviceDesc%     = EDIMAX.ndi,           PCI\VEN_1814&DEV_0201&SUBSYS_71281432

[Hawking]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%Hawking0C54.DeviceDesc%    = HAWKING.ndi,          PCI\VEN_1814&DEV_0201&SUBSYS_0C541432
%Hawking0B54.DeviceDesc%    = HAWKING.ndi,          PCI\VEN_1814&DEV_0201&SUBSYS_0B541432

[Surecom]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%SurecomCardbus.DeviceDesc% = SURECOM.ndi,          PCI\VEN_1814&DEV_0201&SUBSYS_942810bd
%SurecomPCI.DeviceDesc%     = SURECOM.ndi,          PCI\VEN_1814&DEV_0201&SUBSYS_932110bd
%SurecomMPCI.DeviceDesc%    = SURECOM.ndi,          PCI\VEN_1814&DEV_0201&SUBSYS_932210bd

[Gigabyte]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%GigabyteWMKG.DeviceDesc%   = GIGABYTE.ndi,         PCI\VEN_1814&DEV_0201&SUBSYS_E8311458
%GigabyteWIKG.DeviceDesc%   = GIGABYTE.ndi,         PCI\VEN_1814&DEV_0201&SUBSYS_E9311458
%GigabyteWPKG.DeviceDesc%   = GIGABYTE.ndi,         PCI\VEN_1814&DEV_0201&SUBSYS_E9321458

[Billionton]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%BILLIONTON_B.DeviceDesc%   = BILLIONTON.ndi,       PCI\VEN_1814&DEV_0201&SUBSYS_011014CB
%BILLIONTON_N.DeviceDesc%   = BILLIONTON.ndi,       PCI\VEN_1814&DEV_0201&SUBSYS_011114CB

[VTech]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%VTechPCI.DeviceDesc%       = VTECH.ndi,            PCI\VEN_1814&DEV_0201&SUBSYS_301118A3
%VTechCARD.DeviceDesc%      = VTECH.ndi,            PCI\VEN_1814&DEV_0201&SUBSYS_301318A3

[Sitecom]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%Sitecom_WL112.DeviceDesc%  = SITECOM.ndi,          PCI\VEN_1814&DEV_0201&SUBSYS_9070182D
%Sitecom_WL115.DeviceDesc%  = SITECOM.ndi,          PCI\VEN_1814&DEV_0201&SUBSYS_9073182D

[Siemens]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%Siemens.DeviceDesc%        = SIEMENS.ndi,          PCI\VEN_1814&DEV_0201&SUBSYS_3C800681

[Conceptronic]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%Conceptronic_PCCard.DeviceDesc% = CONCEPTRONIC.ndi,  PCI\VEN_1814&DEV_0201&SUBSYS_3C001948
%Conceptronic_PCICard.DeviceDesc% = CONCEPTRONIC.ndi, PCI\VEN_1814&DEV_0201&SUBSYS_3C011948

[CNet]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%CNetGPCI.DeviceDesc%       = CNET.ndi,             PCI\VEN_1814&DEV_0201&SUBSYS_61201371
%CNetGMPCI.DeviceDesc%      = CNET.ndi,             PCI\VEN_1814&DEV_0201&SUBSYS_71201371
%CNetGCB.DeviceDesc%        = CNET.ndi,             PCI\VEN_1814&DEV_0201&SUBSYS_81201371

;*******************************************************************************************
; Windows 9X specific entries
;*******************************************************************************************

[RALINK.ndi]
AddReg                  = PCI0201.ndi.reg, RT25009X.ndi.reg, Common.reg
CopyFiles               = win9x.CopyFiles

[DELTA.ndi]
AddReg                  = PCI0201.ndi.reg, RT25009X.ndi.reg, Common.reg
CopyFiles               = win9x.CopyFiles

[ASUS.ndi]
AddReg                  = PCI0201.ndi.reg, RT25009X.ndi.reg, Common.reg
CopyFiles               = win9x.CopyFiles

[ZINWELL.ndi]
AddReg                  = PCI0201.ndi.reg, RT25009X.ndi.reg, Common.reg
CopyFiles               = win9x.CopyFiles
    
[AMIT.ndi]
AddReg                  = PCI0201.ndi.reg, RT25009X.ndi.reg, Common.reg
CopyFiles               = win9x.CopyFiles

[CASTLENET.ndi]
AddReg                  = PCI0201.ndi.reg, RT25009X.ndi.reg, Common.reg
CopyFiles               = win9x.CopyFiles

[WN4306A.ndi]
AddReg                  = PCI0201.ndi.reg, RT25009X.ndi.reg, Common.reg
CopyFiles               = win9x.CopyFiles

[EDIMAX.ndi]
AddReg                  = PCI0201.ndi.reg, RT25009X.ndi.reg, Common.reg
CopyFiles               = win9x.CopyFiles

[HAWKING.ndi]
AddReg                  = PCI0201.ndi.reg, RT25009X.ndi.reg, Common.reg
CopyFiles               = win9x.CopyFiles

[SURECOM.ndi]
AddReg                  = PCI0201.ndi.reg, RT25009X.ndi.reg, Common.reg
CopyFiles               = win9x.CopyFiles

[GIGABYTE.ndi]
AddReg                  = PCI0201.ndi.reg, RT25009X.ndi.reg, Common.reg
CopyFiles               = win9x.CopyFiles

[BILLIONTON.ndi]
AddReg                  = PCI0201.ndi.reg, RT25009X.ndi.reg, Common.reg
CopyFiles               = win9x.CopyFiles

[VTECH.ndi]
AddReg                  = PCI0201.ndi.reg, RT25009X.ndi.reg, Common.reg
CopyFiles               = win9x.CopyFiles

[SITECOM.ndi]
AddReg                  = PCI0201.ndi.reg, RT25009X.ndi.reg, Common.reg
CopyFiles               = win9x.CopyFiles

[SIEMENS.ndi]
AddReg                  = PCI0201.ndi.reg, RT25009X.ndi.reg, Common.reg
CopyFiles               = win9x.CopyFiles

[CONCEPTRONIC.ndi]
AddReg                  = PCI0201.ndi.reg, RT25009X.ndi.reg, Common.reg
CopyFiles               = win9x.CopyFiles

[CNET.ndi]
AddReg                  = PCI0201.ndi.reg, RT25009X.ndi.reg, Common.reg
CopyFiles               = win9x.CopyFiles

;*******************************************************************************************
; NT specific entries
;*******************************************************************************************

[RALINK.ndi.NT]
AddReg                  = Common.reg, RT2500.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5
CopyFiles               = NT.CopyFiles

[DELTA.ndi.NT]
AddReg                  = Common.reg, RT2500.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5
CopyFiles               = NT.CopyFiles

[ASUS.ndi.NT]
AddReg                  = Common.reg, RT2500.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5
CopyFiles               = NT.CopyFiles

[ZINWELL.ndi.NT]
AddReg                  = Common.reg, RT2500.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5
CopyFiles               = NT.CopyFiles

[AMIT.ndi.NT]
AddReg                  = Common.reg, RT2500.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5
CopyFiles               = NT.CopyFiles

[CASTLENET.ndi.NT]
AddReg                  = Common.reg, RT2500.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5
CopyFiles               = NT.CopyFiles

[WN4306A.ndi.NT]
AddReg                  = Common.reg, RT2500.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5
CopyFiles               = NT.CopyFiles

[EDIMAX.ndi.NT]
AddReg                  = Common.reg, RT2500.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5
CopyFiles               = NT.CopyFiles

[HAWKING.ndi.NT]
AddReg                  = Common.reg, RT2500.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5
CopyFiles               = NT.CopyFiles

[SURECOM.ndi.NT]
AddReg                  = Common.reg, RT2500.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5
CopyFiles               = NT.CopyFiles

[GIGABYTE.ndi.NT]
AddReg                  = Common.reg, RT2500.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5
CopyFiles               = NT.CopyFiles

[BILLIONTON.ndi.NT]
AddReg                  = Common.reg, RT2500.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5
CopyFiles               = NT.CopyFiles

[VTECH.ndi.NT]
AddReg                  = Common.reg, RT2500.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5
CopyFiles               = NT.CopyFiles

[SITECOM.ndi.NT]
AddReg                  = Common.reg, RT2500.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5
CopyFiles               = NT.CopyFiles

[SIEMENS.ndi.NT]
AddReg                  = Common.reg, RT2500.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5
CopyFiles               = NT.CopyFiles

[CONCEPTRONIC.ndi.NT]
AddReg                  = Common.reg, RT2500.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5
CopyFiles               = NT.CopyFiles

[CNET.ndi.NT]
AddReg                  = Common.reg, RT2500.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5
CopyFiles               = NT.CopyFiles

; NT services sections
[RALINK.ndi.NT.Services]
AddService              = RT2500, 2, RALINK.Service, common.EventLog

[DELTA.ndi.NT.Services]
AddService              = RT2500, 2, DELTA.Service, common.EventLog

[ASUS.ndi.NT.Services]
AddService              = RT2500, 2, ASUS.Service, common.EventLog

[ZINWELL.ndi.NT.Services]
AddService              = RT2500, 2, ZINWELL.Service, common.EventLog

[AMIT.ndi.NT.Services]
AddService              = RT2500, 2, AMIT.Service, common.EventLog

[CASTLENET.ndi.NT.Services]
AddService              = RT2500, 2, CASTLENET.Service, common.EventLog

[WN4306A.ndi.NT.Services]
AddService              = RT2500, 2, WN4306A.Service, common.EventLog

[EDIMAX.ndi.NT.Services]
AddService              = RT2500, 2, EDIMAX.Service, common.EventLog

[HAWKING.ndi.NT.Services]
AddService              = RT2500, 2, HAWKING.Service, common.EventLog

[SURECOM.ndi.NT.Services]
AddService              = RT2500, 2, SURECOM.Service, common.EventLog

[GIGABYTE.ndi.NT.Services]
AddService              = RT2500, 2, GIGABYTE.Service, common.EventLog

[BILLIONTON.ndi.NT.Services]
AddService              = RT2500, 2, BILLIONTON.Service, common.EventLog

[VTECH.ndi.NT.Services]
AddService              = RT2500, 2, VTECH.Service, common.EventLog

[SITECOM.ndi.NT.Services]
AddService              = RT2500, 2, SITECOM.Service, common.EventLog

[SIEMENS.ndi.NT.Services]
AddService              = RT2500, 2, SIEMENS.Service, common.EventLog

[CONCEPTRONIC.ndi.NT.Services]
AddService              = RT2500, 2, CONCEPTRONIC.Service, common.EventLog

[CNET.ndi.NT.Services]
AddService              = RT2500, 2, CNET.Service, common.EventLog

;*******************************************************************************************
; common regs for NT and W9x
;*******************************************************************************************

[Common.reg]
;*******************************************************************************************
; System Level Property

;
; Current Profile
;
HKR, ,                    CurProfile,      0,""
HKR, Default,             CurProfile,      0,""

;
; Radio On/Off
;
HKR, ,                            Radio,           0, "0"
HKR, NDI\params\Radio,            ParamDesc,       0, "Radio On/Off"
HKR, NDI\params\Radio,            type,            0, "enum"
HKR, NDI\params\Radio,            default,         0, "0"
HKR, NDI\params\Radio\enum,       1,               0, "Disable"
HKR, NDI\params\Radio\enum,       0,               0, "Enable"

;
; Auto Reconnect Mode
;
HKR, ,                                  AutoReconnect,      0, "1"
HKR, NDI\params\AutoReconnect,          ParamDesc,          0, "Auto Reconnect Mode"
HKR, NDI\params\AutoReconnect,          type,               0, "enum"
HKR, NDI\params\AutoReconnect,          default,            0, "1"
HKR, NDI\params\AutoReconnect\enum,     0,                  0, "Disable"
HKR, NDI\params\AutoReconnect\enum,     1,                  0, "Enable"

;
; Show Hidden SSID in Site Survey Page
;
HKR, ,                                  ShowHiddenSSID,     0, "0"   ; 0=disable(default), 1=enable

;
; Country Region 
;
HKR, ,                                  CountryRegion,      0, "0"
HKR, NDI\params\CountryRegion,         ParamDesc,          0, "Country Region"
HKR, NDI\params\CountryRegion,         type,               0, "enum"
HKR, NDI\params\CountryRegion,         default,            0, "0"
HKR, NDI\params\CountryRegion\enum,    0,                  0, "FCC (Channel 1 - 11)"
HKR, NDI\params\CountryRegion\enum,    1,                  0, "IC (Channel 1 - 11)"
HKR, NDI\params\CountryRegion\enum,    2,                  0, "ETSI (Channel 1 - 13)"
HKR, NDI\params\CountryRegion\enum,    3,                  0, "Spain (Channel 10 - 11)"
HKR, NDI\params\CountryRegion\enum,    4,                  0, "France (Channel 10 - 13)"
HKR, NDI\params\CountryRegion\enum,    5,                  0, "MKK (Channel 14)"
HKR, NDI\params\CountryRegion\enum,    6,                  0, "MKK1 (Channel 1 - 14)"
HKR, NDI\params\CountryRegion\enum,    7,                  0, "Israel (Channel 3 - 9)"

;*******************************************************************************************
; Advance Page

;
; WirelessMode
;
HKR, ,                            WirelessMode,    0, "0"

;
; Enable TX Burst
;
HKR, ,                            TXBurst,         0, "0"

;
; Use Short Slot Time
;
HKR, ,                            ShortSlot,       0, "0"

;
; Use Turbo rate
;
HKR, ,                            TurboRate,       0, "0"

;
; Use Ofdm rate in adhoc mode
;
HKR, ,                            AdhocOfdm,       0, "0"

;
; Use BG Protection
;
HKR, ,                            BGProtection,    0, "0"

;
; CCX2 control
;
HKR, ,                            CCX2Control,     0x00010001, 0x00fa4600

;
; Vendor Description
;
HKR, ,                            VendorDesc,      0, %VENDOR_DESC_DEF_STR%
HKR, Default,                     VendorDesc,      0, %VENDOR_DESC_DEF_STR%

;*******************************************************************************************
; Profile

;
; SSID
;
HKR, ,                            SSID,            0, %SSID_DEF_STR%
HKR, Default,                     SSID,            0, %SSID_DEF_STR%
HKR, NDI\params\SSID,             ParamDesc,       0, "SSID"
HKR, NDI\params\SSID,             type,            0, "edit"
HKR, NDI\params\SSID,             limitText,       0, "32"
HKR, NDI\params\SSID,             default,         0, %SSID_DEF_STR%

;
; Network Type
;
HKR, ,                            NetworkType,     0, %NETWORK_TYPE_DEF_STR%
HKR, Default,                     NetworkType,     0, %NETWORK_TYPE_DEF_STR%
HKR, NDI\params\NetworkType,      ParamDesc,       0, "Network Type"
HKR, NDI\params\NetworkType,      type,            0, "enum"
HKR, NDI\params\NetworkType,      default,         0, %NETWORK_TYPE_DEF_STR%
HKR, NDI\params\NetworkType\enum, 0,               0, "802.11 Ad Hoc"
HKR, NDI\params\NetworkType\enum, 1,               0, "Infrastructure"

;
; Channel
;
HKR, ,                            Channel,         0, %CHANNEL%
HKR, Default,                     Channel,         0, %CHANNEL%


;*******************************************************************************************
; System Configuration Page

;
; Local Administration MAC Network Address
;
HKR, ,                            NetworkAddress,  0, ""
HKR, Default,                     NetworkAddress,  0, ""
HKR, NDI\params\NetworkAddress,   ParamDesc,       0, "Local Administration MAC Network Address"
HKR, NDI\params\NetworkAddress,   type,            0, "edit"
HKR, NDI\params\NetworkAddress,   limitText,       0, "12"
HKR, NDI\params\NetworkAddress,   default,         0, ""

;
; Power Saving Mode
;
HKR, ,                            PSMode,          0, "0"
HKR, Default,                     PSMode,          0, "0"
HKR, NDI\params\PSMode,           ParamDesc,       0, "Power Saving Mode"
HKR, NDI\params\PSMode,           type,            0, "enum"
HKR, NDI\params\PSMode,           default,         0, "0"
HKR, NDI\params\PSMode\enum,      0,               0, "CAM (Constantly Awake Mode)"
HKR, NDI\params\PSMode\enum,      1,               0, "Max_PSP (Max Power Savings)"
HKR, NDI\params\PSMode\enum,      2,               0, "Fast_PSP (Power Save Mode)"

;
; CAM when AC Power
;
HKR, ,                            ACPowerCam,      0, "0"
HKR, Default,                     ACPowerCam,      0, "0"
HKR, NDI\params\ACPowerCam,       ParamDesc,       0, "CAM when AC Power"
HKR, NDI\params\ACPowerCam,       type,            0, "enum"
HKR, NDI\params\ACPowerCam,       default,         0, "0"
HKR, NDI\params\ACPowerCam\enum,  0,               0, "Disable"
HKR, NDI\params\ACPowerCam\enum,  1,               0, "Enable"

;
; Preamble Type
;
HKR, ,                            PreambleType,    0, "0"
HKR, Default,                     PreambleType,    0, "0"

;
; TX Power
;
HKR, ,                            TXPower,         0, "0"
HKR, Default,                     TXPower,         0, "0"

;
; RTS Threshold
;
HKR, ,                            RTSThresh,       0, "2347"
HKR, Default,                     RTSThresh,       0, "2347"
HKR, NDI\params\RTSThresh,        ParamDesc,       0, "RTS Threshold"
HKR, NDI\params\RTSThresh,        type,            0, "int"
HKR, Ndi\params\RTSThresh,        default,         0, "2347"
HKR, NDI\params\RTSThresh,        min,             0, "0"
HKR, NDI\params\RTSThresh,        max,             0, "2347"
HKR, NDI\params\RTSThresh,        step,            0, "32"
HKR, NDI\params\RTSThresh,        optional,        0, "0"

;
; Fragment Threshold
;
HKR, ,                            FragThresh,      0, "2346"
HKR, Default,                     FragThresh,      0, "2346"
HKR, NDI\params\FragThresh,       ParamDesc,       0, "Fragment Threshold"
HKR, NDI\params\FragThresh,       type,            0, "int"
HKR, Ndi\params\FragThresh,       default,         0, "2346"
HKR, NDI\params\FragThresh,       min,             0, "256"
HKR, NDI\params\FragThresh,       max,             0, "2346"
HKR, NDI\params\FragThresh,       step,            0, "32"
HKR, NDI\params\FragThresh,       optional,        0, "0"

;*******************************************************************************************
; Authentication & Security Page

;
; Authentication Type
;
HKR, ,                AuthenType,      0, "0" ; Open System
HKR, Default,         AuthenType,      0, "0"

;
; Encryption
;
HKR, ,                Encryption,      0, "1" ; Disable
HKR, Default,         Encryption,      0, "1"

;
; WEP Keys Length
;
HKR, ,                WEPKeyLen,       0, "0"
HKR, Default,         WEPKeyLen,       0, "0"

;
; WEP Key to use
;
HKR, ,                WEPKeyUse,       0,"1"
HKR, Default,         WEPKeyUse,       0,"1"

;
; WEP Key1
;
HKR, ,                WEPKey1,         0,""
HKR, Default,         WEPKey1,         0,""

;
; WEP Key2
;
HKR, ,                WEPKey2,         0,""
HKR, Default,         WEPKey2,         0,""

;
; WEP Key3
;
HKR, ,                WEPKey3,         0,""
HKR, Default,         WEPKey3,         0,""

;
; WEP Key4
;
HKR, ,                WEPKey4,         0,""
HKR, Default,         WEPKey4,         0,""

;
; WPA PSK
;
HKR, ,                WPAPSK,          0, ""
HKR, Default,         WPAPSK,          0, ""

;*******************************************************************************************
; 802.1x & LEAP

;
; Use 8021X
;
HKR, ,                Use8021X,        0, "0"
HKR, Default,         Use8021X,        0, "0"
 
;
; Authen Protocol
;
HKR, ,                AuthenProtocol,  0, "0"
HKR, Default,         AuthenProtocol,  0, "0"

;
; Tunnel Protocol
;
HKR, ,                TunnelProtocol,  0, "3"
HKR, Default,         TunnelProtocol,  0, "3"

;
; ID
;
HKR, ,                ID,              0, ""
HKR, Default,         ID,              0, ""

;
; Password
;
HKR, ,                Password,        0, ""
HKR, Default,         Password,        0, ""

;
; Tunnel ID
;
HKR, ,                TunnelID,        0, ""
HKR, Default,         TunnelID,        0, ""

;
; Tunnel Password
;
HKR, ,                TunnelPassword,  0, ""
HKR, Default,         TunnelPassword,  0, ""

;
; Session Resumption
;
HKR, ,                SessionResumption, 0, "0"
HKR, Default,         SessionResumption, 0, "0"

;
; Password Mode
;
HKR, ,                PasswordMode,    0, "1"
HKR, Default,         PasswordMode,    0, "1"

;
; Use Client Cert
;
HKR, ,                UseClientCert,   0, "0"
HKR, Default,         UseClientCert,   0, "0"

;
; Use Server Cert
;
HKR, ,                UseServerCert,   0, "0"
HKR, Default,         UseServerCert,   0, "0"

;
; Client Cert Len
;
HKR, ,                ClientCertLen,   0, "0"
HKR, Default,         ClientCertLen,   0, "0"

;
; Client Cert Data
;
HKR, ,                ClientCertData,  0, ""
HKR, Default,         ClientCertData,  0, ""

;
; Server Cert Len
;
HKR, ,                ServerCertLen,   0, "0"
HKR, Default,         ServerCertLen,   0, "0"

;
; Server Cert Data
;
HKR, ,                ServerCertData,  0, ""
HKR, Default,         ServerCertData,  0, ""

;
; Server Name
;
HKR, ,                ServerName,      0, ""
HKR, Default,         ServerName,      0, ""

;
; Name Rule
;
HKR, ,                NameRule,        0, "0"
HKR, Default,         NameRule,        0, "0"

;
; Intermediate Cert
;
HKR, ,                IntermediateCert, 0, "0"
HKR, Default,         IntermediateCert, 0, "0"

;
; Leap Enabled
;
HKR, ,                LeapEnabled,     0, "0"
HKR, Default,         LeapEnabled,     0, "0"

;
; Leap User Name
;
HKR, ,                LeapUserName,    0, ""
HKR, Default,         LeapUserName,    0, ""

;
; Leap Password
;
HKR, ,                LeapPassword,    0, ""
HKR, Default,         LeapPassword,    0, ""


;*******************************************************************************************
; APConfig use
;

;
; WPA Group-Key ReKey Interval
;
HKR, ,                RekeyInterval,   0, "60"

;
; WPA Group-Key ReKey Method
;
HKR, ,                RekeyMethod,     0, "0"


[PCI0201.ndi.reg]
HKR, Ndi,                         DeviceID,         0, "PCI\VEN_1814&DEV_0201"

[RT25009X.ndi.reg]
HKR, ,                            NTMPDriver,       0, RT25009x.sys

HKR, ,                            BusType,          0, 5
HKR, NDI,                         CardType,         0, "PCI"

HKR, ,                            RunningWin9X,     0, "1"
HKR, ,                            DevLoader,        0, "*ndis"
HKR, ,                            DeviceVxDs,       0, "RT25009x.sys"
HKR, ,                            EnumPropPages,    0, "netdi.dll,EnumPropPages"

HKR, Ndi\Interfaces,              DefUpper,         0, "ndis3"
HKR, Ndi\Interfaces,              DefLower,         0, "ethernet"
HKR, Ndi\Interfaces,              UpperRange,       0, "ndis3"
HKR, Ndi\Interfaces,              LowerRange,       0, "ethernet"

HKR, NDIS,                        LogDriverName,    0, "RT25009X"
HKR, NDIS,                        MajorNdisVersion, 1, 03
HKR, NDIS,                        MinorNdisVersion, 1, 0A

;*******************************************************************************************
; DestinationDirs
;*******************************************************************************************

[DestinationDirs]
NT.CopyFiles            = 12    ; system32\drivers subdirectory on NT
XP.CopyFiles            = 12    ; system32\drivers subdirectory on Windows XP
win9x.CopyFiles         = 11    ; system32 subdirectory on win9x

[NT.CopyFiles]
RT2500.sys                      ; NT Installation

[XP.CopyFiles]
RT2500.sys                      ; XP Installation

[win9x.CopyFiles]
RT25009x.sys                    ; Win9x Installation

[SourceDisksNames]
1                       = %INSTALL_DISK_STR%,,,

[SourceDisksFiles] 
RT2500.sys              = 1
RT25009x.sys            = 1


;*******************************************************************************************
; NT specific
;*******************************************************************************************
[RT2500.ndi.NT.reg]
HKR, Ndi,                   Service,            0, "RT2500"
HKR, Ndi\Interfaces,        UpperRange,         0, "ndis5"
HKR, Ndi\Interfaces,        LowerRange,         0, "ethernet"

[RALINK.Service]
DisplayName                 = %RALINK.Service.DispName%
ServiceType                 = 1                             ;%SERVICE_KERNEL_DRIVER%
StartType                   = 3                             ;%SERVICE_AUTO_START%
ErrorControl                = 1                             ;%SERVICE_ERROR_NORMAL%
ServiceBinary               = %12%\RT2500.sys
LoadOrderGroup              = NDIS

[DELTA.Service]
DisplayName                 = %DELTA.Service.DispName%
ServiceType                 = 1                             ;%SERVICE_KERNEL_DRIVER%
StartType                   = 3                             ;%SERVICE_AUTO_START%
ErrorControl                = 1                             ;%SERVICE_ERROR_NORMAL%
ServiceBinary               = %12%\RT2500.sys
LoadOrderGroup              = NDIS

[ASUS.Service]
DisplayName                 = %ASUS.Service.DispName%
ServiceType                 = 1                             ;%SERVICE_KERNEL_DRIVER%
StartType                   = 3                             ;%SERVICE_AUTO_START%
ErrorControl                = 1                             ;%SERVICE_ERROR_NORMAL%
ServiceBinary               = %12%\RT2500.sys
LoadOrderGroup              = NDIS

[ZINWELL.Service]
DisplayName                = %ZINWELL.Service.DispName%
ServiceType                 = 1                             ;%SERVICE_KERNEL_DRIVER%
StartType                   = 3                             ;%SERVICE_AUTO_START%
ErrorControl                = 1                             ;%SERVICE_ERROR_NORMAL%
ServiceBinary               = %12%\RT2500.sys
LoadOrderGroup              = NDIS

[AMIT.Service]
DisplayName                 = %AMIT.Service.DispName%
ServiceType                 = 1                             ;%SERVICE_KERNEL_DRIVER%
StartType                   = 3                             ;%SERVICE_AUTO_START%
ErrorControl                = 1                             ;%SERVICE_ERROR_NORMAL%
ServiceBinary               = %12%\RT2500.sys
LoadOrderGroup              = NDIS

[CASTLENET.Service]
DisplayName                 = %CASTLENET.Service.DispName%
ServiceType                 = 1                             ;%SERVICE_KERNEL_DRIVER%
StartType                   = 3                             ;%SERVICE_AUTO_START%
ErrorControl                = 1                             ;%SERVICE_ERROR_NORMAL%
ServiceBinary               = %12%\RT2500.sys
LoadOrderGroup              = NDIS

[WN4306A.Service]
DisplayName                 = %WN4306A.Service.DispName%
ServiceType                 = 1                             ;%SERVICE_KERNEL_DRIVER%
StartType                   = 3                             ;%SERVICE_AUTO_START%
ErrorControl                = 1                             ;%SERVICE_ERROR_NORMAL%
ServiceBinary               = %12%\RT2500.sys
LoadOrderGroup              = NDIS

[EDIMAX.Service]
DisplayName                 = %EDIMAX.Service.DispName%
ServiceType                 = 1                             ;%SERVICE_KERNEL_DRIVER%
StartType                   = 3                             ;%SERVICE_AUTO_START%
ErrorControl                = 1                             ;%SERVICE_ERROR_NORMAL%
ServiceBinary               = %12%\RT2500.sys
LoadOrderGroup              = NDIS

[HAWKING.Service]
DisplayName                 = %HAWKING.Service.DispName%
ServiceType                 = 1                             ;%SERVICE_KERNEL_DRIVER%
StartType                   = 3                             ;%SERVICE_AUTO_START%
ErrorControl                = 1                             ;%SERVICE_ERROR_NORMAL%
ServiceBinary               = %12%\RT2500.sys
LoadOrderGroup              = NDIS

[SURECOM.Service]
DisplayName                 = %SURECOM.Service.DispName%
ServiceType                 = 1                             ;%SERVICE_KERNEL_DRIVER%
StartType                   = 3                             ;%SERVICE_AUTO_START%
ErrorControl                = 1                             ;%SERVICE_ERROR_NORMAL%
ServiceBinary               = %12%\RT2500.sys
LoadOrderGroup              = NDIS

[GIGABYTE.Service]
DisplayName                 = %Gigabyte.Service.DispName%
ServiceType                 = 1                             ;%SERVICE_KERNEL_DRIVER%
StartType                   = 3                             ;%SERVICE_AUTO_START%
ErrorControl                = 1                             ;%SERVICE_ERROR_NORMAL%
ServiceBinary               = %12%\RT2500.sys
LoadOrderGroup              = NDIS

[BILLIONTON.Service]
DisplayName                 = %BILLIONTON.Service.DispName%
ServiceType                 = 1                             ;%SERVICE_KERNEL_DRIVER%
StartType                   = 3                             ;%SERVICE_AUTO_START%
ErrorControl                = 1                             ;%SERVICE_ERROR_NORMAL%
ServiceBinary               = %12%\RT2500.sys
LoadOrderGroup              = NDIS

[VTECH.Service]
DisplayName                 = %VTECH.Service.DispName%
ServiceType                 = 1                             ;%SERVICE_KERNEL_DRIVER%
StartType                   = 3                             ;%SERVICE_AUTO_START%
ErrorControl                = 1                             ;%SERVICE_ERROR_NORMAL%
ServiceBinary               = %12%\RT2500.sys
LoadOrderGroup              = NDIS

[SITECOM.Service]
DisplayName                 = %SITECOM.Service.DispName%
ServiceType                 = 1                             ;%SERVICE_KERNEL_DRIVER%
StartType                   = 3                             ;%SERVICE_AUTO_START%
ErrorControl                = 1                             ;%SERVICE_ERROR_NORMAL%
ServiceBinary               = %12%\RT2500.sys
LoadOrderGroup              = NDIS

[SIEMENS.Service]
DisplayName                 = %SIEMENS.Service.DispName%
ServiceType                 = 1                             ;%SERVICE_KERNEL_DRIVER%
StartType                   = 3                             ;%SERVICE_AUTO_START%
ErrorControl                = 1                             ;%SERVICE_ERROR_NORMAL%
ServiceBinary               = %12%\RT2500.sys
LoadOrderGroup              = NDIS

[CONCEPTRONIC.Service]
DisplayName                 = %CONCEPTRONIC.Service.DispName%
ServiceType                 = 1                             ;%SERVICE_KERNEL_DRIVER%
StartType                   = 3                             ;%SERVICE_AUTO_START%
ErrorControl                = 1                             ;%SERVICE_ERROR_NORMAL%
ServiceBinary               = %12%\RT2500.sys
LoadOrderGroup              = NDIS

[CNET.Service]
DisplayName                 = %CNET.Service.DispName%
ServiceType                 = 1                             ;%SERVICE_KERNEL_DRIVER%
StartType                   = 3                             ;%SERVICE_AUTO_START%
ErrorControl                = 1                             ;%SERVICE_ERROR_NORMAL%
ServiceBinary               = %12%\RT2500.sys
LoadOrderGroup              = NDIS

[common.EventLog]
AddReg=common.AddEventLog.reg

[common.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll,%%SystemRoot%%\System32\drivers\RT2500.sys"
HKR, , TypesSupported,   0x00010001, 7



;*******************************************************************************************
; Strings
;*******************************************************************************************
[Strings]
Ralink                      = "Ralink Technology, Inc."
Asus                        = "ASUSTeK Computer Inc."
Delta                       = "Delta Networks, Inc."
ZINWELL                     = "ZINWELL Technology, Inc."
AMIT                        = "AMIT Technology, Inc."
CASTLENET                   = "CastleNet Technology, Inc."
ACCTON                      = "Accton Technology Corporation"
Edimax                      = "Edimax Technology Co., Ltd."
Hawking                     = "Hawking Technologies, Inc."
Surecom                     = "Surecom Technology, Inc."
Gigabyte                    = "Gigabyte Technology Corp."
Billionton                  = "Billionton Systems Inc."
VTech                       = "VTech Telecommunications Ltd"
Sitecom                     = "Sitecom"
Siemens                     = "Siemens"
Conceptronic                = "2L (Conceptronic)"
CNet                        = "CNet Technology Inc."

Ralink.DeviceDesc           = "Ralink RT2500 Wireless LAN Card"

ASUS.DeviceDesc             = "ASUS 802.11b/g Wireless LAN Card"
ASUSGEN.DeviceDesc          = "802.11b/g Wireless LAN Card"

DELTA.DeviceDesc            = "802.11 g Wireless LAN PC Card"

QCOM_PCMCIA.DeviceDesc      = "802.11b/g Wireless PC Card"
QCOM_PCI.DeviceDesc         = "802.11b/g Wireless Adapter"

M2500_6833.DeviceDesc       = "802.11g MiniPCI Wireless Network Adapter"
M2500_6834.DeviceDesc       = "802.11g PCI Wireless Network Adapter"
M2500_6835.DeviceDesc       = "802.11g CardBus Wireless Network Adapter"

ZINWELLPCI.DeviceDesc       = "802.11g WLAN PCI Adapter"
ZINWELLMPCI.DeviceDesc      = "802.11g WLAN mini-PCI Adapter"
ZINWELLCARD.DeviceDesc      = "802.11g WLAN CardBus Adapter"
ZINWELLOEM1.DeviceDesc      = "AT&T Plug&Share 54 Mbps Wireless PCI Adapter"
ZINWELLOEM2.DeviceDesc      = "AT&T Plug&Share 54 Mbps Wireless Cardbus Adapter"

WLANm.DeviceDesc            = "WLAN 802.11g miniPCI module"
WLANc.DeviceDesc            = "WLAN 802.11g Cardbus module"

AMIT.DeviceDesc             = "AMIT 802.11 g Wireless LAN PC Card"
AMITMINI.DeviceDesc         = "AMIT MINI 802.11 g Wireless LAN PC Card"
AMITPCI.DeviceDesc          = "AMIT PCI 802.11 g Wireless LAN PC Card"

CASTLENET.DeviceDesc        = "CastleNet WP1280 802.11 g Wireless LAN Card"

WN4306A.DeviceDesc          = "802.11g 54Mbps Wireless PC Card SE"

Edimax7108.DeviceDesc       = "Edimax EW-7108 Series 802.11g Wireless LAN PC Card"
Edimax7128.DeviceDesc       = "Edimax EW-7128 Series 802.11g Wireless LAN PCI Card"
Hawking0C54.DeviceDesc      = "Hawking HWC54GR Hi-Speed Wireless-G CardBus Card"
Hawking0B54.DeviceDesc      = "Hawking HWP54GR Hi-Speed Wireless-G PCI Card"

AMIGO.DeviceDesc1           = "Wireless PC Card"
AMIGO.DeviceDesc2           = "Wireless miniPCI Adapter"
AMIGO.DeviceDesc3           = "Wireless PCI Adapter"

SurecomCardbus.DeviceDesc   = "802.11 g Wireless LAN PC CardBus"
SurecomPCI.DeviceDesc       = "802.11 g Wireless LAN PCI"
SurecomMPCI.DeviceDesc      = "802.11 g Wireless LAN MPCI"

CNetCardbus.DeviceDesc      = "802.11g Wireless LAN CardBus"
CNetPCI.DeviceDesc          = "802.11g Wireless LAN PCI"
CNetMPCI.DeviceDesc         = "802.11g Wireless LAN Mini-PCI"

GigabyteWMKG.DeviceDesc     = "Gigabyte WMKG Cardbus WLAN Card"
GigabyteWIKG.DeviceDesc     = "Gigabyte WIKG mini PCI WLAN Card"
GigabyteWPKG.DeviceDesc     = "Gigabyte WPKG PCI WLAN Card"

BILLIONTON_B.DeviceDesc     = "Billionton 802.11 b/g Wireless LAN Card"
BILLIONTON_N.DeviceDesc     = "802.11 b/g Wireless LAN Card"

Conceptronic_PCCard.DeviceDesc = "Conceptronic 54g Wireless PC-Card"
Conceptronic_PCICard.DeviceDesc = "Conceptronic 54g Wireless PCI Card"

VTechPCI.DeviceDesc         = "VTech Wireless 802.11g PCI Adapter"
VTechCARD.DeviceDesc        = "VTech Wireless 802.11g PCMCIA Adapter"

Sitecom_WL112.DeviceDesc    = "Sitecom Wireless Network PC Card 54G WL-112"
Sitecom_WL115.DeviceDesc    = "Sitecom Wireless Network PCI Adapter 54G WL-115"

Siemens.DeviceDesc           = "Siemens 802.11g PC Card Wireless Network Adapter"

CNetGPCI.DeviceDesc         = "CNet Wireless-G PCI Adapter"
CNetGMPCI.DeviceDesc        = "CNet Wireless-G miniPCI Adapter"
CNetGCB.DeviceDesc          = "CNet Wireless-G Cardbus Adapter"

INSTALL_DISK_STR            = "RT2500 Wireless LAN Installation Disk"

RALINK.Service.DispName     = "RT2500 Wireless Driver"
ASUS.Service.DispName       = "AsusTek RT2500 Wireless Driver"
DELTA.Service.DispName      = "Delta Networks RT2500 Wireless Driver"
ZINWELL.Service.DispName    = "ZINWELL RT2500 Wireless Driver"
AMIT.Service.DispName       = "AMIT RT2500 Wireless Driver"
CASTLENET.Service.DispName  = "CastleNet RT2500 Wireless Driver"
WN4306A.Service.DispName    = "RT2500 802.11g 54Mbps Wireless PC Card SE Driver"
EDIMAX.Service.DispName     = "Edimax RT2500 Wireless Driver"
HAWKING.Service.DispName    = "Hawking RT2500 Wireless Driver"
Surecom.Service.DispName    = "Surecom RT2500 Wireless Driver"
Gigabyte.Service.DispName   = "Gigabyte RT2500 Wireless Driver"
BILLIONTON.Service.DispName = "Billionton RT2500 Wireless Driver"
VTECH.Service.DispName      = "VTech RT2500 802.11g Wireless Driver"
SITECOM.Service.DispName    = "Sitecom RT2500 Wireless Network Driver"
SIEMENS.Service.DispName    = "Siemens RT2500 Wireless 802.11b/g Driver(RT2500)"
CONCEPTRONIC.Service.DispName = "Conceptronic RT2500 54g Wireless Driver"
CNET.Service.DispName       = "CNET RT2500 Wireless Driver"

; Don't put spaces around=sign otherwise installer will not be able to
; find these lines.
SSID_DEF_STR                = ""
VENDOR_DESC_DEF_STR         = "IEEE 802.11g Wireless Card."
NETWORK_TYPE_DEF_STR        = "1"
CHANNEL                     = "1"

