;***********************************************************************
; NetWG111.INF
;
;   This installation script supports Windows 2000, XP for the
;   Wireless LAN Adapters.
;
;   Copyright (c) 2004 Netgear Inc.
;   All Rights Reserved.
;
;***********************************************************************

[Version]
 DriverVer		= 06/04/2004, 3.0.18.201
 Signature		= "$Chicago$"
 Compatible		= 1
 Class			= Net
 ClassGUID		= {4d36e972-e325-11ce-bfc1-08002be10318}
 Provider		= %DRV_PROVIDER_STR%
 CatalogFile.NT	= 	netwg111.cat

[ControlFlags]
;Exclude all PNP adapters from user selection
 ExcludeFromSelect   = *

[Manufacturer]
 %MANUFACTURER_STR% = DeviceList

[DeviceList]
 %WLAN_USB_DESC_STR%     = WLAN_USB1,        USB\VID_0846&PID_4220
 %WLAN_USB_DESC_STR%     = WLAN_USB2,        USB\VID_0846&PID_4240

;==========
[WLAN_USB1.NT]    ; Win2k
 AddReg         = WLAN_USB1_REG, COMMON_USB_REG_NT, COMMON_NDIS_REG_NT, COMMON_REG
 CopyFiles      = WLAN_USB_DRIVER_COPY_NT
 BusType        = 15	;USB
 Characteristics= 0x84

[WLAN_USB1.NT.Services]
 AddService= "wg111nd5", 2, WLAN_DRIVER_USB_SERVICE, WLAN_USB_DRIVER_EVENTLOG

[WLAN_USB1_REG]
 HKR,Ndi,DeviceID,0,"USB\VID_0846&PID_4220"
 HKR,,PlatformID,0,14480
 HKR,,UsbVariant,0,8832
 HKR,,VendorDesc,0,%WLAN_USB_DESC_STR%
 
;==========
[WLAN_USB2.NT]    ; Win2k
 AddReg         = WLAN_USB2_REG, COMMON_USB_REG_NT, COMMON_NDIS_REG_NT, COMMON_REG
 CopyFiles      = WLAN_USB_DRIVER_COPY_NT
 BusType        = 15	;USB
 Characteristics= 0x84

[WLAN_USB2.NT.Services]
 AddService= "wg111nd5", 2, WLAN_DRIVER_USB_SERVICE, WLAN_USB_DRIVER_EVENTLOG

[WLAN_USB2_REG]
 HKR,Ndi,DeviceID,0,"USB\VID_0846&PID_4240"
 HKR,,PlatformID,0,14480
 HKR,,UsbVariant,0,14471
 HKR,,VendorDesc,0,%WLAN_USB_DESC_STR%

;###############################################################################
[WLAN_DRIVER_USB_SERVICE]
 DisplayName    = %WLAN_USB_SERVICE_STR%
 ServiceType    = 1    ; SERVICE_KERNEL_DRIVER
 StartType      = 3    ; SERVICE_DEMAND_START
 ErrorControl   = 1    ; NORMAL
 ServiceBinary  = %12%\wg111nd5.sys
 LoadOrderGroup = NDIS

[WLAN_USB_DRIVER_EVENTLOG]
 AddReg         = WLAN_USB_DRIVER_EVENTLOG_REG

[WLAN_USB_DRIVER_EVENTLOG_REG]
 HKR,           ,EventMessageFile       ,0x00020000     ,"%%SystemRoot%%\System32\netevent.dll"
 HKR,           ,TypesSupported         ,0x00010001     ,7

;############################################################################### 
[COMMON_USB_REG_NT]
 HKR,NDI                ,Service                ,0      ,"wg111nd5"
 HKR,NDI                ,CardType               ,0      ,"USB"
 HKR,                   ,BusType                ,0      ,"0"
 HKR,                   ,DeviceVxDs             ,0      ,"wg111nd5.sys" 

[COMMON_NDIS_REG_NT]
 HKR,NDI\Interfaces     ,UpperRange             ,0      ,"ndis5"
 HKR,NDI\Interfaces     ,LowerRange             ,0      ,"ethernet"

[COMMON_REG]
 HKR,		 ,WLANIOC,0,"XG-300"
   
 HKR,		,RTSThresh,0,2346
 HKR,defaults	,RTSThresh,0,2346
 HKR,		,FragThresh,0,2346
 HKR,defaults	,FragThresh,0,2346
 HKR,		,ConfigProfile,0,256
 HKR,defaults	,ConfigProfile,0,256
 HKR,		,NitroMode,0,1
 HKR,defaults	,NitroMode,0,1
 HKR,		,PSMode,0,1
 HKR,defaults	,PSMode,0,1
 HKR,		,SSID,0,"ANY"
 HKR,defaults	,SSID,0,"ANY"		;Default value is "any"
 HKR,		,NetworkType,0,1
 HKR,defaults	,NetworkType,0,1	;Infrasturcture
 HKR,		,NitroTime,0,1400
 HKR,defaults	,NitroTime,0,1400
 HKR,		,ProfileName,0,"Default"
 HKR,		,11dMode,0,0

 HKR,		,ShortRetryLimit,0,7
 HKR,defaults	,ShortRetryLimit,0,7
 HKR,NDI\params\ShortRetryLimit,default,0,7
 HKR,NDI\params\ShortRetryLimit,ParamDesc,,%SHORT_RETRY_STR%
 HKR,NDI\params\ShortRetryLimit,type,,int
 HKR,NDI\params\ShortRetryLimit,min,0,1
 HKR,NDI\params\ShortRetryLimit,max,0,255
 HKR,NDI\params\ShortRetryLimit,step,0,1

 HKR,		,LongRetryLimit,0,4
 HKR,defaults	,LongRetryLimit,0,4
 HKR,NDI\params\LongRetryLimit,default,0,4
 HKR,NDI\params\LongRetryLimit,ParamDesc,,%LONG_RETRY_STR%
 HKR,NDI\params\LongRetryLimit,type,0,int
 HKR,NDI\params\LongRetryLimit,min,0,1
 HKR,NDI\params\LongRetryLimit,max,0,255
 HKR,NDI\params\LongRetryLimit,step,0,1
 
 ;Country Desc
 HKR,		,CountryCode,0,US
 HKR,defaults	,CountryCode,0,US
 HKR,Ndi\params\CountryCode,default,0,US
 HKR,NDI\params\CountryCode,ParamDesc,,%REGULATOR_DOMAIN%
 HKR,NDI\params\CountryCode,type,,enum
 HKR,NDI\params\CountryCode,flag,1,30,00,00,00
 HKR,NDI\params\CountryCode\enum,US,,%REGULATOR_DOMAIN_US%
 HKR,NDI\params\CountryCode\enum,AT,,%REGULATOR_DOMAIN_AF%
 HKR,NDI\params\CountryCode\enum,BE,,%REGULATOR_DOMAIN_AS%
 HKR,NDI\params\CountryCode\enum,DK,,%REGULATOR_DOMAIN_AU%
 HKR,NDI\params\CountryCode\enum,TW,,%REGULATOR_DOMAIN_CA%
 HKR,NDI\params\CountryCode\enum,GB,,%REGULATOR_DOMAIN_EU%
 HKR,NDI\params\CountryCode\enum,FI,,%REGULATOR_DOMAIN_FR%
 HKR,NDI\params\CountryCode\enum,DE,,%REGULATOR_DOMAIN_JA%
 HKR,NDI\params\CountryCode\enum,GR,,%REGULATOR_DOMAIN_ME%
 HKR,NDI\params\CountryCode\enum,IE,,%REGULATOR_DOMAIN_SA%

;###############################################################################
[DestinationDirs]
;CopyFiles Section      = Destination Directory ID -- see layout.inf
;-----------------        ------------------------
 WLAN_USB_DRIVER_COPY_NT   = 12 ; Win2k=%windir%\system32\drivers

[WLAN_USB_DRIVER_COPY_NT]
 wg111nd5.sys

[SourceDisksNames]
;Source Disk ID         = Disk Name
;--------------           ---------
 1                      = %INSTALL_DISK_STR%,,,

[SourceDisksFiles.X86]  ; Win2k/Xp
 wg111nd5.sys		= 1

;###############################################################################
[Strings]
;String ID			= String Text
;---------			-----------
 DRV_PROVIDER_STR		= "NETGEAR, Inc."
 MANUFACTURER_STR		= "NETGEAR, Inc."
 
 WLAN_USB_SERVICE_STR		= "NETGEAR WG111 802.11g Wireless USB Adapter Driver"
 
 INSTALL_DISK_STR        	= "NETGEAR WG111 Wireless LAN Install Disk"
 WLAN_USB_DESC_STR		= "NETGEAR WG111 802.11g Wireless USB2.0 Adapter"

 SHORT_RETRY_STR         	= "Short Retry Limit"
 LONG_RETRY_STR          	= "Long Retry Limit"
 REGULATOR_DOMAIN		= "Regulator Domain"
 REGULATOR_DOMAIN_US		= "United States"
 REGULATOR_DOMAIN_AF		= "Africa"
 REGULATOR_DOMAIN_AS		= "Asia"
 REGULATOR_DOMAIN_AU		= "Australia"
 REGULATOR_DOMAIN_CA		= "Canada"
 REGULATOR_DOMAIN_EU		= "Europe"
 REGULATOR_DOMAIN_FR		= "France"
 REGULATOR_DOMAIN_JA		= "Japan"
 REGULATOR_DOMAIN_ME		= "Mexico"
 REGULATOR_DOMAIN_SA		= "South America"
 
 