;
;
; Copyright (c) 2007 - 2009
;


[Version]
signature="$CHICAGO$"
LayoutFile=Layout.inf
CatalogFile.NT=cam3820.cat
Class=Image
ClassGUID={6bdd1fc6-810f-11d0-bec7-08002be2092f}
Provider=%Generic%
DriverVer=07/13/2010,6.2.6.2

[SourceDisksNames]
1=%SourceDiskName%,,,


[SourceDisksFiles]
cam3820a.sys = 1
ACamPropertyPage.dll = 1
cocam3820.dll = 1
;cam3820n.ax = 1


[ControlFlags]
; All PnP devices should be excluded from manual AddDevice Applet list
ExcludeFromSelect=*

[Manufacturer]
%GenericMfg%=CamVendor, NTx86.5.1, NTx86.6.0, NTamd64, NTia64

[DestinationDirs]
DefaultDestDir=10, system32  ;%windir%\system32
UvcCam.Files.Ext = 10, system32\drivers ;%windir%\system32\drivers
Plugin.Files = 10, system32; %windir%\system32
Plugin.Files.64 = 10,SysWow64
cocam3820CopyFileSection = 11


[CamVendor]
%USB\VID_058F&PID_3820.DeviceDesc%=UvcCam,USB\VID_058F&PID_3820,USB\VID_058F&PID_3820\FriendlyName
%USB\VID_058F&PID_3820.DeviceDesc%=UvcCam,USB\VID_058F&PID_3821,USB\VID_058F&PID_3821\FriendlyName
%USB\VID_058F&PID_3820.DeviceDesc%=UvcCam,USB\VID_058F&PID_3822,USB\VID_058F&PID_3822\FriendlyName
%USB\VID_058F&PID_3820.DeviceDesc%=UvcCam,USB\VID_058F&PID_3823,USB\VID_058F&PID_3823\FriendlyName
%USB\VID_058F&PID_3820.DeviceDesc%=UvcCam,USB\VID_058F&PID_3824,USB\VID_058F&PID_3824\FriendlyName
%USB\VID_058F&PID_3820.DeviceDesc%=UvcCam,USB\VID_058F&PID_3825,USB\VID_058F&PID_3825\FriendlyName
%USB\VID_058F&PID_3820.DeviceDesc%=UvcCam,USB\VID_058F&PID_3830,USB\VID_058F&PID_3830\FriendlyName
%USB\VID_058F&PID_3820.DeviceDesc%=UvcCam,USB\VID_058F&PID_3831,USB\VID_058F&PID_3831\FriendlyName
%MCNEX_1.DeviceDesc%=UvcCam,USB\VID_1210&PID_25F4,USB\VID_1210&PID_25F4\FriendlyName
%MCNEX_2.DeviceDesc%=UvcCam,USB\VID_1210&PID_25F5,USB\VID_1210&PID_25F5\FriendlyName
%MCNEX_3.DeviceDesc%=UvcCam,USB\VID_1210&PID_2604,USB\VID_1210&PID_2604\FriendlyName
%MCNEX_4.DeviceDesc%=UvcCam,USB\VID_1210&PID_2614,USB\VID_1210&PID_2614\FriendlyName


[CamVendor.NTx86.5.1]
%USB\VID_058F&PID_3820.DeviceDesc%=UvcCam.XP,USB\VID_058F&PID_3820,USB\VID_058F&PID_3820\FriendlyName
%USB\VID_058F&PID_3820.DeviceDesc%=UvcCam.XP,USB\VID_058F&PID_3821,USB\VID_058F&PID_3821\FriendlyName
%USB\VID_058F&PID_3820.DeviceDesc%=UvcCam.XP,USB\VID_058F&PID_3822,USB\VID_058F&PID_3822\FriendlyName
%USB\VID_058F&PID_3820.DeviceDesc%=UvcCam.XP,USB\VID_058F&PID_3823,USB\VID_058F&PID_3823\FriendlyName
%USB\VID_058F&PID_3820.DeviceDesc%=UvcCam.XP,USB\VID_058F&PID_3824,USB\VID_058F&PID_3824\FriendlyName
%USB\VID_058F&PID_3820.DeviceDesc%=UvcCam.XP,USB\VID_058F&PID_3825,USB\VID_058F&PID_3825\FriendlyName
%USB\VID_058F&PID_3820.DeviceDesc%=UvcCam.XP,USB\VID_058F&PID_3830,USB\VID_058F&PID_3830\FriendlyName
%USB\VID_058F&PID_3820.DeviceDesc%=UvcCam.XP,USB\VID_058F&PID_3831,USB\VID_058F&PID_3831\FriendlyName
%MCNEX_1.DeviceDesc%=UvcCam.XP,USB\VID_1210&PID_25F4,USB\VID_1210&PID_25F4\FriendlyName
%MCNEX_2.DeviceDesc%=UvcCam.XP,USB\VID_1210&PID_25F5,USB\VID_1210&PID_25F5\FriendlyName
%MCNEX_3.DeviceDesc%=UvcCam.XP,USB\VID_1210&PID_2604,USB\VID_1210&PID_2604\FriendlyName
%MCNEX_4.DeviceDesc%=UvcCam.XP,USB\VID_1210&PID_2614,USB\VID_1210&PID_2614\FriendlyName

[CamVendor.NTx86.6.0]
%USB\VID_058F&PID_3820.DeviceDesc%=UvcCam.v32,USB\VID_058F&PID_3820&MI_00,USB\VID_058F&PID_3820\FriendlyName
%USB\VID_058F&PID_3820.DeviceDesc%=UvcCam.v32,USB\VID_058F&PID_3821&MI_00,USB\VID_058F&PID_3821\FriendlyName
%USB\VID_058F&PID_3820.DeviceDesc%=UvcCam.v32,USB\VID_058F&PID_3822&MI_00,USB\VID_058F&PID_3822\FriendlyName
%USB\VID_058F&PID_3820.DeviceDesc%=UvcCam.v32,USB\VID_058F&PID_3823&MI_00,USB\VID_058F&PID_3823\FriendlyName
%USB\VID_058F&PID_3820.DeviceDesc%=UvcCam.v32,USB\VID_058F&PID_3824&MI_00,USB\VID_058F&PID_3824\FriendlyName
%USB\VID_058F&PID_3820.DeviceDesc%=UvcCam.v32,USB\VID_058F&PID_3825&MI_00,USB\VID_058F&PID_3825\FriendlyName
%USB\VID_058F&PID_3820.DeviceDesc%=UvcCam.v32,USB\VID_058F&PID_3830&MI_00,USB\VID_058F&PID_3830\FriendlyName
%USB\VID_058F&PID_3820.DeviceDesc%=UvcCam.v32,USB\VID_058F&PID_3831&MI_00,USB\VID_058F&PID_3831\FriendlyName
%MCNEX_1.DeviceDesc%=UvcCam.v32,USB\VID_1210&PID_25F4&MI_00,USB\VID_1210&PID_25F4\FriendlyName
%MCNEX_2.DeviceDesc%=UvcCam.v32,USB\VID_1210&PID_25F5&MI_00,USB\VID_1210&PID_25F5\FriendlyName
%MCNEX_3.DeviceDesc%=UvcCam.v32,USB\VID_1210&PID_2604&MI_00,USB\VID_1210&PID_2604\FriendlyName
%MCNEX_4.DeviceDesc%=UvcCam.v32,USB\VID_1210&PID_2614&MI_00,USB\VID_1210&PID_2614\FriendlyName

[CamVendor.NTamd64]
%USB\VID_058F&PID_3820.DeviceDesc%=UvcCam.w64,USB\VID_058F&PID_3820&MI_00,USB\VID_058F&PID_3820\FriendlyName
%USB\VID_058F&PID_3820.DeviceDesc%=UvcCam.w64,USB\VID_058F&PID_3821&MI_00,USB\VID_058F&PID_3821\FriendlyName
%USB\VID_058F&PID_3820.DeviceDesc%=UvcCam.w64,USB\VID_058F&PID_3822&MI_00,USB\VID_058F&PID_3822\FriendlyName
%USB\VID_058F&PID_3820.DeviceDesc%=UvcCam.w64,USB\VID_058F&PID_3823&MI_00,USB\VID_058F&PID_3823\FriendlyName
%USB\VID_058F&PID_3820.DeviceDesc%=UvcCam.w64,USB\VID_058F&PID_3824&MI_00,USB\VID_058F&PID_3824\FriendlyName
%USB\VID_058F&PID_3820.DeviceDesc%=UvcCam.w64,USB\VID_058F&PID_3825&MI_00,USB\VID_058F&PID_3825\FriendlyName
%USB\VID_058F&PID_3820.DeviceDesc%=UvcCam.w64,USB\VID_058F&PID_3830&MI_00,USB\VID_058F&PID_3830\FriendlyName
%USB\VID_058F&PID_3820.DeviceDesc%=UvcCam.w64,USB\VID_058F&PID_3831&MI_00,USB\VID_058F&PID_3831\FriendlyName
%MCNEX_1.DeviceDesc%=UvcCam.w64,USB\VID_1210&PID_25F4&MI_00,USB\VID_1210&PID_25F4\FriendlyName
%MCNEX_2.DeviceDesc%=UvcCam.w64,USB\VID_1210&PID_25F5&MI_00,USB\VID_1210&PID_25F5\FriendlyName
%MCNEX_3.DeviceDesc%=UvcCam.w64,USB\VID_1210&PID_2604&MI_00,USB\VID_1210&PID_2604\FriendlyName
%MCNEX_4.DeviceDesc%=UvcCam.w64,USB\VID_1210&PID_2614&MI_00,USB\VID_1210&PID_2614\FriendlyName

[CamVendor.NTia64]
%USB\VID_058F&PID_3820.DeviceDesc%=UvcCam.w64,USB\VID_058F&PID_3820&MI_00,USB\VID_058F&PID_3820\FriendlyName
%USB\VID_058F&PID_3820.DeviceDesc%=UvcCam.w64,USB\VID_058F&PID_3821&MI_00,USB\VID_058F&PID_3821\FriendlyName
%USB\VID_058F&PID_3820.DeviceDesc%=UvcCam.w64,USB\VID_058F&PID_3822&MI_00,USB\VID_058F&PID_3822\FriendlyName
%USB\VID_058F&PID_3820.DeviceDesc%=UvcCam.w64,USB\VID_058F&PID_3823&MI_00,USB\VID_058F&PID_3823\FriendlyName
%USB\VID_058F&PID_3820.DeviceDesc%=UvcCam.w64,USB\VID_058F&PID_3824&MI_00,USB\VID_058F&PID_3824\FriendlyName
%USB\VID_058F&PID_3820.DeviceDesc%=UvcCam.w64,USB\VID_058F&PID_3825&MI_00,USB\VID_058F&PID_3825\FriendlyName
%USB\VID_058F&PID_3820.DeviceDesc%=UvcCam.w64,USB\VID_058F&PID_3830&MI_00,USB\VID_058F&PID_3830\FriendlyName
%USB\VID_058F&PID_3820.DeviceDesc%=UvcCam.w64,USB\VID_058F&PID_3831&MI_00,USB\VID_058F&PID_3831\FriendlyName
%MCNEX_1.DeviceDesc%=UvcCam.w64,USB\VID_1210&PID_25F4&MI_00,USB\VID_1210&PID_25F4\FriendlyName
%MCNEX_2.DeviceDesc%=UvcCam.w64,USB\VID_1210&PID_25F5&MI_00,USB\VID_1210&PID_25F5\FriendlyName
%MCNEX_3.DeviceDesc%=UvcCam.w64,USB\VID_1210&PID_2604&MI_00,USB\VID_1210&PID_2604\FriendlyName
%MCNEX_4.DeviceDesc%=UvcCam.w64,USB\VID_1210&PID_2614&MI_00,USB\VID_1210&PID_2614\FriendlyName

[UvcCam]
Include=    ks.inf, kscaptur.inf
Needs=      KS.Registration,KSCAPTUR.Registration
AddReg=     UvcCam.AddReg,UvcCam.DefaultSettings.Addreg
CopyFiles=  UvcCam.Files.Ext,Plugin.Files
;for ACamPropertyPage
RegisterDlls = UvcCamRegSvr
; STI
SubClass=StillImage

; Device type: 1=scanner, 2=camera
DeviceType=2

; Vendor supplied value
DeviceSubType=0x01

; Capabilities is a mask:
; 0x01 = Device generates events
; 0x02 = Polling needed
; 0x04 = Generate event when device installed
; 0x08 = Enable the "auto" port option
Capabilities=0x01

DeviceData=UvcCam.DeviceData
ICMProfiles="sRGB Color Space Profile.icm"

[UvcCam.NT]
Include=    ks.inf, kscaptur.inf, dshowext.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT,DSHOWEXT.Registration
AddReg=     UvcCam.AddReg,UvcCam.DefaultSettings.Addreg
CopyFiles=  UvcCam.Files.Ext,Plugin.Files
;for ACamPropertyPage
RegisterDlls = UvcCamRegSvr
;STI
SubClass=StillImage
DeviceType=2
DeviceSubType=0x01
Capabilities=0x01
DeviceData=UvcCam.DeviceData
ICMProfiles="sRGB Color Space Profile.icm"

[UvcCam.XP]
Include=    ks.inf, kscaptur.inf, dshowext.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT,DSHOWEXT.Registration
AddReg=     UvcCamXP.AddReg,UvcCam.DefaultSettings.Addreg
CopyFiles=  UvcCam.Files.Ext,Plugin.Files
;for ACamPropertyPage
RegisterDlls = UvcCamRegSvr

;WIA
SubClass=StillImage
; Device type: 1=scanner, 2=camera, 3=video
DeviceType=3

; Vendor supplied value
DeviceSubType=0x1

; Capabilities is a mask:
; 0x01 = Device generates events
; 0x02 = Polling needed
; 0x04 = Generate event when device installed
; 0x08 = Enable the "auto" port option
; 0x10 = WIA capable driver
; 0x20 = Driver has reduced functionality
Capabilities=0x00000031
DeviceData=UvcCam.DeviceData
ICMProfiles="sRGB Color Space Profile.icm"

[UvcCam.v32]
Include=    ks.inf, kscaptur.inf, dshowext.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT,DSHOWEXT.Registration
AddReg=     UvcCam.AddReg,UvcCam.DefaultSettings.Addreg
CopyFiles=  UvcCam.Files.Ext,Plugin.Files

;WIA
SubClass=StillImage
; Device type: 1=scanner, 2=camera, 3=video
DeviceType=3

; Vendor supplied value
DeviceSubType=0x1

; Capabilities is a mask:
; 0x01 = Device generates events
; 0x02 = Polling needed
; 0x04 = Generate event when device installed
; 0x08 = Enable the "auto" port option
; 0x10 = WIA capable driver
; 0x20 = Driver has reduced functionality
Capabilities=0x00000031
DeviceData=UvcCam.DeviceData
ICMProfiles="sRGB Color Space Profile.icm"

[UvcCam.w64]
Include=    ks.inf, kscaptur.inf, dshowext.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT,DSHOWEXT.Registration
AddReg=     UvcCam.AddReg,UvcCam.DefaultSettings.Addreg
CopyFiles=  UvcCam.Files.Ext,Plugin.Files.64

;WIA
SubClass=StillImage
; Device type: 1=scanner, 2=camera, 3=video
DeviceType=3

; Vendor supplied value
DeviceSubType=0x1

; Capabilities is a mask:
; 0x01 = Device generates events
; 0x02 = Polling needed
; 0x04 = Generate event when device installed
; 0x08 = Enable the "auto" port option
; 0x10 = WIA capable driver
; 0x20 = Driver has reduced functionality
Capabilities=0x00000031
DeviceData=UvcCam.DeviceData
ICMProfiles="sRGB Color Space Profile.icm"

[UvcCam.AddReg]
HKR,,DevLoader,,*ntkern
HKR,,NTMPDriver,,cam3820a.sys
HKR,,OkToHibernate,3,01
HKR,,DontSuspendIfStreamsAreRunning,3,01
HKR,,PageOutWhenUnopened,3,00
HKR,,PowerDownWhenUnopened,3,01

; WIA
HKR,,HardwareConfig,1,1
HKR,,USDClass,,"{0527d1d0-88c2-11d2-82c7-00c04f8ec183}"

[UvcCamXP.AddReg]
HKR,,DevLoader,,*ntkern
HKR,,NTMPDriver,,cam3820a.sys
HKR,,OkToHibernate,3,01
HKR,,DontSuspendIfStreamsAreRunning,3,01
HKR,,PageOutWhenUnopened,3,00
HKR,,PowerDownWhenUnopened,3,00

; WIA
HKR,,HardwareConfig,1,1
HKR,,USDClass,,"{0527d1d0-88c2-11d2-82c7-00c04f8ec183}"


[UvcCam.DeviceData]
Server=local
UI DLL=sti.dll
UI Class ID={5d8ef5a3-ac13-11d2-a093-00c04f72dc3c}

[UvcCam.Interfaces]
AddInterface=%KSCATEGORY_CAPTURE%,GLOBAL,UvcCam.Interface
AddInterface=%KSCATEGORY_VIDEO%,GLOBAL,UvcCam.Interface

[UvcCam.NT.Interfaces]
AddInterface=%KSCATEGORY_CAPTURE%,GLOBAL,UvcCam.Interface
AddInterface=%KSCATEGORY_VIDEO%,GLOBAL,UvcCam.Interface

[UvcCam.XP.Interfaces]
AddInterface=%KSCATEGORY_CAPTURE%,GLOBAL,UvcCam.XP.Interface
AddInterface=%KSCATEGORY_VIDEO%,GLOBAL,UvcCam.XP.Interface

[UvcCam.v32.Interfaces]
;AddInterface=%KSCATEGORY_CAPTURE%,GLOBAL,UvcCam.XP.Interface
;AddInterface=%KSCATEGORY_VIDEO%,GLOBAL,UvcCam.XP.Interface

[UvcCam.w64.Interfaces]
;AddInterface=%KSCATEGORY_CAPTURE%,GLOBAL,UvcCam.w64.Interface
;AddInterface=%KSCATEGORY_VIDEO%,GLOBAL,UvcCam.w64.Interface

[UvcCam.Interface]
AddReg=UvcCam.Intf.AddReg

[UvcCam.Intf.AddReg]
HKR,,CLSID,,%ProxyVCap.CLSID%

; Custom PropertySet and propertypage
;HKR,PageAliases,"{71F96464-78F3-11d0-A18C-00A0C9118956}",1,f6, f2, 44, 12, 55, 35, b7, 49, 0x87, 0xc3, 0xc5, 0xe6, 0xdf, 0x1a, 0x3c, 0xbc
HKR,PageAliases,"{71F96464-78F3-11d0-A18C-00A0C9118956}",1,4B,30,B5,E1,A0,22,1B,43,B9,E0,5D,7D,71,DE,DA,06
;HKR,PinFactory\1\Interfaces\%InterfaceGUID%,,,
;HKCR,CLSID\%InterfaceGUID%\InProcServer32,,,cam3820n.ax
;HKCR,CLSID\%InterfaceGUID%\InProcServer32,"ThreadingModel",,"Both"
;HKCR,CLSID\%PropertyPageGUID%\InProcServer32,,,cam3820n.ax
;HKCR,CLSID\%PropertyPageGUID%\InProcServer32,"ThreadingModel",,"Both"
;HKLM,System\CurrentControlSet\Control\MediaInterfaces\%InterfaceGUID%,,,"Cam3820 Property Set Handler"
;HKLM,System\CurrentControlSet\Control\MediaSets\%InterfaceGUID%\PropertyPages\%PropertyPageGUID%,,,"Cam3820 Property Page"

;Property Page Alcor UVC DEVICE
HKLM,SYSTEM\CurrentControlSet\Control\MediaSets\{68BBD0B0-61A4-4B83-90B7-A6215F3C4F70}
HKLM,SYSTEM\CurrentControlSet\Control\MediaSets\{68BBD0B0-61A4-4B83-90B7-A6215F3C4F70}\PropertyPages
HKLM,SYSTEM\CurrentControlSet\Control\MediaSets\{68BBD0B0-61A4-4B83-90B7-A6215F3C4F70}\PropertyPages\{E1B5304B-22A0-431B-B9E0-5D7D71DEDA06}


[UvcCam.XP.Interface]
AddReg=UvcCam.XP.Intf.AddReg

[UvcCam.XP.Intf.AddReg]
HKR,,CLSID,,%ProxyVCap.CLSID%

; Custom PropertySet and propertypage
;HKR,PageAliases,"{71F96464-78F3-11d0-A18C-00A0C9118956}",1,f6, f2, 44, 12, 55, 35, b7, 49, 0x87, 0xc3, 0xc5, 0xe6, 0xdf, 0x1a, 0x3c, 0xbc
HKR,PageAliases,"{71F96464-78F3-11d0-A18C-00A0C9118956}",1,4B,30,B5,E1,A0,22,1B,43,B9,E0,5D,7D,71,DE,DA,06
;HKR,PinFactory\1\Interfaces\%InterfaceGUID%,,,
;HKCR,CLSID\%InterfaceGUID%\InProcServer32,,,cam3820n.ax
;HKCR,CLSID\%InterfaceGUID%\InProcServer32,"ThreadingModel",,"Both"
;HKCR,CLSID\%PropertyPageGUID%\InProcServer32,,,cam3820n.ax
;HKCR,CLSID\%PropertyPageGUID%\InProcServer32,"ThreadingModel",,"Both"
;HKLM,System\CurrentControlSet\Control\MediaInterfaces\%InterfaceGUID%,,,"Cam3820 Property Set Handler"
;HKLM,System\CurrentControlSet\Control\MediaSets\%InterfaceGUID%\PropertyPages\%PropertyPageGUID%,,,"Cam3820 Property Page"

;Property Page Alcor UVC DEVICE
HKLM,SYSTEM\CurrentControlSet\Control\MediaSets\{68BBD0B0-61A4-4B83-90B7-A6215F3C4F70}
HKLM,SYSTEM\CurrentControlSet\Control\MediaSets\{68BBD0B0-61A4-4B83-90B7-A6215F3C4F70}\PropertyPages
HKLM,SYSTEM\CurrentControlSet\Control\MediaSets\{68BBD0B0-61A4-4B83-90B7-A6215F3C4F70}\PropertyPages\{E1B5304B-22A0-431B-B9E0-5D7D71DEDA06}

[UvcCam.w64.Interface]
AddReg=UvcCam.w64.Intf.AddReg

[UvcCam.w64.Intf.AddReg]
HKR,,CLSID,,%ProxyVCap.CLSID%

; Custom PropertySet and propertypage
;HKR,PageAliases,"{71F96464-78F3-11d0-A18C-00A0C9118956}",1,f6, f2, 44, 12, 55, 35, b7, 49, 0x87, 0xc3, 0xc5, 0xe6, 0xdf, 0x1a, 0x3c, 0xbc
;HKR,PageAliases,"{71F96464-78F3-11d0-A18C-00A0C9118956}",1,4B,30,B5,E1,A0,22,1B,43,B9,E0,5D,7D,71,DE,DA,06
;HKR,PinFactory\1\Interfaces\%InterfaceGUID%,,,
;HKCR,CLSID\%InterfaceGUID%\InProcServer32,,,cam3820n.ax
;HKCR,CLSID\%InterfaceGUID%\InProcServer32,"ThreadingModel",,"Both"
;HKCR,CLSID\%PropertyPageGUID%\InProcServer32,,,cam3820n.ax
;HKCR,CLSID\%PropertyPageGUID%\InProcServer32,"ThreadingModel",,"Both"
;HKCR,Wow6432Node\CLSID\%InterfaceGUID%\InProcServer32,,,cam3820n.ax
;HKCR,Wow6432Node\CLSID\%InterfaceGUID%\InProcServer32,"ThreadingModel",,"Both"
;HKCR,Wow6432Node\CLSID\%PropertyPageGUID%\InProcServer32,,,cam3820n.ax
;HKCR,Wow6432Node\CLSID\%PropertyPageGUID%\InProcServer32,"ThreadingModel",,"Both"
;HKLM,System\CurrentControlSet\Control\MediaInterfaces\%InterfaceGUID%,,,"Cam3820 Property Set Handler"
;HKLM,System\CurrentControlSet\Control\MediaSets\%InterfaceGUID%\PropertyPages\%PropertyPageGUID%,,,"Cam3820 Property Page"

;Property Page Alcor UVC DEVICE
HKLM,SYSTEM\CurrentControlSet\Control\MediaSets\{68BBD0B0-61A4-4B83-90B7-A6215F3C4F70}
HKLM,SYSTEM\CurrentControlSet\Control\MediaSets\{68BBD0B0-61A4-4B83-90B7-A6215F3C4F70}\PropertyPages
HKLM,SYSTEM\CurrentControlSet\Control\MediaSets\{68BBD0B0-61A4-4B83-90B7-A6215F3C4F70}\PropertyPages\{E1B5304B-22A0-431B-B9E0-5D7D71DEDA06}


[UvcCam.DefaultSettings.Addreg]
; Default Setting
HKR,DefaultSetting,BORDERENABLE,0x00010001,0
HKR,DefaultSetting,EFFECTENABLE,0x00010001,0
HKR,DefaultSetting,PUNCH,0x00010001,0
HKR,DefaultSetting,MOSAIC,0x00010001,0
HKR,DefaultSetting,WHIRL,0x00010001,0
HKR,DefaultSetting,EMBOSS,0x00010001,0
HKR,DefaultSetting,NEGTIVE,0x00010001,0
HKR,DefaultSetting,BW,0x00010001,0
HKR,DefaultSetting,SKETCH,0x00010001,0
HKR,DefaultSetting,CYLINDER,0x00010001,0
HKR,DefaultSetting,POSTER,0x00010001,0
HKR,DefaultSetting,SOLOARIZE,0x00010001,0
HKR,DefaultSetting,MOTION,0x00010001,0
HKR,DefaultSetting,BorderPath,0x00000000,"NOFILE"
;
;HKR,DefaultSetting,SCALE13,0x00010001,3
;HKR,DefaultSetting,SCALE5M,0x00010001,3
;HKR,DefaultSetting,SCALE4M,0x00010001,3
;HKR,DefaultSetting,SCALE3M,0x00010001,3
;HKR,DefaultSetting,SCALE2M,0x00010001,3
;HKR,DefaultSetting,SCALEQVGA2VGA,0x00010001,3
HKR,DefaultSetting,JPGCODEC,0x00010001,1
HKR,DefaultSetting,SELSUSPEND,0x00010001,1
HKR,DefaultSetting,FMTSEL,0x00010001,7
HKR,DefaultSetting,EFFECTYUV,0x00010001,1
;HKR,DefaultSetting,STREAM_CUSTOMIZE,0x00010001,0
;HKR,DefaultSetting,ZoomOffset,0x00010001,0
;HKR,DefaultSetting,ZoomScale,0x00010001,100



; CamNotify
HKR,CamNotify,Capture,0x00010001,0


[UvcCam.NT.Services]
AddService = Cam3820,0x00000002,UvcCam.ServiceInstall

[UvcCam.XP.Services]
AddService = Cam3820,0x00000002,UvcCam.ServiceInstall

[UvcCam.v32.Services]
AddService = Cam3820,0x00000002,UvcCam.ServiceInstall

[UvcCam.w64.Services]
AddService = Cam3820,0x00000002,UvcCam.ServiceInstall

[UvcCam.ServiceInstall]
DisplayName   = %SERVICE_DISPLAY_NAME%
ServiceType   = %SERVICE_KERNEL_DRIVER%
StartType     = %SERVICE_DEMAND_START%
ErrorControl  = %SERVICE_ERROR_NORMAL%
ServiceBinary = %10%\System32\Drivers\cam3820a.sys

[UvcCam.NT.CoInstallers]
CopyFiles = cocam3820CopyFileSection
AddReg = CoInstall.AddReg

[UvcCam.XP.CoInstallers]
CopyFiles = cocam3820CopyFileSection
AddReg = CoInstall.AddReg


[UvcCam.v32.CoInstallers]
CopyFiles = cocam3820CopyFileSection
AddReg = CoInstall.AddReg

[UvcCam.w64.CoInstallers]
CopyFiles = cocam3820CopyFileSection
AddReg = CoInstall.AddReg


[CoInstall.AddReg]
HKR,,CoInstallers32,0x10000,"cocam3820.dll,Cam3820CoInstaller"

[cocam3820CopyFileSection]
cocam3820.dll

[UvcCam.Files.Ext]
cam3820a.sys

[Plugin.Files]
ACamPropertyPage.dll
;cam3820n.ax

[Plugin.Files.64]
ACamPropertyPage.dll
;cam3820n.ax

[UvcCamRegSvr]
11,,ACamPropertyPage.dll, 1

[Strings]

;----------------
; Non-Localizable
;----------------
ProxyVCap.CLSID="{17CCA71B-ECD7-11D0-B908-00A0C9223196}"
KSCATEGORY_CAPTURE="{65E8773D-8F56-11D0-A3B9-00A0C9223196}"
KSCATEGORY_VIDEO="{6994AD05-93EF-11D0-A3CC-00A0C9223196}"

;custom PropertySet and PropertyPage
InterfaceGUID="{68BBD0B0-61A4-4b83-90B7-A6215F3C4F70}"
PropertyPageGUID="{E1B5304B-22A0-431B-B9E0-5D7D71DEDA06}"

SERVICE_DISPLAY_NAME = "Cam3820 PC Camera Driver"
SERVICE_KERNEL_DRIVER=1

; PnP should use demand start
SERVICE_DEMAND_START=3
SERVICE_ERROR_NORMAL=1


;----------------
; Localizable
;----------------
Generic="MCNEX"
GenericMfg="MCNEX"

USB\VID_058F&PID_3820.DeviceDesc="UVC Video Camera"
MCNEX_1.DeviceDesc="WebCam SCB-0350M"
MCNEX_2.DeviceDesc="MCNEX_1.3M_WebCam"
MCNEX_3.DeviceDesc="WebCam SCB-0380M"
MCNEX_4.DeviceDesc="WebCam SCB-1300M"

;USB Camera Friendly Name = "WebCam SCB-0350M"
SourceDiskName="Installation diskette 1"
