; Copyright (c) 2000-2002 Linksys Group Inc., All Rights Reserved 
;
; Windows XP
;
; Installation file (.inf) for the Linksys Group Inc. device.
;

[Version]
  	Signature	= "$Chicago$"
    	Compatible	= 1
    	Provider	= %Linksys%
    	ClassGuid 	= {4d36e972-e325-11ce-bfc1-08002be10318} 
    	Class		= Net
     	CatalogFile	= net83820.cat
    	DriverVer	= 05/15/2002,5.0.2.50

[ControlFlags]
    	ExcludeFromSelect = PCI\VEN_100B&DEV_0022&SUBSYS_10641737

;
; Driver information
;

[Manufacturer]
    	%Linksys% 	= Linksys.Mfg

;
;Model section
;

[Linksys.Mfg]
    	%LinksysEG103264.DeviceDesc% = EG103264.Copper, PCI\VEN_100B&DEV_0022&SUBSYS_10641737 ; Linksys EG103264


;
; General installation section
;

[EG103264.Copper]	
    	Characteristics = 0x84    ; NCF_PHYSICAL | NCF_HAS_UI
    	BusType	    	= 5
    	AddReg          = EG103264.NT.ndi, EG103264.Params.Common, EG103264.Params.Copper
    	CopyFiles       = EG103264.NT.CopyFiles

[EG103264.Copper.NT]	
    	Characteristics = 0x84    ; NCF_PHYSICAL | NCF_HAS_UI
    	BusType	    	= 5
    	AddReg          = EG103264.NT.ndi, EG103264.Params.Common, EG103264.Params.Copper
    	CopyFiles       = EG103264.NT.CopyFiles

[EG103264.Copper.NT.Services]
	AddService = EG103264, 2, EG103264.AddService, EG103264.AddEventLog

[EG103264.AddService]
	DisplayName	= %EG103264.SvcDesc%
	ServiceType    	= 1                 ; SERVICE_KERNEL_DRIVER
	StartType      	= 3                 ; SERVICE_DEMAND_START
	ErrorControl   	= 1                 ; SERVICE_ERROR_NORMAL
	LoadOrderGroup 	= NDIS
	ServiceBinary  	= %12%\EG103264.sys

[EG103264.AddEventLog]
	AddReg 		= EG103264.EventLog.reg

[EG103264.EventLog.reg]
	HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll;%%SystemRoot%%\System32\drivers\EG103264.sys"
	HKR, , TypesSupported,   0x00010001, 7

[EG103264.NT.ndi]
	HKR, Ndi\Interfaces, UpperRange, , "ndis5"
	HKR, Ndi\Interfaces, LowerRange, , "ethernet"
	HKR, Ndi,            Service,   0, "EG103264"

[EG103264.NT.CopyFiles]
    	EG103264.sys,,,0x00000004

[EG103264.Params.common]
    	HKR, ,SlotNumber,        	0, 	"-1"
    	HKR, ,BusNumber,           	0, 	"-1"
    	HKR, ,MediaType,           	0, 	"1"
    	HKR, ,AdapterCFID,         	0, 	"0022100b"

	;
	; For advanced configuration through
	; the registry only.
	;
    	HKR, ,RxDMA,	  		0,	"512"
    	HKR, ,TxDMA,	  		0,	"1024"
    	HKR, ,RxIntrHold, 	   	0,	"0"
    	HKR, ,TxIntrHold, 	   	0,	"0"
    	HKR, ,TxDrth, 			0,	"0"
    	HKR, ,TxFlth, 			0,	"1"
    	HKR, ,RxDrth, 			0,	"0"
    	HKR, ,PsSLo,            	0,  	"4"	
    	HKR, ,PsSHi,            	0,  	"8"	
    	HKR, ,PsDLo,            	0,  	"4"	
    	HKR, ,PsDHi,            	0,  	"8"	
    	HKR, ,PauseCounterVal,  	0,  	"65535"	
    	HKR, ,MultipleVlan,     	0,  	"0"	

    	;
    	;  Recieve Buffers
    	;
    	HKR, Ndi\params\RxQueueSz,          ParamDesc, 0, %RxQueueSz%
    	HKR, Ndi\params\RxQueueSz,          type,      0, "long"
    	HKR, Ndi\params\RxQueueSz,          default,   0, "106"
    	HKR, Ndi\params\RxQueueSz,          Min,       0, "32"
    	HKR, Ndi\params\RxQueueSz,          Max,       0, "2048"
    	HKR, Ndi\params\RxQueueSz,          Step,      0, "1"
    	;
    	;  Transmit Buffers
    	;
    	HKR, Ndi\params\TxQueueSz,          ParamDesc, 0, %TxQueueSz%
    	HKR, Ndi\params\TxQueueSz,          type,      0, "long"
    	HKR, Ndi\params\TxQueueSz,          default,   0, "2048"
    	HKR, Ndi\params\TxQueueSz,          Min,       0, "64"
    	HKR, Ndi\params\TxQueueSz,          Max,       0, "4096"
    	HKR, Ndi\params\TxQueueSz,          Step,      0, "1"
    	;
	; Jumbo Packet Size
    	; 
    	HKR, Ndi\params\JumboFrame, 	 ParamDesc,    0, %JumboFrame%
    	HKR, Ndi\params\JumboFrame,      type,         0, "enum"
    	HKR, Ndi\params\JumboFrame,      default,      0, "1514" 
    	HKR, Ndi\params\JumboFrame\enum, 1514,         0, "1) 1514 (Standard)"
    	HKR, Ndi\params\JumboFrame\enum, 4088,         0, "2) 4088"
    	HKR, Ndi\params\JumboFrame\enum, 9014,         0, "3) 9014 (Alteon)"
    	HKR, Ndi\params\JumboFrame\enum, 10000,        0, "4) 10000"
    	HKR, Ndi\params\JumboFrame\enum, 16128,        0, "5) 16128"
    	;
    	;Network address
    	; 
    	HKR, Ndi\params\NetworkAddress,	ParamDesc,      0, %NetworkAddress%
    	HKR, Ndi\params\NetworkAddress, type,           0, "edit"
    	HKR, Ndi\params\NetworkAddress, LimitText,      0, "12"
    	HKR, Ndi\params\NetworkAddress, UpperCase,      0, "1"
    	HKR, Ndi\params\NetworkAddress, default,        0, ""
    	HKR, Ndi\params\NetworkAddress, optional,       0, "1"
   	;
    	; Checksum 
    	;
    	HKR, Ndi\params\CheckSum,     	ParamDesc, 0, %CheckSum%
    	HKR, Ndi\params\CheckSum,       type,      0, "enum"
    	HKR, Ndi\params\CheckSum,       default,   0, "2"
    	HKR, Ndi\params\CheckSum\enum,  0,         0, "1) Tx Checksum"
    	HKR, Ndi\params\CheckSum\enum,  1,         0, "2) Rx CheckSum"
	HKR, Ndi\params\CheckSum\enum,  2,         0, "3) All CheckSum"
	HKR, Ndi\params\CheckSum\enum,  3,         0, "4) None"
    	;
    	;  Virtual Lan ID
    	;
    	HKR, Ndi\params\VLANID,     	ParamDesc, 0, %VLANID%
    	HKR, Ndi\params\VLANID,         type,      0, "long"
    	HKR, Ndi\params\VLANID,         default,   0, ""
    	HKR, Ndi\params\VLANID,         Min,       0, "1"
    	HKR, Ndi\params\VLANID,         Max,       0, "4095"
    	HKR, Ndi\params\VLANID,         Step,      0, "1"
    	HKR, Ndi\params\VLANID,     	optional,  0, "1"
    	;
    	; Priority Queues
    	;
    	HKR, Ndi\params\PriQ,          	ParamDesc, 0, %PriQ%
    	HKR, Ndi\params\PriQ,          	type,      0, "enum"
    	HKR, Ndi\params\PriQ,          	default,   0, "0"
    	HKR, Ndi\params\PriQ\enum,     	1,         0, "Enable"
    	HKR, Ndi\params\PriQ\enum,     	0,         0, "Disable"


[EG103264.Params.Copper]
	;
	; Network Media Selection 
	;
	HKR, Ndi\params\NetworkMedia,      ParamDesc, 0, %NetworkMedia%
	HKR, Ndi\params\NetworkMedia,      type,      0, "enum"
	HKR, Ndi\params\NetworkMedia,      default,   0, "8"
	HKR, Ndi\params\NetworkMedia\enum, 8,         0, "1) Auto Negotiate"
	HKR, Ndi\params\NetworkMedia\enum, 1,         0, "2) Auto 1000 Mbps"
	HKR, Ndi\params\NetworkMedia\enum, 2,         0, "3) Auto 100 Mbps"
	HKR, Ndi\params\NetworkMedia\enum, 3,         0, "4) Auto 10 Mbps"
	HKR, Ndi\params\NetworkMedia\enum, 4,         0, "5) Force 100 Full"
	HKR, Ndi\params\NetworkMedia\enum, 5,         0, "6) Force 100 Half"
	HKR, Ndi\params\NetworkMedia\enum, 6,         0, "7) Force 10 Full"
	HKR, Ndi\params\NetworkMedia\enum, 7,         0, "8) Force 10 Half"
	;
	; IEEE Non Compliance Bit 
	;
	HKR, Ndi\params\NcBit,      	ParamDesc, 0, %NcBit%
	HKR, Ndi\params\NcBit,      	type,      0, "enum"
	HKR, Ndi\params\NcBit,      	default,   0, "1"
	HKR, Ndi\params\NcBit\enum, 	1,         0, "Enable"
	HKR, Ndi\params\NcBit\enum, 	0,         0, "Disable"
	;
	; Pause Control
	;
	HKR, Ndi\params\FlowControl,      ParamDesc, 0, %PauseControl%
	HKR, Ndi\params\FlowControl,      type,      0, "enum"
	HKR, Ndi\params\FlowControl,      default,   0, "3"
	HKR, Ndi\params\FlowControl\enum, 0,         0, "Disable"
	HKR, Ndi\params\FlowControl\enum, 1,         0, "Tx pause frames"
	HKR, Ndi\params\FlowControl\enum, 3,         0, "Enable"    


;
; Source file information
;

[SourceDisksNames.x86]
    	1 = %DiskId1%,,,""

;
; Files for Installation Disk #1 (Net)
;

[SourceDisksFiles]
    	EG103264.sys 		= 1,,

[DestinationDirs]
   	EG103264.NT.CopyFiles 	= 12
   	DefaultDestDir 		= 11

;
; Localizable Strings
;

[Strings]
	Linksys                    	= "Linksys Group Inc."
	LinksysEG103264.DeviceDesc 	= "Linksys EG1032/EG1064 Instant Gigabit Network Adapter"
    	EG103264.SvcDesc		= "Linksys EG1032/EG1064 Instant Gigabit Ethernet"
    	DiskId1 			= "Linksys Group Inc. Driver Disk"

;
; Advanced property setting 
;
    	NetworkMedia    = "Media Type"
    	PauseControl    = "Pause Control"
    	RxQueueSz       = "Receive Buffers"
    	TxQueueSz       = "Transmit Buffers"
    	JumboFrame      = "Packet Size (maximum)"
    	NcBit      	= "IEEE Compliant Link"
    	NetworkAddress  = "Address"
    	CheckSum	= "Offload Checksum"
    	VLANID		= "VLAN ID"
    	PriQ      	= "Priority Queues"
