; Sierra Wireless Virtual Serial Port using Serial MUX driver Setup File (Win2K/XP)
; Copyright (c) 2008 Sierra Wireless All Rights Reserved.

[Version]
signature="$WINDOWS NT$"
Class=Ports
ClassGuid={4D36E978-E325-11CE-BFC1-08002BE10318}
Provider=%COMPANY%
DriverVer=08/13/2009,1.0.0.5
CatalogFile=swsspser.cat

[Manufacturer]
%COMPANY%=Models, NT.5.1, NTamd64

[Models]
%DEVICENAME4% = Device, SWI_VSP_SER_DEVICE4 ;

[Models.NT.5.1]
%DEVICENAME4% = Device.NT.5.1, SWI_VSP_SER_DEVICE4 ;

[Models.NTamd64]
%DEVICENAME4% = Device.NTamd64, SWI_VSP_SER_DEVICE4 ; 

[Device]
CopyFiles=Device.CopyFiles

[Device.Services]
AddService = swvspser,0x00000002,Device.AddService

[Device.NT.5.1]
CopyFiles=Device.NT.5.1.CopyFiles

[Device.NT.5.1.Services]
AddService = swvspser,0x00000002,Device.AddService

[Device.NTamd64]
CopyFiles=Device.NTamd64.CopyFiles

[Device.NTamd64.Services]
AddService = swvspser,0x00000002,Device.AddService

[Device.AddService]
DisplayName   = %SERVICENAME%
ServiceType   = 1
StartType     = 3
ErrorControl  = 0
ServiceBinary = %12%\swvspser.sys 
AddReg=SWDRIVER.AddRegistry

[SWDRIVER.AddRegistry]
HKR, Parameters, ProductType, 0x00010001, 0x1

[SourceDisksNames]
1 = %DISKID%,,,""

[SourceDisksFiles]
swvspser.sys  = 1,,
swvspser64.sys  = 1,,

[DestinationDirs]
Device.CopyFiles=12
DefaultDestDir=12

[Device.CopyFiles]
swvspser.sys, swvspser.sys

[Device.NT.5.1.CopyFiles]
swvspser.sys, swvspser.sys

[Device.NTamd64.CopyFiles]
swvspser.sys, swvspser64.sys

[Strings]
COMPANY = "Sierra Wireless Inc."
DEVICENAME4 = "Sierra Wireless Application Interface NMEA"
DISKID="Sierra Wireless VSP using Serial MUX Driver Installation Disk"
SERVICENAME="Sierra VSP using Ethernet"
