;
; Copyright Ericsson AB
;

[version]
Signature   = "$Windows NT$"
Class       = Net
ClassGUID   = {4d36e972-e325-11ce-bfc1-08002be10318}
Provider    = %EAB%
CatalogFile = WwanUsbMp.cat
DriverVer=12/09/2009,1.0.0.65

[Manufacturer]
%Ericsson% = Ericsson, NTamd64, NTx86

[ControlFlags]
ExcludeFromSelect = *

[Ericsson.NTx86]
; DisplayName                     Section          DeviceID
; -----------                     -------          --------
;Devgiri Brands
%Ericsson.Dg_DeviceDesc_WWAN%		= ericssondg.ndi,  USB\VID_0BDB&PID_1902&Mi_07&wwan ; Generic DG
%Dell.Dg_DeviceDesc_WWAN%			= ericssondg.ndi,  USB\VID_413C&PID_8147&Mi_07&wwan ; Dell DG
%Lenovo.Dg_DeviceDesc_WWAN%			= ericssondg.ndi,  USB\VID_0BDB&PID_1900&Mi_07&wwan ; Lenovo DG
%Toshiba.Dg_DeviceDesc_WWAN%		= ericssondg.ndi,  USB\VID_0930&PID_130B&Mi_07&wwan ; Toshiba DG

;Sagarmartha Brands 850 MHz
%Ericsson.Sm_DeviceDesc_WWAN%		= ericsson.ndi,  USB\VID_0BDB&PID_1904&Mi_06&wwan ; Generic
%Dell.Sm_DeviceDesc_WWAN%			= ericsson.ndi,  USB\VID_413C&PID_8183&Mi_06&wwan ; Dell
%Lenovo.Sm_DeviceDesc_WWAN%			= ericsson.ndi,  USB\VID_0BDB&PID_1905&Mi_06&wwan ; Lenovo
%Toshiba.Sm_DeviceDesc_WWAN%		= ericsson.ndi,  USB\VID_0930&PID_130C&Mi_06&wwan ; Toshiba
%Hp.BV_DeviceDesc_WWAN%				= ericsson.ndi,  USB\VID_03F0&PID_261D&Mi_06&wwan ; HP

;Sagarmartha Brands 900 MHz
%Ericsson.Sm_DeviceDesc_WWAN%		= ericsson.ndi,  USB\VID_0BDB&PID_1906&Mi_06&wwan ; Generic
%Dell.Sm_DeviceDesc_WWAN%			= ericsson.ndi,  USB\VID_413C&PID_8184&Mi_06&wwan ; Dell
%Lenovo.Sm_DeviceDesc_WWAN%			= ericsson.ndi,  USB\VID_0BDB&PID_1907&Mi_06&wwan ; Lenovo
%Toshiba.Sm_DeviceDesc_WWAN%		= ericsson.ndi,  USB\VID_0930&PID_1311&Mi_06&wwan ; Toshiba
%Hp.BVIII_DeviceDesc_WWAN%			= ericsson.ndi,  USB\VID_03F0&PID_271D&Mi_06&wwan ; HP

;Pollux Brands 850 MHz
%Ericsson.Pl_DeviceDesc_WWAN%		= ericsson.ndi,  USB\VID_0BDB&PID_1909&Mi_06&wwan ; Generic

;Pollux Brands 900 MHz
%Ericsson.Pl_DeviceDesc_WWAN%		= ericsson.ndi,  USB\VID_0BDB&PID_190A&Mi_06&wwan ; Generic

[Ericsson.NTamd64]
; DisplayName                     Section          DeviceID
; -----------                     -------          --------
;Devgiri Brands
%Ericsson.Dg_DeviceDesc_WWAN%		= ericssondg.ndi,  USB\VID_0BDB&PID_1902&Mi_07&wwan ; Generic
%Dell.Dg_DeviceDesc_WWAN%			= ericssondg.ndi,  USB\VID_413C&PID_8147&Mi_07&wwan ; Dell
%Lenovo.Dg_DeviceDesc_WWAN%			= ericssondg.ndi,  USB\VID_0BDB&PID_1900&Mi_07&wwan ; Lenovo
%Toshiba.Dg_DeviceDesc_WWAN%		= ericssondg.ndi,  USB\VID_0930&PID_130B&Mi_07&wwan ; Toshiba

;Sagarmartha Brands 850 MHz
%Ericsson.Sm_DeviceDesc_WWAN%		= ericsson.ndi,  USB\VID_0BDB&PID_1904&Mi_06&wwan ; Generic
%Dell.Sm_DeviceDesc_WWAN%			= ericsson.ndi,  USB\VID_413C&PID_8183&Mi_06&wwan ; Dell
%Lenovo.Sm_DeviceDesc_WWAN%			= ericsson.ndi,  USB\VID_0BDB&PID_1905&Mi_06&wwan ; Lenovo
%Toshiba.Sm_DeviceDesc_WWAN%		= ericsson.ndi,  USB\VID_0930&PID_130C&Mi_06&wwan ; Toshiba
%Hp.BV_DeviceDesc_WWAN%				= ericsson.ndi,  USB\VID_03F0&PID_261D&Mi_06&wwan ; HP

;Sagarmartha Brands 900 MHz
%Ericsson.Sm_DeviceDesc_WWAN%		= ericsson.ndi,  USB\VID_0BDB&PID_1906&Mi_06&wwan ; Generic
%Dell.Sm_DeviceDesc_WWAN%			= ericsson.ndi,  USB\VID_413C&PID_8184&Mi_06&wwan ; Dell
%Lenovo.Sm_DeviceDesc_WWAN%			= ericsson.ndi,  USB\VID_0BDB&PID_1907&Mi_06&wwan ; Lenovo
%Toshiba.Sm_DeviceDesc_WWAN%		= ericsson.ndi,  USB\VID_0930&PID_1311&Mi_06&wwan ; Toshiba
%Hp.BVIII_DeviceDesc_WWAN%			= ericsson.ndi,  USB\VID_03F0&PID_271D&Mi_06&wwan ; HP

;Pollux Brands 850 MHz
%Ericsson.Pl_DeviceDesc_WWAN%		= ericsson.ndi,  USB\VID_0BDB&PID_1909&Mi_06&wwan ; Generic

;Pollux Brands 900 MHz
%Ericsson.Pl_DeviceDesc_WWAN%		= ericsson.ndi,  USB\VID_0BDB&PID_190A&Mi_06&wwan ; Generic

;
;x86
;
[ericsson.ndi.NTx86]
Characteristics    = 0x84
BusType            = 15
AddReg             = ericsson.reg
CopyFiles          = ericsson.CopyFiles

;
;WWan NDIS >= 6.2 
;
*IfType            = 243        ; IF_TYPE_WWANPP GSM
*MediaType         = 9          ; NdisMediumWirelessWan 
*PhysicalMediaType = 8          ; NdisPhysicalMediumWirelessWan 
EnableDhcp         = 0          ; Disable DHCP 

;
;amd64
;
[ericsson.ndi.NTAMD64]
Characteristics    = 0x84
BusType            = 15
AddReg             = ericsson.reg
CopyFiles          = ericsson64.CopyFiles

;
;WWan NDIS >= 6.2 
;
*IfType            = 243        ; IF_TYPE_WWANPP GSM
*MediaType         = 9          ; NdisMediumWirelessWan 
*PhysicalMediaType = 8          ; NdisPhysicalMediumWirelessWan 
EnableDhcp         = 0          ; Disable DHCP 

;
;x86
;
[ericsson.ndi.NTx86.Services]
AddService = WwanUsbServ, 2, ericsson.Service, ericsson.EventLog

;
;amd64
;
[ericsson.ndi.NTAMD64.Services]
AddService = WwanUsbServ, 2, ericsson64.Service, ericsson.EventLog

;
;[HKEY_LOCAL_MACHINE\SYSTEM\ControlSet001\Control\Class\{4D36E972-E325-11CE-BFC1-08002BE10318}\0013]
;
[ericsson.reg]
HKR, Ndi,                         Service,    0, "WwanUsbServ"

;
;NDIS >= 6.2
;
HKR, Ndi\Interfaces,              UpperRange, 0, "flpp4, flpp6"
HKR, Ndi\Interfaces,              LowerRange, 0, "ppip"

;
;goes into [HKEY_LOCAL_MACHINE\SYSTEM\CurrentControlSet\Control\Class\{4D36E972-E325-11CE-BFC1-08002BE10318}\0013]
;HKR, Ndi\Interfaces,              LowerRange, 0, "wlan,ethernet"
;HKR, Ndi\params,  EmulateNdis62, 0x00010001, 1			;enable WWan NDIS 6.2
;
;HKR, Ndi\params,  DefGwMac, 0, "02-80-37-EC-02-81"
;HKR, Ndi\params,  ModuleMac,0, "02-80-37-EC-02-00"
;HKR, Ndi\params,  HardwareRadioSwitch, 0, 2			;1 = Can the radio be disabled trough a switch, 2 = set switch on at load
;HKR, Ndi\params,  SoftwareRadioSwitch, 0, 1			;1 = set switch on at load
;HKR, Ndi\params,  SoftwareRadioSim, 0, 1			;1 = set switch on at load
;HKR, Ndi\params,  EmulateNdis62,    0, 1			;enable WWan NDIS 6.2 on a eth frame module
;HKR, Ndi\params,  GlobalDebugLevel, 0, 7			;the drive log level 1 = low, DBG_ERROR = 7
;HKR, Ndi\params,  ProviderID, 0, ""				
;HKR, Ndi\params,  ManualNetworkSelection, 0, 0
;HKR, Ndi\params,  WwanDataClass, 0x10001, 1
;HKR, Ndi\params,  IsF3507g, 0x10001, 0
;HKR, Ndi\params,  ProvisionedAccessString, 0, ""
;HKR, Ndi\params,  ProvisionedUserName, 0, ""
;HKR, Ndi\params,  ProvisionedPassword, 0, ""
;HKR, Ndi\params,  ProvisionedProviderId, 0, ""
;HKR, Ndi\params,  ContextId, 0x10001, 0
;HKR, Ndi\params,  ContextType, 0x10001, 0
;HKR, Ndi\params,  ProvisionedCompression, 0x10001, 0
;HKR, Ndi\params,  ProvisionedAuthType, 0x10001, 0


HKR, Params,  DefGwMac, 0, "02-80-37-EC-02-81"
HKR, Params,  ModuleMac,0, "02-80-37-EC-02-00"
HKR, Params,  HardwareRadioSwitch, 0, 2			;1 = Can the radio be disabled trough a switch, 2 = set switch on at load
HKR, Params,  SoftwareRadioSwitch, 0, 1			;1 = set switch on at load
HKR, Params,  SoftwareRadioSim, 0, 1			;1 = set switch on at load
HKR, Params,  EmulateNdis62,    0, 1			;enable WWan NDIS 6.2 on a eth frame module
HKR, Params,  GlobalDebugLevel, 0, 7			;the drive log level 1 = low, DBG_ERROR = 7
HKR, Params,  ProviderID, 0, ""				
HKR, Params,  ManualNetworkSelection, 0, 0
HKR, Params,  WwanDataClass, 0x10001, 1
HKR, Params,  IsF3507g, 0x10001, 0
HKR, Params,  ProvisionedAccessString, 0, ""
HKR, Params,  ProvisionedUserName, 0, ""
HKR, Params,  ProvisionedPassword, 0, ""
HKR, Params,  ProvisionedProviderId, 0, ""
HKR, Params,  ContextId, 0x10001, 0
HKR, Params,  ContextType, 0x10001, 0
HKR, Params,  ProvisionedCompression, 0x10001, 0
HKR, Params,  ProvisionedAuthType, 0x10001, 0
HKR, Params,  RadioAccessCFUN, 0x10001, 1


;
;[HKEY_LOCAL_MACHINE\SYSTEM\ControlSet001\Control\Class\{4D36E972-E325-11CE-BFC1-08002BE10318}\0007\Ndi\Params\*ReceiveBuffers]
;
HKR, Ndi\params\*ReceiveBuffers,  ParamDesc,  0, "%ReceiveBuffers%"
HKR, Ndi\params\*ReceiveBuffers,  default,    0, "64"

;
;[HKEY_LOCAL_MACHINE\SYSTEM\ControlSet001\Control\Class\{4D36E972-E325-11CE-BFC1-08002BE10318}\0007\Ndi\Params\*TransmitBuffers]
;
HKR, Ndi\params\*TransmitBuffers, ParamDesc,  0, "%TransmitBuffers%"
HKR, Ndi\params\*TransmitBuffers, default,    0, "15"

;
;	
;
[ericsson.Service]
DisplayName     = %Ericsson.Service.DispName%
ServiceType     = 1             ;SERVICE_KERNEL_DRIVER
StartType       = 3             ;SERVICE_DEMAND_START
ErrorControl    = 1             ;SERVICE_ERROR_NORMAL
ServiceBinary   = %12%\WwanUsbMp.sys
LoadOrderGroup  = NDIS

[ericsson64.Service]
DisplayName     = %Ericsson.Service.DispName%
ServiceType     = 1             ;SERVICE_KERNEL_DRIVER
StartType       = 3             ;SERVICE_DEMAND_START
ErrorControl    = 1             ;SERVICE_ERROR_NORMAL
ServiceBinary   = %12%\WwanUsbMp64.sys
LoadOrderGroup  = NDIS


[ericsson.EventLog]
AddReg = ericsson.AddEventLog.reg

[ericsson.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll"
HKR, , TypesSupported,   0x00010001, 7

[ericsson.CopyFiles]
WwanUsbMp.sys,,,2

[ericsson64.CopyFiles]
WwanUsbMp64.sys,,,2

[SourceDisksNames.x86]
1 = %DiskDescription%,WwanUsbMp.sys,,\i386

[SourceDisksNames.amd64]
1 = %DiskDescription%,WwanUsbMp64.sys,,\amd64


[SourceDisksFiles.x86]
WwanUsbMp.sys = 1,,
WdfCoInstaller01009.dll = 1

[SourceDisksFiles.amd64]
WwanUsbMp64.sys = 1,,
WdfCoInstaller01009.dll = 1

[DestinationDirs]
ericsson.CopyFiles         = 12
ericsson64.CopyFiles         = 12
;DefaultDestDirs            = 11


;-------------- WDF Coinstaller installation

[DestinationDirs]
;CoInstaller_CopyFiles = 11

[ericsson.ndi.NTx86.CoInstallers]
AddReg    = CoInstaller_AddReg
CopyFiles = CoInstaller_CopyFiles

[ericsson.ndi.NTAMD64.CoInstallers]
AddReg    = CoInstaller_AddReg
CopyFiles = CoInstaller_CopyFiles
;
;	wdfcoinstaller01009
;
[CoInstaller_CopyFiles]
wdfcoinstaller01009.dll

[SourceDisksFiles]
wdfcoinstaller01009.dll=1 ; make sure the number matches with SourceDisksNames

[CoInstaller_AddReg]
;HKR,,CoInstallers32,0x00010000, "wdfcoinstaller$KMDFCOINSTALLERVERSION$.dll,WdfCoInstaller"

[ericsson.ndi.NTx86.Wdf]
KmdfService = WwanUsbServ, ericsson_wdfsect

[ericsson.ndi.NTAMD64.Wdf]
KmdfService = WwanUsbServ, ericsson_wdfsect

[ericsson_wdfsect]
KmdfLibraryVersion = 1.9


;%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
; This is for supporting Devgiri
;%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
;
;x86
;
[ericssondg.ndi.NTx86]
Characteristics    = 0x84
BusType            = 15
AddReg             = ericssondg.reg
CopyFiles          = ericssondg.CopyFiles

;
;WWan NDIS >= 6.2 
;
*IfType            = 243        ; IF_TYPE_WWANPP GSM
*MediaType         = 9          ; NdisMediumWirelessWan 
*PhysicalMediaType = 8          ; NdisPhysicalMediumWirelessWan 
EnableDhcp         = 0          ; Disable DHCP 

;
;amd64
;
[ericssondg.ndi.NTAMD64]
Characteristics    = 0x84
BusType            = 15
AddReg             = ericssondg.reg
CopyFiles          = ericssondg64.CopyFiles

;
;WWan NDIS >= 6.2 
;
*IfType            = 243        ; IF_TYPE_WWANPP GSM
*MediaType         = 9          ; NdisMediumWirelessWan 
*PhysicalMediaType = 8          ; NdisPhysicalMediumWirelessWan 
EnableDhcp         = 0          ; Disable DHCP 

;
;x86
;
[ericssondg.ndi.NTx86.Services]
AddService = WwanUsbServ, 2, ericssondg.Service, ericssondg.EventLog

;
;amd64
;
[ericssondg.ndi.NTAMD64.Services]
AddService = WwanUsbServ, 2, ericssondg64.Service, ericssondg.EventLog

;
;[HKEY_LOCAL_MACHINE\SYSTEM\ControlSet001\Control\Class\{4D36E972-E325-11CE-BFC1-08002BE10318}\0013]
;
[ericssondg.reg]
HKR, Ndi,                         Service,    0, "WwanUsbServ"

;
;NDIS >= 6.2
;
HKR, Ndi\Interfaces,              UpperRange, 0, "flpp4, flpp6"
HKR, Ndi\Interfaces,              LowerRange, 0, "ppip"

;
;goes into [HKEY_LOCAL_MACHINE\SYSTEM\CurrentControlSet\Control\Class\{4D36E972-E325-11CE-BFC1-08002BE10318}\0013]
;HKR, Ndi\Interfaces,              LowerRange, 0, "wlan,ethernet"
;HKR, Ndi\params,  EmulateNdis62, 0x00010001, 1			;enable WWan NDIS 6.2
;
;HKR, Ndi\params,  DefGwMac, 0, "02-80-37-EC-02-81"
;HKR, Ndi\params,  ModuleMac,0, "02-80-37-EC-02-00"
;HKR, Ndi\params,  HardwareRadioSwitch, 0, 2			;1 = Can the radio be disabled trough a switch, 2 = set switch on at load
;HKR, Ndi\params,  SoftwareRadioSwitch, 0, 1			;1 = set switch on at load
;HKR, Ndi\params,  SoftwareRadioSim, 0, 1			;1 = set switch on at load
;HKR, Ndi\params,  EmulateNdis62,    0, 1			;enable WWan NDIS 6.2 on a eth frame module
;HKR, Ndi\params,  GlobalDebugLevel, 0, 7			;the drive log level 1 = low, DBG_ERROR = 7
;HKR, Ndi\params,  ProviderID, 0, ""				
;HKR, Ndi\params,  ManualNetworkSelection, 0, 0
;HKR, Ndi\params,  WwanDataClass, 0x10001, 1
;HKR, Ndi\params,  IsF3507g, 0x10001, 1
;HKR, Ndi\params,  ProvisionedAccessString, 0, ""
;HKR, Ndi\params,  ProvisionedUserName, 0, ""
;HKR, Ndi\params,  ProvisionedPassword, 0, ""
;HKR, Ndi\params,  ProvisionedProviderId, 0, ""
;HKR, Ndi\params,  ContextId, 0x10001, 0
;HKR, Ndi\params,  ContextType, 0x10001, 0
;HKR, Ndi\params,  ProvisionedCompression, 0x10001, 0
;HKR, Ndi\params,  ProvisionedAuthType, 0x10001, 0


HKR, Params,  DefGwMac, 0, "02-80-37-EC-02-81"
HKR, Params,  ModuleMac,0, "02-80-37-EC-02-00"
HKR, Params,  HardwareRadioSwitch, 0, 2			;1 = Can the radio be disabled trough a switch, 2 = set switch on at load
HKR, Params,  SoftwareRadioSwitch, 0, 1			;1 = set switch on at load
HKR, Params,  SoftwareRadioSim, 0, 1			;1 = set switch on at load
HKR, Params,  EmulateNdis62,    0, 1			;enable WWan NDIS 6.2 on a eth frame module
HKR, Params,  GlobalDebugLevel, 0, 7			;the drive log level 1 = low, DBG_ERROR = 7
HKR, Params,  ProviderID, 0, ""				
HKR, Params,  ManualNetworkSelection, 0, 0
HKR, Params,  WwanDataClass, 0x10001, 1
HKR, Params,  IsF3507g, 0x10001, 1
HKR, Params,  ProvisionedAccessString, 0, ""
HKR, Params,  ProvisionedUserName, 0, ""
HKR, Params,  ProvisionedPassword, 0, ""
HKR, Params,  ProvisionedProviderId, 0, ""
HKR, Params,  ContextId, 0x10001, 0
HKR, Params,  ContextType, 0x10001, 0
HKR, Params,  ProvisionedCompression, 0x10001, 0
HKR, Params,  ProvisionedAuthType, 0x10001, 0
HKR, Params,  RadioAccessCFUN, 0x10001, 1

;
;[HKEY_LOCAL_MACHINE\SYSTEM\ControlSet001\Control\Class\{4D36E972-E325-11CE-BFC1-08002BE10318}\0007\Ndi\Params\*ReceiveBuffers]
;
HKR, Ndi\params\*ReceiveBuffers,  ParamDesc,  0, "%ReceiveBuffers%"
HKR, Ndi\params\*ReceiveBuffers,  default,    0, "64"

;
;[HKEY_LOCAL_MACHINE\SYSTEM\ControlSet001\Control\Class\{4D36E972-E325-11CE-BFC1-08002BE10318}\0007\Ndi\Params\*TransmitBuffers]
;
HKR, Ndi\params\*TransmitBuffers, ParamDesc,  0, "%TransmitBuffers%"
HKR, Ndi\params\*TransmitBuffers, default,    0, "15"

;
;	
;
[ericssondg.Service]
DisplayName = %Ericsson.Service.DispName%
ServiceType = 1                            ;SERVICE_KERNEL_DRIVER
StartType = 3                              ;SERVICE_DEMAND_START
ErrorControl = 1                           ;SERVICE_ERROR_NORMAL
ServiceBinary = %12%\WwanUsbMp.sys
LoadOrderGroup = NDIS

[ericssondg64.Service]
DisplayName = %Ericsson.Service.DispName%
ServiceType = 1                            ;SERVICE_KERNEL_DRIVER
StartType = 3                              ;SERVICE_DEMAND_START
ErrorControl = 1                           ;SERVICE_ERROR_NORMAL
ServiceBinary = %12%\WwanUsbMp64.sys
LoadOrderGroup = NDIS


[ericssondg.EventLog]
AddReg = ericssondg.AddEventLog.reg

[ericssondg.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll"
HKR, , TypesSupported,   0x00010001, 7

[ericssondg.CopyFiles]
WwanUsbMp.sys,,,2

[ericssondg64.CopyFiles]
WwanUsbMp64.sys,,,2

[SourceDisksNames.x86]
1 = %DiskDescription%,WwanUsbMp.sys,,\i386

[SourceDisksNames.amd64]
1 = %DiskDescription%,WwanUsbMp64.sys,,\amd64


[SourceDisksFiles.x86]
WwanUsbMp.sys = 1,,
WdfCoInstaller01009.dll = 1

[SourceDisksFiles.amd64]
WwanUsbMp64.sys = 1,,
WdfCoInstaller01009.dll = 1


[DestinationDirs]
ericssondg.CopyFiles = 12
ericssondg64.CopyFiles = 12
DefaultDestDirs = 11

;-------------- WDF Coinstaller installation
[DestinationDirs]
CoInstaller_CopyFiles = 11

[ericssondg.ndi.NTx86.CoInstallers]
AddReg    = CoInstaller_AddReg
CopyFiles = CoInstaller_CopyFiles

[ericssondg.ndi.NTAMD64.CoInstallers]
AddReg    = CoInstaller_AddReg
CopyFiles = CoInstaller_CopyFiles
;
;	wdfcoinstaller01009
;
[CoInstaller_CopyFiles]
wdfcoinstaller01009.dll

[SourceDisksFiles]
wdfcoinstaller01009.dll=1 ; make sure the number matches with SourceDisksNames

[CoInstaller_AddReg]
HKR,,CoInstallers32,0x00010000, "wdfcoinstaller01009.dll,WdfCoInstaller"

[ericssondg.ndi.NTx86.Wdf]
KmdfService = WwanUsbServ, ericssondg_wdfsect

[ericssondg.ndi.NTAMD64.Wdf]
KmdfService = WwanUsbServ, ericssondg_wdfsect

[ericssondg_wdfsect]
KmdfLibraryVersion = 1.9

;%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
;End Of Devgiri Section
;%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%


[Strings]
EAB = "Ericsson"
Ericsson = "Ericsson AB"

Ericsson.Sm_DeviceDesc_WWAN = "F3607gw Mobile Broadband Driver"
Ericsson.Dg_DeviceDesc_WWAN = "F3507g Mobile Broadband Driver"
Lenovo.Sm_DeviceDesc_WWAN = "F3607gw Mobile Broadband Driver"
Lenovo.Dg_DeviceDesc_WWAN = "F3507g Mobile Broadband Driver"
Dell.Sm_DeviceDesc_WWAN = "Dell Wireless 5540 HSPA Mini-Card Network Adapter"
Dell.Dg_DeviceDesc_WWAN = "Dell Wireless 5530 HSPA Mini-Card Network Adapter"
Hp.BV_DeviceDesc_WWAN    = "HP hs2320 Mobile Broadband Module Network Adapter" ; Band V
Hp.BVIII_DeviceDesc_WWAN = "HP hs2330 Mobile Broadband Module Network Adapter" ;Band VIII
Toshiba.Sm_DeviceDesc_WWAN = "Ericsson F3607gw for TOSHIBA Mobile Broadband Network Adapter"
Toshiba.Dg_DeviceDesc_WWAN = "TOSHIBA F3507g Mobile Broadband Network Adapter"
Ericsson.Pl_DeviceDesc_WWAN = "F3307 Mobile Broadband Driver"

Ericsson.Service.DispName         = "Ericsson WWAN Wireless Module Device Driver"	;;;don't match with WwanUsbServ Remove USB
DiskDescription                   = "Ericsson WWAN USB Driver Disk 1"
TransmitBuffers                   = "Transmit Buffers"
ReceiveBuffers                    = "Receive Buffers"
