; Sierra Wireless Virtual Network Port Setup File
; Copyright (c) 2004 Sierra Wireless Inc. All Rights Reserved.

[Version]
Signature="$WINDOWS NT$"
Class=Net
ClassGUID={4d36e972-e325-11ce-bfc1-08002be10318}
Provider=%Manufacturer%
DriverVer=09/28/2009,6.20.0.8
CatalogFile=SWNC5E00.cat

[SourceDisksNames]
1 = %DISKID%,,,""

[SourceDisksFiles]
SWNC5E00.sys = 1,,
SWNC5E00x64.sys = 1,,
SWNC5E00win7.sys = 1,,
SWNC5E00win7x64.sys = 1,,

[DestinationDirs]
SWDRIVER.CopyFiles=12
SWDRIVER.NTamd64.CopyFiles=12
SWDRIVER.NTx86.6.1.CopyFiles=12
SWDRIVER.NTamd64.6.1.CopyFiles=12
DefaultDestDir=12

[Manufacturer]
%Manufacturer%=SWI, NTamd64, NTx86.6.0, NTamd64.6.0, NTx86.6.1, NTamd64.6.1

[SWI]
%DEVICE0T598.SWNETWORK% = SWPORT, SWMUXBUS\SW_NET_0_VID_1199&PID_0025
%DEVICE0T11.SWNETWORK% = SWPORT, SWMUXBUS\SW_NET_0_VID_1199&PID_0026
%DEVICE0EM5625.SWNETWORK% = SWPORT, SWMUXBUS\SW_NET_0_VID_1199&PID_0017
%DEVICE0MC8600.SWNETWORK% = SWPORT, SWMUXBUS\SW_NET_0_VID_1199&PID_6800
%DEVICE0MC5720.SWNETWORK% = SWPORT, SWMUXBUS\SW_NET_0_VID_1199&PID_0018
%DEVICE0MC5725.SWNETWORK% = SWPORT, SWMUXBUS\SW_NET_0_VID_1199&PID_0020
%DEVICE0AC595.SWNETWORK% = SWPORT, SWMUXBUS\SW_NET_0_VID_1199&PID_0019
%DEVICE0AC595E.SWNETWORK% = SWPORT, SWMUXBUS\SW_NET_0_VID_1199&PID_0021
%DEVICE0MC5725U.SWNETWORK% = SWPORT, SWMUXBUS\SW_NET_0_VID_1199&PID_0120
%DEVICE0EM5725.SWNETWORK% = SWPORT, SWMUXBUS\SW_NET_0_VID_1199&PID_0022
%DEVICE0AC597.SWNETWORK% = SWPORT, SWMUXBUS\SW_NET_0_VID_1199&PID_0023
%DEVICE0MC5727.SWNETWORK% = SWPORT, SWMUXBUS\SW_NET_0_VID_1199&PID_0024
%DEVICE0AC402.SWNETWORK% = SWPORT, SWMUXBUS\SW_NET_0_VID_1199&PID_0027
%DEVICE0MC5728.SWNETWORK% = SWPORT, SWMUXBUS\SW_NET_0_VID_1199&PID_0028
%DEVICEETH.SWNETWORK% = SWPORTETH, SWMUXBUS\SW_NET_0_VID_1199&PID_0029
%DEVICE0NC.SWNETWORK% = SWPORT, SWMUXBUS\SW_NET_0_VID_1199&PID_0300
%DEVICE0NC.SWNETWORK% = SWPORT, SWMUXBUS\SW_NET_0_VID_1199&PID_0301
%DEVICE0NC.SWNETWORK% = SWPORT, SWMUXBUS\SW_NET_0_VID_1199&PID_0302
%DEVICE0NC.SWNETWORK% = SWPORT, SWMUXBUS\SW_NET_0_VID_1199&PID_0303
%DEVICE0NC.SWNETWORK% = SWPORT, SWMUXBUS\SW_NET_0_VID_1199&PID_0304
%DEVICE0C.SWNETWORK% = SWPORT, SWMUXBUS\SW_NET_0_VID_1199&PID_0400
%DEVICE0C.SWNETWORK% = SWPORT, SWMUXBUS\SW_NET_0_VID_1199&PID_0401
%DEVICE0C.SWNETWORK% = SWPORT, SWMUXBUS\SW_NET_0_VID_1199&PID_0402
%DEVICE0C.SWNETWORK% = SWPORT, SWMUXBUS\SW_NET_0_VID_1199&PID_0403
%DEVICE0C.SWNETWORK% = SWPORT, SWMUXBUS\SW_NET_0_VID_1199&PID_0404
;;

[SWI.NTamd64]
%DEVICE0T598.SWNETWORK% = SWPORT.NTamd64, SWMUXBUS\SW_NET_0_VID_1199&PID_0025
%DEVICE0T11.SWNETWORK% = SWPORT.NTamd64, SWMUXBUS\SW_NET_0_VID_1199&PID_0026
%DEVICE0EM5625.SWNETWORK% = SWPORT.NTamd64, SWMUXBUS\SW_NET_0_VID_1199&PID_0017
%DEVICE0MC8600.SWNETWORK% = SWPORT.NTamd64, SWMUXBUS\SW_NET_0_VID_1199&PID_6800
%DEVICE0MC5720.SWNETWORK% = SWPORT.NTamd64, SWMUXBUS\SW_NET_0_VID_1199&PID_0018
%DEVICE0MC5725.SWNETWORK% = SWPORT.NTamd64, SWMUXBUS\SW_NET_0_VID_1199&PID_0020
%DEVICE0AC595.SWNETWORK% = SWPORT.NTamd64, SWMUXBUS\SW_NET_0_VID_1199&PID_0019
%DEVICE0AC595E.SWNETWORK% = SWPORT.NTamd64, SWMUXBUS\SW_NET_0_VID_1199&PID_0021
%DEVICE0MC5725U.SWNETWORK% = SWPORT.NTamd64, SWMUXBUS\SW_NET_0_VID_1199&PID_0120
%DEVICE0EM5725.SWNETWORK% = SWPORT.NTamd64, SWMUXBUS\SW_NET_0_VID_1199&PID_0022
%DEVICE0AC597.SWNETWORK% = SWPORT.NTamd64, SWMUXBUS\SW_NET_0_VID_1199&PID_0023
%DEVICE0MC5727.SWNETWORK% = SWPORT.NTamd64, SWMUXBUS\SW_NET_0_VID_1199&PID_0024
%DEVICE0AC402.SWNETWORK% = SWPORT.NTamd64, SWMUXBUS\SW_NET_0_VID_1199&PID_0027
%DEVICE0MC5728.SWNETWORK% = SWPORT.NTamd64, SWMUXBUS\SW_NET_0_VID_1199&PID_0028
%DEVICEETH.SWNETWORK% = SWPORTETH.NTamd64, SWMUXBUS\SW_NET_0_VID_1199&PID_0029
%DEVICE0NC.SWNETWORK% = SWPORT.NTamd64, SWMUXBUS\SW_NET_0_VID_1199&PID_0300
%DEVICE0NC.SWNETWORK% = SWPORT.NTamd64, SWMUXBUS\SW_NET_0_VID_1199&PID_0301
%DEVICE0NC.SWNETWORK% = SWPORT.NTamd64, SWMUXBUS\SW_NET_0_VID_1199&PID_0302
%DEVICE0NC.SWNETWORK% = SWPORT.NTamd64, SWMUXBUS\SW_NET_0_VID_1199&PID_0303
%DEVICE0NC.SWNETWORK% = SWPORT.NTamd64, SWMUXBUS\SW_NET_0_VID_1199&PID_0304
%DEVICE0C.SWNETWORK% = SWPORT.NTamd64, SWMUXBUS\SW_NET_0_VID_1199&PID_0400
%DEVICE0C.SWNETWORK% = SWPORT.NTamd64, SWMUXBUS\SW_NET_0_VID_1199&PID_0401
%DEVICE0C.SWNETWORK% = SWPORT.NTamd64, SWMUXBUS\SW_NET_0_VID_1199&PID_0402
%DEVICE0C.SWNETWORK% = SWPORT.NTamd64, SWMUXBUS\SW_NET_0_VID_1199&PID_0403
%DEVICE0C.SWNETWORK% = SWPORT.NTamd64, SWMUXBUS\SW_NET_0_VID_1199&PID_0404
;;

[SWI.NTx86.6.0]
%DEVICE0T598.SWNETWORK% = SWPORT, SWMUXBUS\SW_NET_0_VID_1199&PID_0025
%DEVICE0T11.SWNETWORK% = SWPORT, SWMUXBUS\SW_NET_0_VID_1199&PID_0026
%DEVICE0EM5625.SWNETWORK% = SWPORT, SWMUXBUS\SW_NET_0_VID_1199&PID_0017
%DEVICE0MC8600.SWNETWORK% = SWPORT, SWMUXBUS\SW_NET_0_VID_1199&PID_6800
%DEVICE0MC5720.SWNETWORK% = SWPORT, SWMUXBUS\SW_NET_0_VID_1199&PID_0018
%DEVICE0MC5725.SWNETWORK% = SWPORT, SWMUXBUS\SW_NET_0_VID_1199&PID_0020
%DEVICE0AC595.SWNETWORK% = SWPORT, SWMUXBUS\SW_NET_0_VID_1199&PID_0019
%DEVICE0AC595E.SWNETWORK% = SWPORT, SWMUXBUS\SW_NET_0_VID_1199&PID_0021
%DEVICE0MC5725U.SWNETWORK% = SWPORT, SWMUXBUS\SW_NET_0_VID_1199&PID_0120
%DEVICE0EM5725.SWNETWORK% = SWPORT, SWMUXBUS\SW_NET_0_VID_1199&PID_0022
%DEVICE0AC597.SWNETWORK% = SWPORT, SWMUXBUS\SW_NET_0_VID_1199&PID_0023
%DEVICE0MC5727.SWNETWORK% = SWPORT, SWMUXBUS\SW_NET_0_VID_1199&PID_0024
%DEVICE0AC402.SWNETWORK% = SWPORT, SWMUXBUS\SW_NET_0_VID_1199&PID_0027
%DEVICE0MC5728.SWNETWORK% = SWPORT, SWMUXBUS\SW_NET_0_VID_1199&PID_0028
%DEVICEETH.SWNETWORK% = SWPORTETH, SWMUXBUS\SW_NET_0_VID_1199&PID_0029
%DEVICE0NC.SWNETWORK% = SWPORT, SWMUXBUS\SW_NET_0_VID_1199&PID_0300
%DEVICE0NC.SWNETWORK% = SWPORT, SWMUXBUS\SW_NET_0_VID_1199&PID_0301
%DEVICE0NC.SWNETWORK% = SWPORT, SWMUXBUS\SW_NET_0_VID_1199&PID_0302
%DEVICE0NC.SWNETWORK% = SWPORT, SWMUXBUS\SW_NET_0_VID_1199&PID_0303
%DEVICE0NC.SWNETWORK% = SWPORT, SWMUXBUS\SW_NET_0_VID_1199&PID_0304
%DEVICE0C.SWNETWORK% = SWPORT, SWMUXBUS\SW_NET_0_VID_1199&PID_0400
%DEVICE0C.SWNETWORK% = SWPORT, SWMUXBUS\SW_NET_0_VID_1199&PID_0401
%DEVICE0C.SWNETWORK% = SWPORT, SWMUXBUS\SW_NET_0_VID_1199&PID_0402
%DEVICE0C.SWNETWORK% = SWPORT, SWMUXBUS\SW_NET_0_VID_1199&PID_0403
%DEVICE0C.SWNETWORK% = SWPORT, SWMUXBUS\SW_NET_0_VID_1199&PID_0404
;;

[SWI.NTamd64.6.0]
%DEVICE0T598.SWNETWORK% = SWPORT.NTamd64, SWMUXBUS\SW_NET_0_VID_1199&PID_0025
%DEVICE0T11.SWNETWORK% = SWPORT.NTamd64, SWMUXBUS\SW_NET_0_VID_1199&PID_0026
%DEVICE0EM5625.SWNETWORK% = SWPORT.NTamd64, SWMUXBUS\SW_NET_0_VID_1199&PID_0017
%DEVICE0MC8600.SWNETWORK% = SWPORT.NTamd64, SWMUXBUS\SW_NET_0_VID_1199&PID_6800
%DEVICE0MC5720.SWNETWORK% = SWPORT.NTamd64, SWMUXBUS\SW_NET_0_VID_1199&PID_0018
%DEVICE0MC5725.SWNETWORK% = SWPORT.NTamd64, SWMUXBUS\SW_NET_0_VID_1199&PID_0020
%DEVICE0AC595.SWNETWORK% = SWPORT.NTamd64, SWMUXBUS\SW_NET_0_VID_1199&PID_0019
%DEVICE0AC595E.SWNETWORK% = SWPORT.NTamd64, SWMUXBUS\SW_NET_0_VID_1199&PID_0021
%DEVICE0MC5725U.SWNETWORK% = SWPORT.NTamd64, SWMUXBUS\SW_NET_0_VID_1199&PID_0120
%DEVICE0EM5725.SWNETWORK% = SWPORT.NTamd64, SWMUXBUS\SW_NET_0_VID_1199&PID_0022
%DEVICE0AC597.SWNETWORK% = SWPORT.NTamd64, SWMUXBUS\SW_NET_0_VID_1199&PID_0023
%DEVICE0MC5727.SWNETWORK% = SWPORT.NTamd64, SWMUXBUS\SW_NET_0_VID_1199&PID_0024
%DEVICE0AC402.SWNETWORK% = SWPORT.NTamd64, SWMUXBUS\SW_NET_0_VID_1199&PID_0027
%DEVICE0MC5728.SWNETWORK% = SWPORT.NTamd64, SWMUXBUS\SW_NET_0_VID_1199&PID_0028
%DEVICEETH.SWNETWORK% = SWPORTETH.NTamd64, SWMUXBUS\SW_NET_0_VID_1199&PID_0029
%DEVICE0NC.SWNETWORK% = SWPORT.NTamd64, SWMUXBUS\SW_NET_0_VID_1199&PID_0300
%DEVICE0NC.SWNETWORK% = SWPORT.NTamd64, SWMUXBUS\SW_NET_0_VID_1199&PID_0301
%DEVICE0NC.SWNETWORK% = SWPORT.NTamd64, SWMUXBUS\SW_NET_0_VID_1199&PID_0302
%DEVICE0NC.SWNETWORK% = SWPORT.NTamd64, SWMUXBUS\SW_NET_0_VID_1199&PID_0303
%DEVICE0NC.SWNETWORK% = SWPORT.NTamd64, SWMUXBUS\SW_NET_0_VID_1199&PID_0304
%DEVICE0C.SWNETWORK% = SWPORT.NTamd64, SWMUXBUS\SW_NET_0_VID_1199&PID_0400
%DEVICE0C.SWNETWORK% = SWPORT.NTamd64, SWMUXBUS\SW_NET_0_VID_1199&PID_0401
%DEVICE0C.SWNETWORK% = SWPORT.NTamd64, SWMUXBUS\SW_NET_0_VID_1199&PID_0402
%DEVICE0C.SWNETWORK% = SWPORT.NTamd64, SWMUXBUS\SW_NET_0_VID_1199&PID_0403
%DEVICE0C.SWNETWORK% = SWPORT.NTamd64, SWMUXBUS\SW_NET_0_VID_1199&PID_0404
;;

[SWI.NTx86.6.1]
%DEVICE0T598.SWNETWORK% = SWPORT.NTx86.6.1, SWMUXBUS\SW_NET_0_VID_1199&PID_0025
%DEVICE0T11.SWNETWORK% = SWPORT.NTx86.6.1, SWMUXBUS\SW_NET_0_VID_1199&PID_0026
%DEVICE0EM5625.SWNETWORK% = SWPORT.NTx86.6.1, SWMUXBUS\SW_NET_0_VID_1199&PID_0017
%DEVICE0MC8600.SWNETWORK% = SWPORT.NTx86.6.1, SWMUXBUS\SW_NET_0_VID_1199&PID_6800
%DEVICE0MC5720.SWNETWORK% = SWPORT.NTx86.6.1, SWMUXBUS\SW_NET_0_VID_1199&PID_0018
%DEVICE0MC5725.SWNETWORK% = SWPORT.NTx86.6.1, SWMUXBUS\SW_NET_0_VID_1199&PID_0020
%DEVICE0AC595.SWNETWORK% = SWPORT.NTx86.6.1, SWMUXBUS\SW_NET_0_VID_1199&PID_0019
%DEVICE0AC595E.SWNETWORK% = SWPORT.NTx86.6.1, SWMUXBUS\SW_NET_0_VID_1199&PID_0021
%DEVICE0MC5725U.SWNETWORK% = SWPORT.NTx86.6.1, SWMUXBUS\SW_NET_0_VID_1199&PID_0120
%DEVICE0EM5725.SWNETWORK% = SWPORT.NTx86.6.1, SWMUXBUS\SW_NET_0_VID_1199&PID_0022
%DEVICE0AC597.SWNETWORK% = SWPORT.NTx86.6.1, SWMUXBUS\SW_NET_0_VID_1199&PID_0023
%DEVICE0MC5727.SWNETWORK% = SWPORT.NTx86.6.1, SWMUXBUS\SW_NET_0_VID_1199&PID_0024
%DEVICE0AC402.SWNETWORK% = SWPORT.NTx86.6.1, SWMUXBUS\SW_NET_0_VID_1199&PID_0027
%DEVICE0MC5728.SWNETWORK% = SWPORT.NTx86.6.1, SWMUXBUS\SW_NET_0_VID_1199&PID_0028
%DEVICEETH.SWNETWORK% = SWPORTETH.NTx86.6.1, SWMUXBUS\SW_NET_0_VID_1199&PID_0029
%DEVICE0NC.SWNETWORK% = SWPORT.NTx86.6.1, SWMUXBUS\SW_NET_0_VID_1199&PID_0300
%DEVICE0NC.SWNETWORK% = SWPORT.NTx86.6.1, SWMUXBUS\SW_NET_0_VID_1199&PID_0301
%DEVICE0NC.SWNETWORK% = SWPORT.NTx86.6.1, SWMUXBUS\SW_NET_0_VID_1199&PID_0302
%DEVICE0NC.SWNETWORK% = SWPORT.NTx86.6.1, SWMUXBUS\SW_NET_0_VID_1199&PID_0303
%DEVICE0NC.SWNETWORK% = SWPORT.NTx86.6.1, SWMUXBUS\SW_NET_0_VID_1199&PID_0304
%DEVICE0C.SWNETWORK% = SWPORT.NTx86.6.1, SWMUXBUS\SW_NET_0_VID_1199&PID_0400
%DEVICE0C.SWNETWORK% = SWPORT.NTx86.6.1, SWMUXBUS\SW_NET_0_VID_1199&PID_0401
%DEVICE0C.SWNETWORK% = SWPORT.NTx86.6.1, SWMUXBUS\SW_NET_0_VID_1199&PID_0402
%DEVICE0C.SWNETWORK% = SWPORT.NTx86.6.1, SWMUXBUS\SW_NET_0_VID_1199&PID_0403
%DEVICE0C.SWNETWORK% = SWPORT.NTx86.6.1, SWMUXBUS\SW_NET_0_VID_1199&PID_0404

[SWI.NTamd64.6.1]
%DEVICE0T598.SWNETWORK% = SWPORT.NTamd64.6.1, SWMUXBUS\SW_NET_0_VID_1199&PID_0025
%DEVICE0T11.SWNETWORK% = SWPORT.NTamd64.6.1, SWMUXBUS\SW_NET_0_VID_1199&PID_0026
%DEVICE0EM5625.SWNETWORK% = SWPORT.NTamd64.6.1, SWMUXBUS\SW_NET_0_VID_1199&PID_0017
%DEVICE0MC8600.SWNETWORK% = SWPORT.NTamd64.6.1, SWMUXBUS\SW_NET_0_VID_1199&PID_6800
%DEVICE0MC5720.SWNETWORK% = SWPORT.NTamd64.6.1, SWMUXBUS\SW_NET_0_VID_1199&PID_0018
%DEVICE0MC5725.SWNETWORK% = SWPORT.NTamd64.6.1, SWMUXBUS\SW_NET_0_VID_1199&PID_0020
%DEVICE0AC595.SWNETWORK% = SWPORT.NTamd64.6.1, SWMUXBUS\SW_NET_0_VID_1199&PID_0019
%DEVICE0AC595E.SWNETWORK% = SWPORT.NTamd64.6.1, SWMUXBUS\SW_NET_0_VID_1199&PID_0021
%DEVICE0MC5725U.SWNETWORK% = SWPORT.NTamd64.6.1, SWMUXBUS\SW_NET_0_VID_1199&PID_0120
%DEVICE0EM5725.SWNETWORK% = SWPORT.NTamd64.6.1, SWMUXBUS\SW_NET_0_VID_1199&PID_0022
%DEVICE0AC597.SWNETWORK% = SWPORT.NTamd64.6.1, SWMUXBUS\SW_NET_0_VID_1199&PID_0023
%DEVICE0MC5727.SWNETWORK% = SWPORT.NTamd64.6.1, SWMUXBUS\SW_NET_0_VID_1199&PID_0024
%DEVICE0AC402.SWNETWORK% = SWPORT.NTamd64.6.1, SWMUXBUS\SW_NET_0_VID_1199&PID_0027
%DEVICE0MC5728.SWNETWORK% = SWPORT.NTamd64.6.1, SWMUXBUS\SW_NET_0_VID_1199&PID_0028
%DEVICEETH.SWNETWORK% = SWPORTETH.NTamd64.6.1, SWMUXBUS\SW_NET_0_VID_1199&PID_0029
%DEVICE0NC.SWNETWORK% = SWPORT.NTamd64.6.1, SWMUXBUS\SW_NET_0_VID_1199&PID_0300
%DEVICE0NC.SWNETWORK% = SWPORT.NTamd64.6.1, SWMUXBUS\SW_NET_0_VID_1199&PID_0301
%DEVICE0NC.SWNETWORK% = SWPORT.NTamd64.6.1, SWMUXBUS\SW_NET_0_VID_1199&PID_0302
%DEVICE0NC.SWNETWORK% = SWPORT.NTamd64.6.1, SWMUXBUS\SW_NET_0_VID_1199&PID_0303
%DEVICE0NC.SWNETWORK% = SWPORT.NTamd64.6.1, SWMUXBUS\SW_NET_0_VID_1199&PID_0304
%DEVICE0C.SWNETWORK% = SWPORT.NTamd64.6.1, SWMUXBUS\SW_NET_0_VID_1199&PID_0400
%DEVICE0C.SWNETWORK% = SWPORT.NTamd64.6.1, SWMUXBUS\SW_NET_0_VID_1199&PID_0401
%DEVICE0C.SWNETWORK% = SWPORT.NTamd64.6.1, SWMUXBUS\SW_NET_0_VID_1199&PID_0402
%DEVICE0C.SWNETWORK% = SWPORT.NTamd64.6.1, SWMUXBUS\SW_NET_0_VID_1199&PID_0403
%DEVICE0C.SWNETWORK% = SWPORT.NTamd64.6.1, SWMUXBUS\SW_NET_0_VID_1199&PID_0404

[SWPORT]
AddReg=SWPORT.AddReg, SWPORT.AddReg.Params
CopyFiles=SWDRIVER.CopyFiles
Characteristics=0x81 ; NCF_VIRTUAL|NCF_HAS_UI

;;

[SWPORT.Services]
AddService=SWNC5E00, 0x00000002, SWDRIVER.AddService

[SWDRIVER.CopyFiles]
SWNC5E00.sys,,,2

;;

[SWPORT.NTamd64]
AddReg=SWPORT.AddReg, SWPORT.AddReg.Params
CopyFiles=SWDRIVER.NTamd64.CopyFiles
Characteristics=0x81 ; NCF_VIRTUAL|NCF_HAS_UI

;;

[SWPORT.NTamd64.Services]
AddService=SWNC5E00, 0x00000002, SWDRIVER.AddService

[SWDRIVER.NTamd64.CopyFiles]
SWNC5E00.sys,SWNC5E00x64.sys,,2

[SWDRIVER.AddService]
DisplayName     = %SERVICENAME%
ServiceType     = 1 ;SERVICE_KERNEL_DRIVER
StartType       = 3 ;SERVICE_DEMAND_START
ErrorControl    = 1 ;SERVICE_ERROR_NORMAL
ServiceBinary   = %12%\SWNC5E00.sys
LoadOrderGroup  = NDIS

;;

[SWPORT.NTx86.6.1]
AddReg=SWPORT.NT.6.1.AddReg, SWPORT.AddReg.Params
CopyFiles=SWDRIVER.NTx86.6.1.CopyFiles
Characteristics=0x81 ; NCF_VIRTUAL|NCF_HAS_UI
*IfType         = 244       ; IF_TYPE_WWANPP2
*MediaType      = 9			; NdisMediumWirelessWan
*PhysicalMediaType = 8		; NdisPhysicalMediumWirelessWan
EnableDhcp      = 0			; DHCP

[SWPORT.NTx86.6.1.Services]
AddService=SWNC5E00, 0x00000002, SWDRIVER.AddService

[SWDRIVER.NTx86.6.1.CopyFiles]
SWNC5E00.sys,SWNC5E00win7.sys,,2

[SWPORT.NTamd64.6.1]
AddReg=SWPORT.NT.6.1.AddReg, SWPORT.AddReg.Params
CopyFiles=SWDRIVER.NTamd64.6.1.CopyFiles
Characteristics=0x81 ; NCF_VIRTUAL|NCF_HAS_UI
*IfType         = 244       ; IF_TYPE_WWANPP2
*MediaType      = 9			; NdisMediumWirelessWan
*PhysicalMediaType = 8		; NdisPhysicalMediumWirelessWan
EnableDhcp      = 0			; DHCP

[SWPORT.NTamd64.6.1.Services]
AddService=SWNC5E00, 0x00000002, SWDRIVER.AddService

[SWDRIVER.NTamd64.6.1.CopyFiles]
SWNC5E00.sys,SWNC5E00win7x64.sys,,2

[SWPORTETH]
AddReg=SWPORTETH.AddReg, SWPORT.AddReg.Params
CopyFiles=SWDRIVER.CopyFiles
Characteristics=0x81 ; NCF_VIRTUAL|NCF_HAS_UI

[SWPORTETH.Services]
AddService=SWNC5E00, 0x00000002, SWDRIVER.AddService

[SWPORTETH.NTamd64]
AddReg=SWPORTETH.AddReg, SWPORT.AddReg.Params
CopyFiles=SWDRIVER.NTamd64.CopyFiles
Characteristics=0x81 ; NCF_VIRTUAL|NCF_HAS_UI

[SWPORTETH.NTamd64.Services]
AddService=SWNC5E00, 0x00000002, SWDRIVER.AddService

[SWPORTETH.NTx86.6.1]
AddReg=SWPORTETH.NT.6.1.AddReg, SWPORT.AddReg.Params
CopyFiles=SWDRIVER.NTx86.6.1.CopyFiles
Characteristics=0x81 ; NCF_VIRTUAL|NCF_HAS_UI
*IfType         = 6; IF_TYPE_ETHERNET_CSMACD   
*MediaType      = 0			;NdisMedium802_3   0 
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3 8
EnableDhcp = 1			; DHCP

[SWPORTETH.NTx86.6.1.Services]
AddService=SWNC5E00, 0x00000002, SWDRIVER.AddService

[SWPORTETH.NTamd64.6.1]
AddReg=SWPORTETH.NT.6.1.AddReg, SWPORT.AddReg.Params
CopyFiles=SWDRIVER.NTamd64.6.1.CopyFiles
Characteristics=0x81 ; NCF_VIRTUAL|NCF_HAS_UI
*IfType         = 6; IF_TYPE_ETHERNET_CSMACD  
*MediaType      = 0			;NdisMedium802_3   0 
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3 8 
EnableDhcp = 1			; DHCP

[SWPORTETH.NTamd64.6.1.Services]
AddService=SWNC5E00, 0x00000002, SWDRIVER.AddService

;;

[Strings]
Manufacturer = "Sierra Wireless"
DEVICE0EM5625.SWNETWORK = "Sierra Wireless 1xEV-DO Network Adapter"
DEVICE0MC8600.SWNETWORK = "Sierra Wireless 1xEV-DO Network Adapter (UMTS)"
DEVICE0MC5720.SWNETWORK = "Sierra Wireless 1xEV-DO Network Adapter"
DEVICE0MC5725.SWNETWORK = "Sierra Wireless MC5725 1xEV-DO Network Adapter"
DEVICE0AC595.SWNETWORK = "Sierra Wireless AC595 1xEV-DO Network Adapter"
DEVICE0AC595E.SWNETWORK = "Sierra Wireless AC597E 1xEV-DO Network Adapter"
DEVICE0MC5725U.SWNETWORK = "Sierra Wireless AC595U 1xEV-DO Network Adapter"
DEVICE0EM5725.SWNETWORK = "Sierra Wireless EM5725 1xEV-DO Network Adapter"
DEVICE0AC597.SWNETWORK = "Sierra Wireless Compass 597 EVDO Network Adapter"
DEVICE0MC5727.SWNETWORK = "Sierra Wireless MC5727 EVDO Network Adapter"
DISKID="Sierra Wireless Driver Installation Disk"
SERVICENAME="Sierra Wireless MUX NDIS Driver (#00)"
IPPacketSize	= "IPPacketSize"
IPAddress		= "IPAddress"
MaxMRU			= "MaxMRU"
BufferAdjustment = "BufferAdjustment"
EnableWINS		= "EnableWINS"
DEVICE0T598.SWNETWORK = "Sierra Wireless USB 598 EVDO Network Adapter"
DEVICE0T11.SWNETWORK  = "Sierra Wireless Network Adapter"	; USB 11
DEVICE0AC402.SWNETWORK  = "Sierra Wireless Network Adapter"	; AC402
DEVICE0MC5728.SWNETWORK  = "Sierra Wireless Network Adapter"	; MC5728
DEVICE0NC.SWNETWORK  = "Sierra Wireless Network Adapter"	; Non-Composite
DEVICE0C.SWNETWORK  = "Sierra Wireless Network Adapter"		; Composite
DEVICEETH.SWNETWORK = "Sierra Wireless Network Adapter"         ; Eagle

;;

[SWPORT.AddReg]
HKR, Ndi, Service,  0,  SWNC5E00
HKR, Ndi\Interfaces, DefUpper, 0, "ndis5"
HKR, Ndi\Interfaces, DefLower, 0, "ethernet"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis5"
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"
HKR,               , OsType,     0, "6"
HKR,               , MACAddress, 0, "00A0D5FFFF85"
HKR,               , VendorDesc, 0, "EM56xx"

[SWPORT.NT.6.1.AddReg]
HKR, Ndi, Service,  0,  SWNC5E00
HKR, Ndi\Interfaces, DefUpper, 0, "ndis5"
HKR, Ndi\Interfaces, DefLower, 0, "ethernet"
HKR, Ndi\Interfaces, UpperRange, 0, "flpp4"
HKR, Ndi\Interfaces, LowerRange, 0, "ppip"
HKR,               , OsType,     0, "6"
HKR,               , MACAddress, 0, "00A0D5FFFF85"
HKR,               , VendorDesc, 0, "EM56xx"
HKR,               , EnableDhcp, 0x10001, 0

[SWPORTETH.AddReg]
HKR, Ndi, Service,  0,  SWNC5E00
HKR, Ndi\Interfaces, DefUpper, 0, "ndis5"
HKR, Ndi\Interfaces, DefLower, 0, "ethernet"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis5"
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"
HKR,               , OsType,     0, "6"
HKR,               , MACAddress, 0, "00A0D5FFFFAF"
HKR,               , VendorDesc, 0, "EthMux"

[SWPORTETH.NT.6.1.AddReg]
HKR, Ndi, Service,  0, SWNC5E00
HKR, Ndi\Interfaces, DefUpper, 0, "ndis5"
HKR, Ndi\Interfaces, DefLower, 0, "ethernet"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis5"
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"
HKR,               , OsType,     0, "6"
HKR,               , MACAddress, 0, "00A0D5FFFFAF"
HKR,               , VendorDesc, 0, "EthMux"

; Optional Custom Parameters in the Registry ("Advanced" menu).
[SWPORT.AddReg.Params]
HKR, NDI\params\IPPacketSize, ParamDesc,  0, %IPPacketSize%
HKR, NDI\params\IPPacketSize, type,       0, "edit"
HKR, NDI\params\IPPacketSize, LimitText,  0, "4"
HKR, NDI\params\IPPacketSize, UpperCase,  0, "1"
HKR, NDI\params\IPPacketSize, default,    0, "1450"
HKR, NDI\params\IPPacketSize, optional,   0, "0"

HKR, NDI\params\IPAddress, ParamDesc,  0, %IPAddress%
HKR, NDI\params\IPAddress, type,       0, "enum"
HKR, NDI\params\IPAddress, LimitText,  0, "15"
HKR, NDI\params\IPAddress, UpperCase,  0, "1"
HKR, NDI\params\IPAddress, default,    0, "0"
HKR, NDI\params\IPAddress, optional,   0, "0"
HKR, NDI\params\IPAddress\enum, "0",   0, "10.0.0.5"
HKR, NDI\params\IPAddress\enum, "1",   0, "192.168.0.5"
HKR, NDI\params\IPAddress\enum, "2",   0, "172.16.0.5"

HKR, NDI\params\MaxMRU, ParamDesc,  0, %MaxMRU%
HKR, NDI\params\MaxMRU, type,       0, "edit"
HKR, NDI\params\MaxMRU, LimitText,  0, "4"
HKR, NDI\params\MaxMRU, UpperCase,  0, "1"
HKR, NDI\params\MaxMRU, default,    0, "1500"
HKR, NDI\params\MaxMRU, optional,   0, "0"

HKR, NDI\params\BufferAdjustment, ParamDesc,  0, %BufferAdjustment%
HKR, NDI\params\BufferAdjustment, type,       0, "word"
HKR, NDI\params\BufferAdjustment, default,    0, "0"
HKR, NDI\params\BufferAdjustment, optional,   0, "0"
HKR, NDI\params\BufferAdjustment, min,        0, "0"
HKR, NDI\params\BufferAdjustment, max,        0, "90"
HKR, NDI\params\BufferAdjustment, step,       0, "10"

HKR, NDI\params\EnableWINS, ParamDesc,  0, %EnableWINS%
HKR, NDI\params\EnableWINS, type,       0, "edit"
HKR, NDI\params\EnableWINS, LimitText,  0, "4"
HKR, NDI\params\EnableWINS, UpperCase,  0, "1"
HKR, NDI\params\EnableWINS, default,    0, "0"
HKR, NDI\params\EnableWINS, optional,   0, "0"


